// Copyright (C) 2020  Intel Corporation. All rights reserved.
// Your use of Intel Corporation's design tools, logic functions 
// and other software and tools, and any partner logic 
// functions, and any output files from any of the foregoing 
// (including device programming or simulation files), and any 
// associated documentation or information are expressly subject 
// to the terms and conditions of the Intel Program License 
// Subscription Agreement, the Intel Quartus Prime License Agreement,
// the Intel FPGA IP License Agreement, or other applicable license
// agreement, including, without limitation, that your use is for
// the sole purpose of programming logic devices manufactured by
// Intel and sold by Intel or its authorized distributors.  Please
// refer to the applicable agreement for further details, at
// https://fpgasoftware.intel.com/eula.

// VENDOR "Altera"
// PROGRAM "Quartus Prime"
// VERSION "Version 20.1.0 Build 711 06/05/2020 SJ Standard Edition"

// DATE "05/03/2022 00:21:29"

// 
// Device: Altera 5CSEMA5F31C6 Package FBGA896
// 

// 
// This Verilog file should be used for ModelSim (Verilog) only
// 

`timescale 1 ps/ 1 ps

module vga_top (
	CLOCK_50,
	KEY,
	LEDR,
	SW,
	HEX0,
	HEX1,
	HEX2,
	HEX3,
	HEX4,
	HEX5,
	VGA_CLK,
	VGA_HS,
	VGA_VS,
	VGA_BLANK_N,
	VGA_SYNC_N,
	VGA_R,
	VGA_G,
	VGA_B);
input 	CLOCK_50;
input 	[3:0] KEY;
output 	[9:0] LEDR;
input 	[9:0] SW;
output 	[7:0] HEX0;
output 	[7:0] HEX1;
output 	[7:0] HEX2;
output 	[7:0] HEX3;
output 	[7:0] HEX4;
output 	[7:0] HEX5;
output 	VGA_CLK;
output 	VGA_HS;
output 	VGA_VS;
output 	VGA_BLANK_N;
output 	VGA_SYNC_N;
output 	[7:0] VGA_R;
output 	[7:0] VGA_G;
output 	[7:0] VGA_B;

// Design Ports Information
// KEY[1]	=>  Location: PIN_AA15,	 I/O Standard: 2.5 V,	 Current Strength: Default
// KEY[2]	=>  Location: PIN_W15,	 I/O Standard: 2.5 V,	 Current Strength: Default
// LEDR[0]	=>  Location: PIN_V16,	 I/O Standard: 2.5 V,	 Current Strength: Default
// LEDR[1]	=>  Location: PIN_W16,	 I/O Standard: 2.5 V,	 Current Strength: Default
// LEDR[2]	=>  Location: PIN_V17,	 I/O Standard: 2.5 V,	 Current Strength: Default
// LEDR[3]	=>  Location: PIN_V18,	 I/O Standard: 2.5 V,	 Current Strength: Default
// LEDR[4]	=>  Location: PIN_W17,	 I/O Standard: 2.5 V,	 Current Strength: Default
// LEDR[5]	=>  Location: PIN_W19,	 I/O Standard: 2.5 V,	 Current Strength: Default
// LEDR[6]	=>  Location: PIN_Y19,	 I/O Standard: 2.5 V,	 Current Strength: Default
// LEDR[7]	=>  Location: PIN_W20,	 I/O Standard: 2.5 V,	 Current Strength: Default
// LEDR[8]	=>  Location: PIN_W21,	 I/O Standard: 2.5 V,	 Current Strength: Default
// LEDR[9]	=>  Location: PIN_Y21,	 I/O Standard: 2.5 V,	 Current Strength: Default
// SW[0]	=>  Location: PIN_AB12,	 I/O Standard: 2.5 V,	 Current Strength: Default
// SW[1]	=>  Location: PIN_AC12,	 I/O Standard: 2.5 V,	 Current Strength: Default
// SW[2]	=>  Location: PIN_AF9,	 I/O Standard: 2.5 V,	 Current Strength: Default
// SW[3]	=>  Location: PIN_AF10,	 I/O Standard: 2.5 V,	 Current Strength: Default
// SW[4]	=>  Location: PIN_AD11,	 I/O Standard: 2.5 V,	 Current Strength: Default
// SW[5]	=>  Location: PIN_AD12,	 I/O Standard: 2.5 V,	 Current Strength: Default
// SW[6]	=>  Location: PIN_AE11,	 I/O Standard: 2.5 V,	 Current Strength: Default
// SW[7]	=>  Location: PIN_AC9,	 I/O Standard: 2.5 V,	 Current Strength: Default
// SW[8]	=>  Location: PIN_AD10,	 I/O Standard: 2.5 V,	 Current Strength: Default
// HEX0[0]	=>  Location: PIN_AE26,	 I/O Standard: 2.5 V,	 Current Strength: Default
// HEX0[1]	=>  Location: PIN_AE27,	 I/O Standard: 2.5 V,	 Current Strength: Default
// HEX0[2]	=>  Location: PIN_AE28,	 I/O Standard: 2.5 V,	 Current Strength: Default
// HEX0[3]	=>  Location: PIN_AG27,	 I/O Standard: 2.5 V,	 Current Strength: Default
// HEX0[4]	=>  Location: PIN_AF28,	 I/O Standard: 2.5 V,	 Current Strength: Default
// HEX0[5]	=>  Location: PIN_AG28,	 I/O Standard: 2.5 V,	 Current Strength: Default
// HEX0[6]	=>  Location: PIN_AH28,	 I/O Standard: 2.5 V,	 Current Strength: Default
// HEX0[7]	=>  Location: PIN_AJ19,	 I/O Standard: 2.5 V,	 Current Strength: Default
// HEX1[0]	=>  Location: PIN_AJ29,	 I/O Standard: 2.5 V,	 Current Strength: Default
// HEX1[1]	=>  Location: PIN_AH29,	 I/O Standard: 2.5 V,	 Current Strength: Default
// HEX1[2]	=>  Location: PIN_AH30,	 I/O Standard: 2.5 V,	 Current Strength: Default
// HEX1[3]	=>  Location: PIN_AG30,	 I/O Standard: 2.5 V,	 Current Strength: Default
// HEX1[4]	=>  Location: PIN_AF29,	 I/O Standard: 2.5 V,	 Current Strength: Default
// HEX1[5]	=>  Location: PIN_AF30,	 I/O Standard: 2.5 V,	 Current Strength: Default
// HEX1[6]	=>  Location: PIN_AD27,	 I/O Standard: 2.5 V,	 Current Strength: Default
// HEX1[7]	=>  Location: PIN_AA25,	 I/O Standard: 2.5 V,	 Current Strength: Default
// HEX2[0]	=>  Location: PIN_AB23,	 I/O Standard: 2.5 V,	 Current Strength: Default
// HEX2[1]	=>  Location: PIN_AE29,	 I/O Standard: 2.5 V,	 Current Strength: Default
// HEX2[2]	=>  Location: PIN_AD29,	 I/O Standard: 2.5 V,	 Current Strength: Default
// HEX2[3]	=>  Location: PIN_AC28,	 I/O Standard: 2.5 V,	 Current Strength: Default
// HEX2[4]	=>  Location: PIN_AD30,	 I/O Standard: 2.5 V,	 Current Strength: Default
// HEX2[5]	=>  Location: PIN_AC29,	 I/O Standard: 2.5 V,	 Current Strength: Default
// HEX2[6]	=>  Location: PIN_AC30,	 I/O Standard: 2.5 V,	 Current Strength: Default
// HEX2[7]	=>  Location: PIN_G8,	 I/O Standard: 2.5 V,	 Current Strength: Default
// HEX3[0]	=>  Location: PIN_AD26,	 I/O Standard: 2.5 V,	 Current Strength: Default
// HEX3[1]	=>  Location: PIN_AC27,	 I/O Standard: 2.5 V,	 Current Strength: Default
// HEX3[2]	=>  Location: PIN_AD25,	 I/O Standard: 2.5 V,	 Current Strength: Default
// HEX3[3]	=>  Location: PIN_AC25,	 I/O Standard: 2.5 V,	 Current Strength: Default
// HEX3[4]	=>  Location: PIN_AB28,	 I/O Standard: 2.5 V,	 Current Strength: Default
// HEX3[5]	=>  Location: PIN_AB25,	 I/O Standard: 2.5 V,	 Current Strength: Default
// HEX3[6]	=>  Location: PIN_AB22,	 I/O Standard: 2.5 V,	 Current Strength: Default
// HEX3[7]	=>  Location: PIN_AJ17,	 I/O Standard: 2.5 V,	 Current Strength: Default
// HEX4[0]	=>  Location: PIN_AK27,	 I/O Standard: 2.5 V,	 Current Strength: Default
// HEX4[1]	=>  Location: PIN_AD17,	 I/O Standard: 2.5 V,	 Current Strength: Default
// HEX4[2]	=>  Location: PIN_D1,	 I/O Standard: 2.5 V,	 Current Strength: Default
// HEX4[3]	=>  Location: PIN_AH9,	 I/O Standard: 2.5 V,	 Current Strength: Default
// HEX4[4]	=>  Location: PIN_V23,	 I/O Standard: 2.5 V,	 Current Strength: Default
// HEX4[5]	=>  Location: PIN_F9,	 I/O Standard: 2.5 V,	 Current Strength: Default
// HEX4[6]	=>  Location: PIN_J7,	 I/O Standard: 2.5 V,	 Current Strength: Default
// HEX4[7]	=>  Location: PIN_AB17,	 I/O Standard: 2.5 V,	 Current Strength: Default
// HEX5[0]	=>  Location: PIN_AF5,	 I/O Standard: 2.5 V,	 Current Strength: Default
// HEX5[1]	=>  Location: PIN_AF18,	 I/O Standard: 2.5 V,	 Current Strength: Default
// HEX5[2]	=>  Location: PIN_B8,	 I/O Standard: 2.5 V,	 Current Strength: Default
// HEX5[3]	=>  Location: PIN_AG23,	 I/O Standard: 2.5 V,	 Current Strength: Default
// HEX5[4]	=>  Location: PIN_AC23,	 I/O Standard: 2.5 V,	 Current Strength: Default
// HEX5[5]	=>  Location: PIN_AG8,	 I/O Standard: 2.5 V,	 Current Strength: Default
// HEX5[6]	=>  Location: PIN_AA26,	 I/O Standard: 2.5 V,	 Current Strength: Default
// HEX5[7]	=>  Location: PIN_A5,	 I/O Standard: 2.5 V,	 Current Strength: Default
// VGA_CLK	=>  Location: PIN_A11,	 I/O Standard: 2.5 V,	 Current Strength: Default
// VGA_HS	=>  Location: PIN_B11,	 I/O Standard: 2.5 V,	 Current Strength: Default
// VGA_VS	=>  Location: PIN_D11,	 I/O Standard: 2.5 V,	 Current Strength: Default
// VGA_BLANK_N	=>  Location: PIN_F10,	 I/O Standard: 2.5 V,	 Current Strength: Default
// VGA_SYNC_N	=>  Location: PIN_C10,	 I/O Standard: 2.5 V,	 Current Strength: Default
// VGA_R[0]	=>  Location: PIN_A13,	 I/O Standard: 2.5 V,	 Current Strength: Default
// VGA_R[1]	=>  Location: PIN_C13,	 I/O Standard: 2.5 V,	 Current Strength: Default
// VGA_R[2]	=>  Location: PIN_E13,	 I/O Standard: 2.5 V,	 Current Strength: Default
// VGA_R[3]	=>  Location: PIN_B12,	 I/O Standard: 2.5 V,	 Current Strength: Default
// VGA_R[4]	=>  Location: PIN_C12,	 I/O Standard: 2.5 V,	 Current Strength: Default
// VGA_R[5]	=>  Location: PIN_D12,	 I/O Standard: 2.5 V,	 Current Strength: Default
// VGA_R[6]	=>  Location: PIN_E12,	 I/O Standard: 2.5 V,	 Current Strength: Default
// VGA_R[7]	=>  Location: PIN_F13,	 I/O Standard: 2.5 V,	 Current Strength: Default
// VGA_G[0]	=>  Location: PIN_J9,	 I/O Standard: 2.5 V,	 Current Strength: Default
// VGA_G[1]	=>  Location: PIN_J10,	 I/O Standard: 2.5 V,	 Current Strength: Default
// VGA_G[2]	=>  Location: PIN_H12,	 I/O Standard: 2.5 V,	 Current Strength: Default
// VGA_G[3]	=>  Location: PIN_G10,	 I/O Standard: 2.5 V,	 Current Strength: Default
// VGA_G[4]	=>  Location: PIN_G11,	 I/O Standard: 2.5 V,	 Current Strength: Default
// VGA_G[5]	=>  Location: PIN_G12,	 I/O Standard: 2.5 V,	 Current Strength: Default
// VGA_G[6]	=>  Location: PIN_F11,	 I/O Standard: 2.5 V,	 Current Strength: Default
// VGA_G[7]	=>  Location: PIN_E11,	 I/O Standard: 2.5 V,	 Current Strength: Default
// VGA_B[0]	=>  Location: PIN_B13,	 I/O Standard: 2.5 V,	 Current Strength: Default
// VGA_B[1]	=>  Location: PIN_G13,	 I/O Standard: 2.5 V,	 Current Strength: Default
// VGA_B[2]	=>  Location: PIN_H13,	 I/O Standard: 2.5 V,	 Current Strength: Default
// VGA_B[3]	=>  Location: PIN_F14,	 I/O Standard: 2.5 V,	 Current Strength: Default
// VGA_B[4]	=>  Location: PIN_H14,	 I/O Standard: 2.5 V,	 Current Strength: Default
// VGA_B[5]	=>  Location: PIN_F15,	 I/O Standard: 2.5 V,	 Current Strength: Default
// VGA_B[6]	=>  Location: PIN_G15,	 I/O Standard: 2.5 V,	 Current Strength: Default
// VGA_B[7]	=>  Location: PIN_J14,	 I/O Standard: 2.5 V,	 Current Strength: Default
// SW[9]	=>  Location: PIN_AE12,	 I/O Standard: 2.5 V,	 Current Strength: Default
// KEY[3]	=>  Location: PIN_Y16,	 I/O Standard: 2.5 V,	 Current Strength: Default
// KEY[0]	=>  Location: PIN_AA14,	 I/O Standard: 2.5 V,	 Current Strength: Default
// CLOCK_50	=>  Location: PIN_AF14,	 I/O Standard: 2.5 V,	 Current Strength: Default


wire gnd;
wire vcc;
wire unknown;

assign gnd = 1'b0;
assign vcc = 1'b1;
assign unknown = 1'bx;

tri1 devclrn;
tri1 devpor;
tri1 devoe;
wire \KEY[1]~input_o ;
wire \KEY[2]~input_o ;
wire \SW[0]~input_o ;
wire \SW[1]~input_o ;
wire \SW[2]~input_o ;
wire \SW[3]~input_o ;
wire \SW[4]~input_o ;
wire \SW[5]~input_o ;
wire \SW[6]~input_o ;
wire \SW[7]~input_o ;
wire \SW[8]~input_o ;
wire \~QUARTUS_CREATED_GND~I_combout ;
wire \SW[9]~input_o ;
wire \KEY[3]~input_o ;
wire \CLOCK_50~input_o ;
wire \KEY[0]~input_o ;
wire \rClk_c[0]~0_combout ;
wire \vga_control|Add3~37_sumout ;
wire \vga_control|Add3~18 ;
wire \vga_control|Add3~33_sumout ;
wire \vga_control|Add3~34 ;
wire \vga_control|Add3~29_sumout ;
wire \vga_control|Add3~30 ;
wire \vga_control|Add3~25_sumout ;
wire \vga_control|h_cont[8]~DUPLICATE_q ;
wire \vga_control|LessThan7~0_combout ;
wire \vga_control|LessThan7~1_combout ;
wire \vga_control|Add3~38 ;
wire \vga_control|Add3~41_sumout ;
wire \vga_control|Add3~42 ;
wire \vga_control|Add3~49_sumout ;
wire \vga_control|h_cont[2]~DUPLICATE_q ;
wire \vga_control|Add3~50 ;
wire \vga_control|Add3~45_sumout ;
wire \vga_control|Add3~46 ;
wire \vga_control|Add3~5_sumout ;
wire \vga_control|h_cont[4]~DUPLICATE_q ;
wire \vga_control|Add3~6 ;
wire \vga_control|Add3~13_sumout ;
wire \vga_control|Add3~14 ;
wire \vga_control|Add3~9_sumout ;
wire \vga_control|h_cont[6]~DUPLICATE_q ;
wire \vga_control|Add3~10 ;
wire \vga_control|Add3~1_sumout ;
wire \vga_control|Add3~2 ;
wire \vga_control|Add3~21_sumout ;
wire \vga_control|Add3~22 ;
wire \vga_control|Add3~17_sumout ;
wire \vga_control|Equal0~0_combout ;
wire \vga_control|LessThan8~0_combout ;
wire \vga_control|mVGA_H_SYNC~q ;
wire \vga_control|ovga_h_sync~q ;
wire \vga_control|Add4~5_sumout ;
wire \vga_control|Equal0~1_combout ;
wire \vga_control|Equal0~2_combout ;
wire \vga_control|Add4~6 ;
wire \vga_control|Add4~1_sumout ;
wire \vga_control|V_Cont[1]~DUPLICATE_q ;
wire \vga_control|Add4~2 ;
wire \vga_control|Add4~17_sumout ;
wire \vga_control|V_Cont[2]~DUPLICATE_q ;
wire \vga_control|Add4~18 ;
wire \vga_control|Add4~14 ;
wire \vga_control|Add4~9_sumout ;
wire \vga_control|V_Cont[4]~DUPLICATE_q ;
wire \vga_control|Add4~10 ;
wire \vga_control|Add4~21_sumout ;
wire \vga_control|V_Cont[5]~DUPLICATE_q ;
wire \vga_control|Add4~22 ;
wire \vga_control|Add4~33_sumout ;
wire \vga_control|V_Cont[6]~DUPLICATE_q ;
wire \vga_control|Add4~34 ;
wire \vga_control|Add4~29_sumout ;
wire \vga_control|V_Cont[7]~DUPLICATE_q ;
wire \vga_control|Add4~30 ;
wire \vga_control|Add4~25_sumout ;
wire \vga_control|V_Cont[8]~DUPLICATE_q ;
wire \vga_control|Add4~26 ;
wire \vga_control|Add4~37_sumout ;
wire \vga_control|V_Cont[9]~DUPLICATE_q ;
wire \vga_control|Add4~38 ;
wire \vga_control|Add4~49_sumout ;
wire \vga_control|V_Cont[10]~DUPLICATE_q ;
wire \vga_control|Add4~50 ;
wire \vga_control|Add4~45_sumout ;
wire \vga_control|V_Cont[11]~DUPLICATE_q ;
wire \vga_control|Add4~46 ;
wire \vga_control|Add4~41_sumout ;
wire \vga_control|V_Cont[12]~DUPLICATE_q ;
wire \vga_control|mvga_r~5_combout ;
wire \vga_control|LessThan6~2_combout ;
wire \vga_control|V_Cont[0]~DUPLICATE_q ;
wire \vga_control|LessThan9~0_combout ;
wire \vga_control|LessThan9~1_combout ;
wire \vga_control|Add4~13_sumout ;
wire \vga_control|V_Cont[3]~DUPLICATE_q ;
wire \vga_control|mVGA_V_SYNC~DUPLICATE_q ;
wire \vga_control|LessThan10~0_combout ;
wire \vga_control|mVGA_V_SYNC~0_combout ;
wire \vga_control|mVGA_V_SYNC~q ;
wire \vga_control|ovga_v_sync~q ;
wire \vga_control|mVGA_BLANK~combout ;
wire \vga_control|ovga_blank~q ;
wire \vga_control|mvga_r~1_combout ;
wire \vga_control|mvga_r~0_combout ;
wire \vga_control|LessThan6~1_combout ;
wire \vga_control|LessThan6~0_combout ;
wire \vga_control|mvga_r~2_combout ;
wire \CLOCK_50~inputCLKENA0_outclk ;
wire \vga_control|Add2~26 ;
wire \vga_control|Add2~30 ;
wire \vga_control|Add2~18 ;
wire \vga_control|Add2~22 ;
wire \vga_control|Add2~34 ;
wire \vga_control|Add2~14 ;
wire \vga_control|Add2~38 ;
wire \vga_control|Add2~42 ;
wire \vga_control|Add2~5_sumout ;
wire \vga_control|Add2~6 ;
wire \vga_control|Add2~9_sumout ;
wire \vga_control|Add2~10 ;
wire \vga_control|Add2~1_sumout ;
wire \vga_control|Add2~2 ;
wire \vga_control|Add2~45_sumout ;
wire \red_c~0_combout ;
wire \vga_control|Add2~41_sumout ;
wire \vga_control|Add2~37_sumout ;
wire \LessThan4~0_combout ;
wire \vga_control|Add2~13_sumout ;
wire \vga_control|Add2~29_sumout ;
wire \vga_control|row[0]~0_combout ;
wire \vga_control|row[0]~DUPLICATE_q ;
wire \vga_control|Add2~25_sumout ;
wire \vga_control|row[1]~DUPLICATE_q ;
wire \vga_control|Add2~17_sumout ;
wire \vga_control|row[3]~DUPLICATE_q ;
wire \vga_control|Add2~21_sumout ;
wire \vga_control|row[4]~DUPLICATE_q ;
wire \vga_control|Add2~33_sumout ;
wire \vga_control|row[5]~DUPLICATE_q ;
wire \LessThan2~0_combout ;
wire \red_c~1_combout ;
wire \LessThan4~1_combout ;
wire \LessThan4~2_combout ;
wire \vga_control|Add1~50_cout ;
wire \vga_control|Add1~46_cout ;
wire \vga_control|Add1~18 ;
wire \vga_control|Add1~5_sumout ;
wire \vga_control|Add1~17_sumout ;
wire \vga_control|Add1~6 ;
wire \vga_control|Add1~10 ;
wire \vga_control|Add1~13_sumout ;
wire \vga_control|Add1~9_sumout ;
wire \vga_control|Add1~14 ;
wire \vga_control|Add1~38 ;
wire \vga_control|Add1~42 ;
wire \vga_control|Add1~1_sumout ;
wire \always1~0_combout ;
wire \LessThan3~0_combout ;
wire \vga_control|row[8]~DUPLICATE_q ;
wire \vga_control|Add1~2 ;
wire \vga_control|Add1~22 ;
wire \vga_control|Add1~26 ;
wire \vga_control|Add1~29_sumout ;
wire \vga_control|Add1~21_sumout ;
wire \vga_control|Add1~30 ;
wire \vga_control|Add1~33_sumout ;
wire \vga_control|Add1~25_sumout ;
wire \always1~1_combout ;
wire \vga_control|Add1~41_sumout ;
wire \vga_control|Add1~37_sumout ;
wire \always1~2_combout ;
wire \always1~3_combout ;
wire \LessThan1~1_combout ;
wire \LessThan1~0_combout ;
wire \LessThan1~2_combout ;
wire \red_c[0]~2_combout ;
wire \vga_control|mvga_r[0]~3_combout ;
wire \vga_control|ored[1]~feeder_combout ;
wire \LessThan0~0_combout ;
wire \LessThan0~1_combout ;
wire \red_c[2]~3_combout ;
wire \vga_control|mvga_r[2]~4_combout ;
wire \vga_control|ored[3]~feeder_combout ;
wire \vga_control|ored[4]~feeder_combout ;
wire \vga_control|ored[6]~feeder_combout ;
wire \LessThan0~2_combout ;
wire \green_c[2]~0_combout ;
wire \always1~4_combout ;
wire \green_c[0]~1_combout ;
wire \vga_control|mVGA_G[0]~0_combout ;
wire \green_c[1]~2_combout ;
wire \vga_control|mVGA_G[1]~1_combout ;
wire \green_c[2]~3_combout ;
wire \vga_control|mVGA_G[2]~2_combout ;
wire \green_c[3]~4_combout ;
wire \vga_control|mVGA_G[3]~3_combout ;
wire \blue_c[0]~0_combout ;
wire \vga_control|mVGA_B[0]~0_combout ;
wire \vga_control|oblue[0]~feeder_combout ;
wire \vga_control|oblue[2]~feeder_combout ;
wire \blue_c[4]~1_combout ;
wire \vga_control|mVGA_B[4]~1_combout ;
wire [9:0] \vga_control|ored ;
wire [1:0] rClk;
wire [12:0] \vga_control|V_Cont ;
wire [7:0] red;
wire [12:0] \vga_control|h_cont ;
wire [9:0] \vga_control|ogreen ;
wire [7:0] green;
wire [9:0] \vga_control|oblue ;
wire [7:0] blue;
wire [12:0] \vga_control|row ;
wire [12:0] \vga_control|col ;


// Location: IOOBUF_X52_Y0_N2
cyclonev_io_obuf \LEDR[0]~output (
	.i(\SW[9]~input_o ),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(LEDR[0]),
	.obar());
// synopsys translate_off
defparam \LEDR[0]~output .bus_hold = "false";
defparam \LEDR[0]~output .open_drain_output = "false";
defparam \LEDR[0]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X52_Y0_N19
cyclonev_io_obuf \LEDR[1]~output (
	.i(gnd),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(LEDR[1]),
	.obar());
// synopsys translate_off
defparam \LEDR[1]~output .bus_hold = "false";
defparam \LEDR[1]~output .open_drain_output = "false";
defparam \LEDR[1]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X60_Y0_N2
cyclonev_io_obuf \LEDR[2]~output (
	.i(gnd),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(LEDR[2]),
	.obar());
// synopsys translate_off
defparam \LEDR[2]~output .bus_hold = "false";
defparam \LEDR[2]~output .open_drain_output = "false";
defparam \LEDR[2]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X80_Y0_N2
cyclonev_io_obuf \LEDR[3]~output (
	.i(gnd),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(LEDR[3]),
	.obar());
// synopsys translate_off
defparam \LEDR[3]~output .bus_hold = "false";
defparam \LEDR[3]~output .open_drain_output = "false";
defparam \LEDR[3]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X60_Y0_N19
cyclonev_io_obuf \LEDR[4]~output (
	.i(gnd),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(LEDR[4]),
	.obar());
// synopsys translate_off
defparam \LEDR[4]~output .bus_hold = "false";
defparam \LEDR[4]~output .open_drain_output = "false";
defparam \LEDR[4]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X80_Y0_N19
cyclonev_io_obuf \LEDR[5]~output (
	.i(gnd),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(LEDR[5]),
	.obar());
// synopsys translate_off
defparam \LEDR[5]~output .bus_hold = "false";
defparam \LEDR[5]~output .open_drain_output = "false";
defparam \LEDR[5]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X84_Y0_N2
cyclonev_io_obuf \LEDR[6]~output (
	.i(gnd),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(LEDR[6]),
	.obar());
// synopsys translate_off
defparam \LEDR[6]~output .bus_hold = "false";
defparam \LEDR[6]~output .open_drain_output = "false";
defparam \LEDR[6]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X89_Y6_N5
cyclonev_io_obuf \LEDR[7]~output (
	.i(gnd),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(LEDR[7]),
	.obar());
// synopsys translate_off
defparam \LEDR[7]~output .bus_hold = "false";
defparam \LEDR[7]~output .open_drain_output = "false";
defparam \LEDR[7]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X89_Y8_N5
cyclonev_io_obuf \LEDR[8]~output (
	.i(gnd),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(LEDR[8]),
	.obar());
// synopsys translate_off
defparam \LEDR[8]~output .bus_hold = "false";
defparam \LEDR[8]~output .open_drain_output = "false";
defparam \LEDR[8]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X89_Y6_N22
cyclonev_io_obuf \LEDR[9]~output (
	.i(gnd),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(LEDR[9]),
	.obar());
// synopsys translate_off
defparam \LEDR[9]~output .bus_hold = "false";
defparam \LEDR[9]~output .open_drain_output = "false";
defparam \LEDR[9]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X89_Y8_N39
cyclonev_io_obuf \HEX0[0]~output (
	.i(\KEY[3]~input_o ),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(HEX0[0]),
	.obar());
// synopsys translate_off
defparam \HEX0[0]~output .bus_hold = "false";
defparam \HEX0[0]~output .open_drain_output = "false";
defparam \HEX0[0]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X89_Y11_N79
cyclonev_io_obuf \HEX0[1]~output (
	.i(gnd),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(HEX0[1]),
	.obar());
// synopsys translate_off
defparam \HEX0[1]~output .bus_hold = "false";
defparam \HEX0[1]~output .open_drain_output = "false";
defparam \HEX0[1]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X89_Y11_N96
cyclonev_io_obuf \HEX0[2]~output (
	.i(gnd),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(HEX0[2]),
	.obar());
// synopsys translate_off
defparam \HEX0[2]~output .bus_hold = "false";
defparam \HEX0[2]~output .open_drain_output = "false";
defparam \HEX0[2]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X89_Y4_N79
cyclonev_io_obuf \HEX0[3]~output (
	.i(gnd),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(HEX0[3]),
	.obar());
// synopsys translate_off
defparam \HEX0[3]~output .bus_hold = "false";
defparam \HEX0[3]~output .open_drain_output = "false";
defparam \HEX0[3]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X89_Y13_N56
cyclonev_io_obuf \HEX0[4]~output (
	.i(gnd),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(HEX0[4]),
	.obar());
// synopsys translate_off
defparam \HEX0[4]~output .bus_hold = "false";
defparam \HEX0[4]~output .open_drain_output = "false";
defparam \HEX0[4]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X89_Y13_N39
cyclonev_io_obuf \HEX0[5]~output (
	.i(gnd),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(HEX0[5]),
	.obar());
// synopsys translate_off
defparam \HEX0[5]~output .bus_hold = "false";
defparam \HEX0[5]~output .open_drain_output = "false";
defparam \HEX0[5]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X89_Y4_N96
cyclonev_io_obuf \HEX0[6]~output (
	.i(gnd),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(HEX0[6]),
	.obar());
// synopsys translate_off
defparam \HEX0[6]~output .bus_hold = "false";
defparam \HEX0[6]~output .open_drain_output = "false";
defparam \HEX0[6]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X60_Y0_N36
cyclonev_io_obuf \HEX0[7]~output (
	.i(gnd),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(HEX0[7]),
	.obar());
// synopsys translate_off
defparam \HEX0[7]~output .bus_hold = "false";
defparam \HEX0[7]~output .open_drain_output = "false";
defparam \HEX0[7]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X89_Y6_N39
cyclonev_io_obuf \HEX1[0]~output (
	.i(gnd),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(HEX1[0]),
	.obar());
// synopsys translate_off
defparam \HEX1[0]~output .bus_hold = "false";
defparam \HEX1[0]~output .open_drain_output = "false";
defparam \HEX1[0]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X89_Y6_N56
cyclonev_io_obuf \HEX1[1]~output (
	.i(gnd),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(HEX1[1]),
	.obar());
// synopsys translate_off
defparam \HEX1[1]~output .bus_hold = "false";
defparam \HEX1[1]~output .open_drain_output = "false";
defparam \HEX1[1]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X89_Y16_N39
cyclonev_io_obuf \HEX1[2]~output (
	.i(gnd),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(HEX1[2]),
	.obar());
// synopsys translate_off
defparam \HEX1[2]~output .bus_hold = "false";
defparam \HEX1[2]~output .open_drain_output = "false";
defparam \HEX1[2]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X89_Y16_N56
cyclonev_io_obuf \HEX1[3]~output (
	.i(gnd),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(HEX1[3]),
	.obar());
// synopsys translate_off
defparam \HEX1[3]~output .bus_hold = "false";
defparam \HEX1[3]~output .open_drain_output = "false";
defparam \HEX1[3]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X89_Y15_N39
cyclonev_io_obuf \HEX1[4]~output (
	.i(gnd),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(HEX1[4]),
	.obar());
// synopsys translate_off
defparam \HEX1[4]~output .bus_hold = "false";
defparam \HEX1[4]~output .open_drain_output = "false";
defparam \HEX1[4]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X89_Y15_N56
cyclonev_io_obuf \HEX1[5]~output (
	.i(gnd),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(HEX1[5]),
	.obar());
// synopsys translate_off
defparam \HEX1[5]~output .bus_hold = "false";
defparam \HEX1[5]~output .open_drain_output = "false";
defparam \HEX1[5]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X89_Y8_N56
cyclonev_io_obuf \HEX1[6]~output (
	.i(gnd),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(HEX1[6]),
	.obar());
// synopsys translate_off
defparam \HEX1[6]~output .bus_hold = "false";
defparam \HEX1[6]~output .open_drain_output = "false";
defparam \HEX1[6]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X89_Y9_N39
cyclonev_io_obuf \HEX1[7]~output (
	.i(gnd),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(HEX1[7]),
	.obar());
// synopsys translate_off
defparam \HEX1[7]~output .bus_hold = "false";
defparam \HEX1[7]~output .open_drain_output = "false";
defparam \HEX1[7]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X89_Y9_N22
cyclonev_io_obuf \HEX2[0]~output (
	.i(gnd),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(HEX2[0]),
	.obar());
// synopsys translate_off
defparam \HEX2[0]~output .bus_hold = "false";
defparam \HEX2[0]~output .open_drain_output = "false";
defparam \HEX2[0]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X89_Y23_N39
cyclonev_io_obuf \HEX2[1]~output (
	.i(gnd),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(HEX2[1]),
	.obar());
// synopsys translate_off
defparam \HEX2[1]~output .bus_hold = "false";
defparam \HEX2[1]~output .open_drain_output = "false";
defparam \HEX2[1]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X89_Y23_N56
cyclonev_io_obuf \HEX2[2]~output (
	.i(gnd),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(HEX2[2]),
	.obar());
// synopsys translate_off
defparam \HEX2[2]~output .bus_hold = "false";
defparam \HEX2[2]~output .open_drain_output = "false";
defparam \HEX2[2]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X89_Y20_N79
cyclonev_io_obuf \HEX2[3]~output (
	.i(gnd),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(HEX2[3]),
	.obar());
// synopsys translate_off
defparam \HEX2[3]~output .bus_hold = "false";
defparam \HEX2[3]~output .open_drain_output = "false";
defparam \HEX2[3]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X89_Y25_N39
cyclonev_io_obuf \HEX2[4]~output (
	.i(gnd),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(HEX2[4]),
	.obar());
// synopsys translate_off
defparam \HEX2[4]~output .bus_hold = "false";
defparam \HEX2[4]~output .open_drain_output = "false";
defparam \HEX2[4]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X89_Y20_N96
cyclonev_io_obuf \HEX2[5]~output (
	.i(gnd),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(HEX2[5]),
	.obar());
// synopsys translate_off
defparam \HEX2[5]~output .bus_hold = "false";
defparam \HEX2[5]~output .open_drain_output = "false";
defparam \HEX2[5]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X89_Y25_N56
cyclonev_io_obuf \HEX2[6]~output (
	.i(gnd),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(HEX2[6]),
	.obar());
// synopsys translate_off
defparam \HEX2[6]~output .bus_hold = "false";
defparam \HEX2[6]~output .open_drain_output = "false";
defparam \HEX2[6]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X24_Y81_N19
cyclonev_io_obuf \HEX2[7]~output (
	.i(gnd),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(HEX2[7]),
	.obar());
// synopsys translate_off
defparam \HEX2[7]~output .bus_hold = "false";
defparam \HEX2[7]~output .open_drain_output = "false";
defparam \HEX2[7]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X89_Y16_N5
cyclonev_io_obuf \HEX3[0]~output (
	.i(gnd),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(HEX3[0]),
	.obar());
// synopsys translate_off
defparam \HEX3[0]~output .bus_hold = "false";
defparam \HEX3[0]~output .open_drain_output = "false";
defparam \HEX3[0]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X89_Y16_N22
cyclonev_io_obuf \HEX3[1]~output (
	.i(gnd),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(HEX3[1]),
	.obar());
// synopsys translate_off
defparam \HEX3[1]~output .bus_hold = "false";
defparam \HEX3[1]~output .open_drain_output = "false";
defparam \HEX3[1]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X89_Y4_N45
cyclonev_io_obuf \HEX3[2]~output (
	.i(gnd),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(HEX3[2]),
	.obar());
// synopsys translate_off
defparam \HEX3[2]~output .bus_hold = "false";
defparam \HEX3[2]~output .open_drain_output = "false";
defparam \HEX3[2]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X89_Y4_N62
cyclonev_io_obuf \HEX3[3]~output (
	.i(gnd),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(HEX3[3]),
	.obar());
// synopsys translate_off
defparam \HEX3[3]~output .bus_hold = "false";
defparam \HEX3[3]~output .open_drain_output = "false";
defparam \HEX3[3]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X89_Y21_N39
cyclonev_io_obuf \HEX3[4]~output (
	.i(gnd),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(HEX3[4]),
	.obar());
// synopsys translate_off
defparam \HEX3[4]~output .bus_hold = "false";
defparam \HEX3[4]~output .open_drain_output = "false";
defparam \HEX3[4]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X89_Y11_N62
cyclonev_io_obuf \HEX3[5]~output (
	.i(gnd),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(HEX3[5]),
	.obar());
// synopsys translate_off
defparam \HEX3[5]~output .bus_hold = "false";
defparam \HEX3[5]~output .open_drain_output = "false";
defparam \HEX3[5]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X89_Y9_N5
cyclonev_io_obuf \HEX3[6]~output (
	.i(gnd),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(HEX3[6]),
	.obar());
// synopsys translate_off
defparam \HEX3[6]~output .bus_hold = "false";
defparam \HEX3[6]~output .open_drain_output = "false";
defparam \HEX3[6]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X58_Y0_N42
cyclonev_io_obuf \HEX3[7]~output (
	.i(gnd),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(HEX3[7]),
	.obar());
// synopsys translate_off
defparam \HEX3[7]~output .bus_hold = "false";
defparam \HEX3[7]~output .open_drain_output = "false";
defparam \HEX3[7]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X80_Y0_N53
cyclonev_io_obuf \HEX4[0]~output (
	.i(gnd),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(HEX4[0]),
	.obar());
// synopsys translate_off
defparam \HEX4[0]~output .bus_hold = "false";
defparam \HEX4[0]~output .open_drain_output = "false";
defparam \HEX4[0]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X64_Y0_N19
cyclonev_io_obuf \HEX4[1]~output (
	.i(gnd),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(HEX4[1]),
	.obar());
// synopsys translate_off
defparam \HEX4[1]~output .bus_hold = "false";
defparam \HEX4[1]~output .open_drain_output = "false";
defparam \HEX4[1]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X6_Y81_N53
cyclonev_io_obuf \HEX4[2]~output (
	.i(gnd),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(HEX4[2]),
	.obar());
// synopsys translate_off
defparam \HEX4[2]~output .bus_hold = "false";
defparam \HEX4[2]~output .open_drain_output = "false";
defparam \HEX4[2]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X18_Y0_N93
cyclonev_io_obuf \HEX4[3]~output (
	.i(gnd),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(HEX4[3]),
	.obar());
// synopsys translate_off
defparam \HEX4[3]~output .bus_hold = "false";
defparam \HEX4[3]~output .open_drain_output = "false";
defparam \HEX4[3]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X89_Y15_N5
cyclonev_io_obuf \HEX4[4]~output (
	.i(gnd),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(HEX4[4]),
	.obar());
// synopsys translate_off
defparam \HEX4[4]~output .bus_hold = "false";
defparam \HEX4[4]~output .open_drain_output = "false";
defparam \HEX4[4]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X2_Y81_N42
cyclonev_io_obuf \HEX4[5]~output (
	.i(gnd),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(HEX4[5]),
	.obar());
// synopsys translate_off
defparam \HEX4[5]~output .bus_hold = "false";
defparam \HEX4[5]~output .open_drain_output = "false";
defparam \HEX4[5]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X16_Y81_N2
cyclonev_io_obuf \HEX4[6]~output (
	.i(gnd),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(HEX4[6]),
	.obar());
// synopsys translate_off
defparam \HEX4[6]~output .bus_hold = "false";
defparam \HEX4[6]~output .open_drain_output = "false";
defparam \HEX4[6]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X56_Y0_N19
cyclonev_io_obuf \HEX4[7]~output (
	.i(gnd),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(HEX4[7]),
	.obar());
// synopsys translate_off
defparam \HEX4[7]~output .bus_hold = "false";
defparam \HEX4[7]~output .open_drain_output = "false";
defparam \HEX4[7]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X8_Y0_N19
cyclonev_io_obuf \HEX5[0]~output (
	.i(gnd),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(HEX5[0]),
	.obar());
// synopsys translate_off
defparam \HEX5[0]~output .bus_hold = "false";
defparam \HEX5[0]~output .open_drain_output = "false";
defparam \HEX5[0]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X50_Y0_N59
cyclonev_io_obuf \HEX5[1]~output (
	.i(gnd),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(HEX5[1]),
	.obar());
// synopsys translate_off
defparam \HEX5[1]~output .bus_hold = "false";
defparam \HEX5[1]~output .open_drain_output = "false";
defparam \HEX5[1]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X30_Y81_N53
cyclonev_io_obuf \HEX5[2]~output (
	.i(gnd),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(HEX5[2]),
	.obar());
// synopsys translate_off
defparam \HEX5[2]~output .bus_hold = "false";
defparam \HEX5[2]~output .open_drain_output = "false";
defparam \HEX5[2]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X64_Y0_N36
cyclonev_io_obuf \HEX5[3]~output (
	.i(gnd),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(HEX5[3]),
	.obar());
// synopsys translate_off
defparam \HEX5[3]~output .bus_hold = "false";
defparam \HEX5[3]~output .open_drain_output = "false";
defparam \HEX5[3]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X86_Y0_N19
cyclonev_io_obuf \HEX5[4]~output (
	.i(gnd),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(HEX5[4]),
	.obar());
// synopsys translate_off
defparam \HEX5[4]~output .bus_hold = "false";
defparam \HEX5[4]~output .open_drain_output = "false";
defparam \HEX5[4]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X8_Y0_N53
cyclonev_io_obuf \HEX5[5]~output (
	.i(gnd),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(HEX5[5]),
	.obar());
// synopsys translate_off
defparam \HEX5[5]~output .bus_hold = "false";
defparam \HEX5[5]~output .open_drain_output = "false";
defparam \HEX5[5]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X89_Y23_N5
cyclonev_io_obuf \HEX5[6]~output (
	.i(gnd),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(HEX5[6]),
	.obar());
// synopsys translate_off
defparam \HEX5[6]~output .bus_hold = "false";
defparam \HEX5[6]~output .open_drain_output = "false";
defparam \HEX5[6]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X26_Y81_N93
cyclonev_io_obuf \HEX5[7]~output (
	.i(gnd),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(HEX5[7]),
	.obar());
// synopsys translate_off
defparam \HEX5[7]~output .bus_hold = "false";
defparam \HEX5[7]~output .open_drain_output = "false";
defparam \HEX5[7]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X38_Y81_N36
cyclonev_io_obuf \VGA_CLK~output (
	.i(!rClk[0]),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(VGA_CLK),
	.obar());
// synopsys translate_off
defparam \VGA_CLK~output .bus_hold = "false";
defparam \VGA_CLK~output .open_drain_output = "false";
defparam \VGA_CLK~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X36_Y81_N53
cyclonev_io_obuf \VGA_HS~output (
	.i(\vga_control|ovga_h_sync~q ),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(VGA_HS),
	.obar());
// synopsys translate_off
defparam \VGA_HS~output .bus_hold = "false";
defparam \VGA_HS~output .open_drain_output = "false";
defparam \VGA_HS~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X34_Y81_N42
cyclonev_io_obuf \VGA_VS~output (
	.i(\vga_control|ovga_v_sync~q ),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(VGA_VS),
	.obar());
// synopsys translate_off
defparam \VGA_VS~output .bus_hold = "false";
defparam \VGA_VS~output .open_drain_output = "false";
defparam \VGA_VS~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X6_Y81_N19
cyclonev_io_obuf \VGA_BLANK_N~output (
	.i(\vga_control|ovga_blank~q ),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(VGA_BLANK_N),
	.obar());
// synopsys translate_off
defparam \VGA_BLANK_N~output .bus_hold = "false";
defparam \VGA_BLANK_N~output .open_drain_output = "false";
defparam \VGA_BLANK_N~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X28_Y81_N36
cyclonev_io_obuf \VGA_SYNC_N~output (
	.i(gnd),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(VGA_SYNC_N),
	.obar());
// synopsys translate_off
defparam \VGA_SYNC_N~output .bus_hold = "false";
defparam \VGA_SYNC_N~output .open_drain_output = "false";
defparam \VGA_SYNC_N~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X40_Y81_N53
cyclonev_io_obuf \VGA_R[0]~output (
	.i(\vga_control|ored [0]),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(VGA_R[0]),
	.obar());
// synopsys translate_off
defparam \VGA_R[0]~output .bus_hold = "false";
defparam \VGA_R[0]~output .open_drain_output = "false";
defparam \VGA_R[0]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X38_Y81_N2
cyclonev_io_obuf \VGA_R[1]~output (
	.i(\vga_control|ored [1]),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(VGA_R[1]),
	.obar());
// synopsys translate_off
defparam \VGA_R[1]~output .bus_hold = "false";
defparam \VGA_R[1]~output .open_drain_output = "false";
defparam \VGA_R[1]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X26_Y81_N59
cyclonev_io_obuf \VGA_R[2]~output (
	.i(\vga_control|ored [2]),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(VGA_R[2]),
	.obar());
// synopsys translate_off
defparam \VGA_R[2]~output .bus_hold = "false";
defparam \VGA_R[2]~output .open_drain_output = "false";
defparam \VGA_R[2]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X38_Y81_N19
cyclonev_io_obuf \VGA_R[3]~output (
	.i(\vga_control|ored [3]),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(VGA_R[3]),
	.obar());
// synopsys translate_off
defparam \VGA_R[3]~output .bus_hold = "false";
defparam \VGA_R[3]~output .open_drain_output = "false";
defparam \VGA_R[3]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X36_Y81_N36
cyclonev_io_obuf \VGA_R[4]~output (
	.i(\vga_control|ored [4]),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(VGA_R[4]),
	.obar());
// synopsys translate_off
defparam \VGA_R[4]~output .bus_hold = "false";
defparam \VGA_R[4]~output .open_drain_output = "false";
defparam \VGA_R[4]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X22_Y81_N19
cyclonev_io_obuf \VGA_R[5]~output (
	.i(\vga_control|ored [5]),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(VGA_R[5]),
	.obar());
// synopsys translate_off
defparam \VGA_R[5]~output .bus_hold = "false";
defparam \VGA_R[5]~output .open_drain_output = "false";
defparam \VGA_R[5]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X22_Y81_N2
cyclonev_io_obuf \VGA_R[6]~output (
	.i(\vga_control|ored [6]),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(VGA_R[6]),
	.obar());
// synopsys translate_off
defparam \VGA_R[6]~output .bus_hold = "false";
defparam \VGA_R[6]~output .open_drain_output = "false";
defparam \VGA_R[6]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X26_Y81_N42
cyclonev_io_obuf \VGA_R[7]~output (
	.i(\vga_control|ored [7]),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(VGA_R[7]),
	.obar());
// synopsys translate_off
defparam \VGA_R[7]~output .bus_hold = "false";
defparam \VGA_R[7]~output .open_drain_output = "false";
defparam \VGA_R[7]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X4_Y81_N19
cyclonev_io_obuf \VGA_G[0]~output (
	.i(\vga_control|ogreen [0]),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(VGA_G[0]),
	.obar());
// synopsys translate_off
defparam \VGA_G[0]~output .bus_hold = "false";
defparam \VGA_G[0]~output .open_drain_output = "false";
defparam \VGA_G[0]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X4_Y81_N2
cyclonev_io_obuf \VGA_G[1]~output (
	.i(\vga_control|ogreen [1]),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(VGA_G[1]),
	.obar());
// synopsys translate_off
defparam \VGA_G[1]~output .bus_hold = "false";
defparam \VGA_G[1]~output .open_drain_output = "false";
defparam \VGA_G[1]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X20_Y81_N19
cyclonev_io_obuf \VGA_G[2]~output (
	.i(\vga_control|ogreen [2]),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(VGA_G[2]),
	.obar());
// synopsys translate_off
defparam \VGA_G[2]~output .bus_hold = "false";
defparam \VGA_G[2]~output .open_drain_output = "false";
defparam \VGA_G[2]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X6_Y81_N2
cyclonev_io_obuf \VGA_G[3]~output (
	.i(\vga_control|ogreen [3]),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(VGA_G[3]),
	.obar());
// synopsys translate_off
defparam \VGA_G[3]~output .bus_hold = "false";
defparam \VGA_G[3]~output .open_drain_output = "false";
defparam \VGA_G[3]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X10_Y81_N59
cyclonev_io_obuf \VGA_G[4]~output (
	.i(\vga_control|ogreen [4]),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(VGA_G[4]),
	.obar());
// synopsys translate_off
defparam \VGA_G[4]~output .bus_hold = "false";
defparam \VGA_G[4]~output .open_drain_output = "false";
defparam \VGA_G[4]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X10_Y81_N42
cyclonev_io_obuf \VGA_G[5]~output (
	.i(\vga_control|ogreen [5]),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(VGA_G[5]),
	.obar());
// synopsys translate_off
defparam \VGA_G[5]~output .bus_hold = "false";
defparam \VGA_G[5]~output .open_drain_output = "false";
defparam \VGA_G[5]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X18_Y81_N42
cyclonev_io_obuf \VGA_G[6]~output (
	.i(\vga_control|ogreen [6]),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(VGA_G[6]),
	.obar());
// synopsys translate_off
defparam \VGA_G[6]~output .bus_hold = "false";
defparam \VGA_G[6]~output .open_drain_output = "false";
defparam \VGA_G[6]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X18_Y81_N59
cyclonev_io_obuf \VGA_G[7]~output (
	.i(\vga_control|ogreen [7]),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(VGA_G[7]),
	.obar());
// synopsys translate_off
defparam \VGA_G[7]~output .bus_hold = "false";
defparam \VGA_G[7]~output .open_drain_output = "false";
defparam \VGA_G[7]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X40_Y81_N36
cyclonev_io_obuf \VGA_B[0]~output (
	.i(\vga_control|oblue [0]),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(VGA_B[0]),
	.obar());
// synopsys translate_off
defparam \VGA_B[0]~output .bus_hold = "false";
defparam \VGA_B[0]~output .open_drain_output = "false";
defparam \VGA_B[0]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X28_Y81_N19
cyclonev_io_obuf \VGA_B[1]~output (
	.i(\vga_control|oblue [1]),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(VGA_B[1]),
	.obar());
// synopsys translate_off
defparam \VGA_B[1]~output .bus_hold = "false";
defparam \VGA_B[1]~output .open_drain_output = "false";
defparam \VGA_B[1]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X20_Y81_N2
cyclonev_io_obuf \VGA_B[2]~output (
	.i(\vga_control|oblue [2]),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(VGA_B[2]),
	.obar());
// synopsys translate_off
defparam \VGA_B[2]~output .bus_hold = "false";
defparam \VGA_B[2]~output .open_drain_output = "false";
defparam \VGA_B[2]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X36_Y81_N19
cyclonev_io_obuf \VGA_B[3]~output (
	.i(\vga_control|oblue [3]),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(VGA_B[3]),
	.obar());
// synopsys translate_off
defparam \VGA_B[3]~output .bus_hold = "false";
defparam \VGA_B[3]~output .open_drain_output = "false";
defparam \VGA_B[3]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X28_Y81_N2
cyclonev_io_obuf \VGA_B[4]~output (
	.i(\vga_control|oblue [4]),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(VGA_B[4]),
	.obar());
// synopsys translate_off
defparam \VGA_B[4]~output .bus_hold = "false";
defparam \VGA_B[4]~output .open_drain_output = "false";
defparam \VGA_B[4]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X36_Y81_N2
cyclonev_io_obuf \VGA_B[5]~output (
	.i(\vga_control|oblue [5]),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(VGA_B[5]),
	.obar());
// synopsys translate_off
defparam \VGA_B[5]~output .bus_hold = "false";
defparam \VGA_B[5]~output .open_drain_output = "false";
defparam \VGA_B[5]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X40_Y81_N19
cyclonev_io_obuf \VGA_B[6]~output (
	.i(\vga_control|oblue [6]),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(VGA_B[6]),
	.obar());
// synopsys translate_off
defparam \VGA_B[6]~output .bus_hold = "false";
defparam \VGA_B[6]~output .open_drain_output = "false";
defparam \VGA_B[6]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOOBUF_X32_Y81_N19
cyclonev_io_obuf \VGA_B[7]~output (
	.i(\vga_control|oblue [7]),
	.oe(vcc),
	.dynamicterminationcontrol(gnd),
	.seriesterminationcontrol(16'b0000000000000000),
	.parallelterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(VGA_B[7]),
	.obar());
// synopsys translate_off
defparam \VGA_B[7]~output .bus_hold = "false";
defparam \VGA_B[7]~output .open_drain_output = "false";
defparam \VGA_B[7]~output .shift_series_termination_control = "false";
// synopsys translate_on

// Location: IOIBUF_X2_Y0_N58
cyclonev_io_ibuf \SW[9]~input (
	.i(SW[9]),
	.ibar(gnd),
	.dynamicterminationcontrol(gnd),
	.o(\SW[9]~input_o ));
// synopsys translate_off
defparam \SW[9]~input .bus_hold = "false";
defparam \SW[9]~input .simulate_z_as = "z";
// synopsys translate_on

// Location: IOIBUF_X40_Y0_N18
cyclonev_io_ibuf \KEY[3]~input (
	.i(KEY[3]),
	.ibar(gnd),
	.dynamicterminationcontrol(gnd),
	.o(\KEY[3]~input_o ));
// synopsys translate_off
defparam \KEY[3]~input .bus_hold = "false";
defparam \KEY[3]~input .simulate_z_as = "z";
// synopsys translate_on

// Location: IOIBUF_X32_Y0_N1
cyclonev_io_ibuf \CLOCK_50~input (
	.i(CLOCK_50),
	.ibar(gnd),
	.dynamicterminationcontrol(gnd),
	.o(\CLOCK_50~input_o ));
// synopsys translate_off
defparam \CLOCK_50~input .bus_hold = "false";
defparam \CLOCK_50~input .simulate_z_as = "z";
// synopsys translate_on

// Location: IOIBUF_X36_Y0_N1
cyclonev_io_ibuf \KEY[0]~input (
	.i(KEY[0]),
	.ibar(gnd),
	.dynamicterminationcontrol(gnd),
	.o(\KEY[0]~input_o ));
// synopsys translate_off
defparam \KEY[0]~input .bus_hold = "false";
defparam \KEY[0]~input .simulate_z_as = "z";
// synopsys translate_on

// Location: LABCELL_X31_Y77_N54
cyclonev_lcell_comb \rClk_c[0]~0 (
// Equation(s):
// \rClk_c[0]~0_combout  = ( !rClk[0] & ( \KEY[0]~input_o  ) )

	.dataa(gnd),
	.datab(gnd),
	.datac(!\KEY[0]~input_o ),
	.datad(gnd),
	.datae(gnd),
	.dataf(!rClk[0]),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(\rClk_c[0]~0_combout ),
	.sumout(),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \rClk_c[0]~0 .extended_lut = "off";
defparam \rClk_c[0]~0 .lut_mask = 64'h0F0F0F0F00000000;
defparam \rClk_c[0]~0 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X31_Y77_N59
dffeas \rClk[0] (
	.clk(\CLOCK_50~input_o ),
	.d(gnd),
	.asdata(\rClk_c[0]~0_combout ),
	.clrn(vcc),
	.aload(gnd),
	.sclr(gnd),
	.sload(vcc),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(rClk[0]),
	.prn(vcc));
// synopsys translate_off
defparam \rClk[0] .is_wysiwyg = "true";
defparam \rClk[0] .power_up = "low";
// synopsys translate_on

// Location: LABCELL_X31_Y77_N0
cyclonev_lcell_comb \vga_control|Add3~37 (
// Equation(s):
// \vga_control|Add3~37_sumout  = SUM(( \vga_control|h_cont [0] ) + ( VCC ) + ( !VCC ))
// \vga_control|Add3~38  = CARRY(( \vga_control|h_cont [0] ) + ( VCC ) + ( !VCC ))

	.dataa(!\vga_control|h_cont [0]),
	.datab(gnd),
	.datac(gnd),
	.datad(gnd),
	.datae(gnd),
	.dataf(gnd),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(),
	.sumout(\vga_control|Add3~37_sumout ),
	.cout(\vga_control|Add3~38 ),
	.shareout());
// synopsys translate_off
defparam \vga_control|Add3~37 .extended_lut = "off";
defparam \vga_control|Add3~37 .lut_mask = 64'h0000000000005555;
defparam \vga_control|Add3~37 .shared_arith = "off";
// synopsys translate_on

// Location: LABCELL_X31_Y77_N27
cyclonev_lcell_comb \vga_control|Add3~17 (
// Equation(s):
// \vga_control|Add3~17_sumout  = SUM(( \vga_control|h_cont [9] ) + ( GND ) + ( \vga_control|Add3~22  ))
// \vga_control|Add3~18  = CARRY(( \vga_control|h_cont [9] ) + ( GND ) + ( \vga_control|Add3~22  ))

	.dataa(!\vga_control|h_cont [9]),
	.datab(gnd),
	.datac(gnd),
	.datad(gnd),
	.datae(gnd),
	.dataf(gnd),
	.datag(gnd),
	.cin(\vga_control|Add3~22 ),
	.sharein(gnd),
	.combout(),
	.sumout(\vga_control|Add3~17_sumout ),
	.cout(\vga_control|Add3~18 ),
	.shareout());
// synopsys translate_off
defparam \vga_control|Add3~17 .extended_lut = "off";
defparam \vga_control|Add3~17 .lut_mask = 64'h0000FFFF00005555;
defparam \vga_control|Add3~17 .shared_arith = "off";
// synopsys translate_on

// Location: LABCELL_X31_Y77_N30
cyclonev_lcell_comb \vga_control|Add3~33 (
// Equation(s):
// \vga_control|Add3~33_sumout  = SUM(( \vga_control|h_cont [10] ) + ( GND ) + ( \vga_control|Add3~18  ))
// \vga_control|Add3~34  = CARRY(( \vga_control|h_cont [10] ) + ( GND ) + ( \vga_control|Add3~18  ))

	.dataa(gnd),
	.datab(!\vga_control|h_cont [10]),
	.datac(gnd),
	.datad(gnd),
	.datae(gnd),
	.dataf(gnd),
	.datag(gnd),
	.cin(\vga_control|Add3~18 ),
	.sharein(gnd),
	.combout(),
	.sumout(\vga_control|Add3~33_sumout ),
	.cout(\vga_control|Add3~34 ),
	.shareout());
// synopsys translate_off
defparam \vga_control|Add3~33 .extended_lut = "off";
defparam \vga_control|Add3~33 .lut_mask = 64'h0000FFFF00003333;
defparam \vga_control|Add3~33 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X31_Y77_N32
dffeas \vga_control|h_cont[10] (
	.clk(rClk[0]),
	.d(\vga_control|Add3~33_sumout ),
	.asdata(vcc),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(\vga_control|LessThan7~1_combout ),
	.sload(gnd),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|h_cont [10]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|h_cont[10] .is_wysiwyg = "true";
defparam \vga_control|h_cont[10] .power_up = "low";
// synopsys translate_on

// Location: LABCELL_X31_Y77_N33
cyclonev_lcell_comb \vga_control|Add3~29 (
// Equation(s):
// \vga_control|Add3~29_sumout  = SUM(( \vga_control|h_cont [11] ) + ( GND ) + ( \vga_control|Add3~34  ))
// \vga_control|Add3~30  = CARRY(( \vga_control|h_cont [11] ) + ( GND ) + ( \vga_control|Add3~34  ))

	.dataa(!\vga_control|h_cont [11]),
	.datab(gnd),
	.datac(gnd),
	.datad(gnd),
	.datae(gnd),
	.dataf(gnd),
	.datag(gnd),
	.cin(\vga_control|Add3~34 ),
	.sharein(gnd),
	.combout(),
	.sumout(\vga_control|Add3~29_sumout ),
	.cout(\vga_control|Add3~30 ),
	.shareout());
// synopsys translate_off
defparam \vga_control|Add3~29 .extended_lut = "off";
defparam \vga_control|Add3~29 .lut_mask = 64'h0000FFFF00005555;
defparam \vga_control|Add3~29 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X31_Y77_N34
dffeas \vga_control|h_cont[11] (
	.clk(rClk[0]),
	.d(\vga_control|Add3~29_sumout ),
	.asdata(vcc),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(\vga_control|LessThan7~1_combout ),
	.sload(gnd),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|h_cont [11]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|h_cont[11] .is_wysiwyg = "true";
defparam \vga_control|h_cont[11] .power_up = "low";
// synopsys translate_on

// Location: LABCELL_X31_Y77_N36
cyclonev_lcell_comb \vga_control|Add3~25 (
// Equation(s):
// \vga_control|Add3~25_sumout  = SUM(( \vga_control|h_cont [12] ) + ( GND ) + ( \vga_control|Add3~30  ))

	.dataa(gnd),
	.datab(gnd),
	.datac(!\vga_control|h_cont [12]),
	.datad(gnd),
	.datae(gnd),
	.dataf(gnd),
	.datag(gnd),
	.cin(\vga_control|Add3~30 ),
	.sharein(gnd),
	.combout(),
	.sumout(\vga_control|Add3~25_sumout ),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \vga_control|Add3~25 .extended_lut = "off";
defparam \vga_control|Add3~25 .lut_mask = 64'h0000FFFF00000F0F;
defparam \vga_control|Add3~25 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X31_Y77_N38
dffeas \vga_control|h_cont[12] (
	.clk(rClk[0]),
	.d(\vga_control|Add3~25_sumout ),
	.asdata(vcc),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(\vga_control|LessThan7~1_combout ),
	.sload(gnd),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|h_cont [12]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|h_cont[12] .is_wysiwyg = "true";
defparam \vga_control|h_cont[12] .power_up = "low";
// synopsys translate_on

// Location: FF_X31_Y77_N26
dffeas \vga_control|h_cont[8]~DUPLICATE (
	.clk(rClk[0]),
	.d(\vga_control|Add3~21_sumout ),
	.asdata(vcc),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(\vga_control|LessThan7~1_combout ),
	.sload(gnd),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|h_cont[8]~DUPLICATE_q ),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|h_cont[8]~DUPLICATE .is_wysiwyg = "true";
defparam \vga_control|h_cont[8]~DUPLICATE .power_up = "low";
// synopsys translate_on

// Location: LABCELL_X30_Y77_N12
cyclonev_lcell_comb \vga_control|LessThan7~0 (
// Equation(s):
// \vga_control|LessThan7~0_combout  = ( \vga_control|h_cont[6]~DUPLICATE_q  & ( \vga_control|h_cont [7] & ( (\vga_control|h_cont [9] & \vga_control|h_cont[8]~DUPLICATE_q ) ) ) ) # ( !\vga_control|h_cont[6]~DUPLICATE_q  & ( \vga_control|h_cont [7] & ( 
// (\vga_control|h_cont [9] & \vga_control|h_cont[8]~DUPLICATE_q ) ) ) ) # ( \vga_control|h_cont[6]~DUPLICATE_q  & ( !\vga_control|h_cont [7] & ( (\vga_control|h_cont [9] & \vga_control|h_cont[8]~DUPLICATE_q ) ) ) ) # ( !\vga_control|h_cont[6]~DUPLICATE_q  & 
// ( !\vga_control|h_cont [7] & ( (\vga_control|h_cont [9] & (\vga_control|h_cont [5] & \vga_control|h_cont[8]~DUPLICATE_q )) ) ) )

	.dataa(!\vga_control|h_cont [9]),
	.datab(gnd),
	.datac(!\vga_control|h_cont [5]),
	.datad(!\vga_control|h_cont[8]~DUPLICATE_q ),
	.datae(!\vga_control|h_cont[6]~DUPLICATE_q ),
	.dataf(!\vga_control|h_cont [7]),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(\vga_control|LessThan7~0_combout ),
	.sumout(),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \vga_control|LessThan7~0 .extended_lut = "off";
defparam \vga_control|LessThan7~0 .lut_mask = 64'h0005005500550055;
defparam \vga_control|LessThan7~0 .shared_arith = "off";
// synopsys translate_on

// Location: LABCELL_X30_Y77_N3
cyclonev_lcell_comb \vga_control|LessThan7~1 (
// Equation(s):
// \vga_control|LessThan7~1_combout  = ( \vga_control|h_cont [12] & ( \vga_control|LessThan7~0_combout  ) ) # ( !\vga_control|h_cont [12] & ( \vga_control|LessThan7~0_combout  ) ) # ( \vga_control|h_cont [12] & ( !\vga_control|LessThan7~0_combout  ) ) # ( 
// !\vga_control|h_cont [12] & ( !\vga_control|LessThan7~0_combout  & ( (\vga_control|h_cont [11]) # (\vga_control|h_cont [10]) ) ) )

	.dataa(!\vga_control|h_cont [10]),
	.datab(gnd),
	.datac(gnd),
	.datad(!\vga_control|h_cont [11]),
	.datae(!\vga_control|h_cont [12]),
	.dataf(!\vga_control|LessThan7~0_combout ),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(\vga_control|LessThan7~1_combout ),
	.sumout(),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \vga_control|LessThan7~1 .extended_lut = "off";
defparam \vga_control|LessThan7~1 .lut_mask = 64'h55FFFFFFFFFFFFFF;
defparam \vga_control|LessThan7~1 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X31_Y77_N1
dffeas \vga_control|h_cont[0] (
	.clk(rClk[0]),
	.d(\vga_control|Add3~37_sumout ),
	.asdata(vcc),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(\vga_control|LessThan7~1_combout ),
	.sload(gnd),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|h_cont [0]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|h_cont[0] .is_wysiwyg = "true";
defparam \vga_control|h_cont[0] .power_up = "low";
// synopsys translate_on

// Location: LABCELL_X31_Y77_N3
cyclonev_lcell_comb \vga_control|Add3~41 (
// Equation(s):
// \vga_control|Add3~41_sumout  = SUM(( \vga_control|h_cont [1] ) + ( GND ) + ( \vga_control|Add3~38  ))
// \vga_control|Add3~42  = CARRY(( \vga_control|h_cont [1] ) + ( GND ) + ( \vga_control|Add3~38  ))

	.dataa(gnd),
	.datab(gnd),
	.datac(gnd),
	.datad(!\vga_control|h_cont [1]),
	.datae(gnd),
	.dataf(gnd),
	.datag(gnd),
	.cin(\vga_control|Add3~38 ),
	.sharein(gnd),
	.combout(),
	.sumout(\vga_control|Add3~41_sumout ),
	.cout(\vga_control|Add3~42 ),
	.shareout());
// synopsys translate_off
defparam \vga_control|Add3~41 .extended_lut = "off";
defparam \vga_control|Add3~41 .lut_mask = 64'h0000FFFF000000FF;
defparam \vga_control|Add3~41 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X31_Y77_N5
dffeas \vga_control|h_cont[1] (
	.clk(rClk[0]),
	.d(\vga_control|Add3~41_sumout ),
	.asdata(vcc),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(\vga_control|LessThan7~1_combout ),
	.sload(gnd),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|h_cont [1]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|h_cont[1] .is_wysiwyg = "true";
defparam \vga_control|h_cont[1] .power_up = "low";
// synopsys translate_on

// Location: LABCELL_X31_Y77_N6
cyclonev_lcell_comb \vga_control|Add3~49 (
// Equation(s):
// \vga_control|Add3~49_sumout  = SUM(( \vga_control|h_cont[2]~DUPLICATE_q  ) + ( GND ) + ( \vga_control|Add3~42  ))
// \vga_control|Add3~50  = CARRY(( \vga_control|h_cont[2]~DUPLICATE_q  ) + ( GND ) + ( \vga_control|Add3~42  ))

	.dataa(!\vga_control|h_cont[2]~DUPLICATE_q ),
	.datab(gnd),
	.datac(gnd),
	.datad(gnd),
	.datae(gnd),
	.dataf(gnd),
	.datag(gnd),
	.cin(\vga_control|Add3~42 ),
	.sharein(gnd),
	.combout(),
	.sumout(\vga_control|Add3~49_sumout ),
	.cout(\vga_control|Add3~50 ),
	.shareout());
// synopsys translate_off
defparam \vga_control|Add3~49 .extended_lut = "off";
defparam \vga_control|Add3~49 .lut_mask = 64'h0000FFFF00005555;
defparam \vga_control|Add3~49 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X31_Y77_N7
dffeas \vga_control|h_cont[2]~DUPLICATE (
	.clk(rClk[0]),
	.d(\vga_control|Add3~49_sumout ),
	.asdata(vcc),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(\vga_control|LessThan7~1_combout ),
	.sload(gnd),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|h_cont[2]~DUPLICATE_q ),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|h_cont[2]~DUPLICATE .is_wysiwyg = "true";
defparam \vga_control|h_cont[2]~DUPLICATE .power_up = "low";
// synopsys translate_on

// Location: LABCELL_X31_Y77_N9
cyclonev_lcell_comb \vga_control|Add3~45 (
// Equation(s):
// \vga_control|Add3~45_sumout  = SUM(( \vga_control|h_cont [3] ) + ( GND ) + ( \vga_control|Add3~50  ))
// \vga_control|Add3~46  = CARRY(( \vga_control|h_cont [3] ) + ( GND ) + ( \vga_control|Add3~50  ))

	.dataa(gnd),
	.datab(gnd),
	.datac(!\vga_control|h_cont [3]),
	.datad(gnd),
	.datae(gnd),
	.dataf(gnd),
	.datag(gnd),
	.cin(\vga_control|Add3~50 ),
	.sharein(gnd),
	.combout(),
	.sumout(\vga_control|Add3~45_sumout ),
	.cout(\vga_control|Add3~46 ),
	.shareout());
// synopsys translate_off
defparam \vga_control|Add3~45 .extended_lut = "off";
defparam \vga_control|Add3~45 .lut_mask = 64'h0000FFFF00000F0F;
defparam \vga_control|Add3~45 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X31_Y77_N10
dffeas \vga_control|h_cont[3] (
	.clk(rClk[0]),
	.d(\vga_control|Add3~45_sumout ),
	.asdata(vcc),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(\vga_control|LessThan7~1_combout ),
	.sload(gnd),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|h_cont [3]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|h_cont[3] .is_wysiwyg = "true";
defparam \vga_control|h_cont[3] .power_up = "low";
// synopsys translate_on

// Location: LABCELL_X31_Y77_N12
cyclonev_lcell_comb \vga_control|Add3~5 (
// Equation(s):
// \vga_control|Add3~5_sumout  = SUM(( \vga_control|h_cont[4]~DUPLICATE_q  ) + ( GND ) + ( \vga_control|Add3~46  ))
// \vga_control|Add3~6  = CARRY(( \vga_control|h_cont[4]~DUPLICATE_q  ) + ( GND ) + ( \vga_control|Add3~46  ))

	.dataa(gnd),
	.datab(gnd),
	.datac(gnd),
	.datad(!\vga_control|h_cont[4]~DUPLICATE_q ),
	.datae(gnd),
	.dataf(gnd),
	.datag(gnd),
	.cin(\vga_control|Add3~46 ),
	.sharein(gnd),
	.combout(),
	.sumout(\vga_control|Add3~5_sumout ),
	.cout(\vga_control|Add3~6 ),
	.shareout());
// synopsys translate_off
defparam \vga_control|Add3~5 .extended_lut = "off";
defparam \vga_control|Add3~5 .lut_mask = 64'h0000FFFF000000FF;
defparam \vga_control|Add3~5 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X31_Y77_N14
dffeas \vga_control|h_cont[4]~DUPLICATE (
	.clk(rClk[0]),
	.d(\vga_control|Add3~5_sumout ),
	.asdata(vcc),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(\vga_control|LessThan7~1_combout ),
	.sload(gnd),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|h_cont[4]~DUPLICATE_q ),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|h_cont[4]~DUPLICATE .is_wysiwyg = "true";
defparam \vga_control|h_cont[4]~DUPLICATE .power_up = "low";
// synopsys translate_on

// Location: LABCELL_X31_Y77_N15
cyclonev_lcell_comb \vga_control|Add3~13 (
// Equation(s):
// \vga_control|Add3~13_sumout  = SUM(( \vga_control|h_cont [5] ) + ( GND ) + ( \vga_control|Add3~6  ))
// \vga_control|Add3~14  = CARRY(( \vga_control|h_cont [5] ) + ( GND ) + ( \vga_control|Add3~6  ))

	.dataa(gnd),
	.datab(gnd),
	.datac(!\vga_control|h_cont [5]),
	.datad(gnd),
	.datae(gnd),
	.dataf(gnd),
	.datag(gnd),
	.cin(\vga_control|Add3~6 ),
	.sharein(gnd),
	.combout(),
	.sumout(\vga_control|Add3~13_sumout ),
	.cout(\vga_control|Add3~14 ),
	.shareout());
// synopsys translate_off
defparam \vga_control|Add3~13 .extended_lut = "off";
defparam \vga_control|Add3~13 .lut_mask = 64'h0000FFFF00000F0F;
defparam \vga_control|Add3~13 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X31_Y77_N17
dffeas \vga_control|h_cont[5] (
	.clk(rClk[0]),
	.d(\vga_control|Add3~13_sumout ),
	.asdata(vcc),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(\vga_control|LessThan7~1_combout ),
	.sload(gnd),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|h_cont [5]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|h_cont[5] .is_wysiwyg = "true";
defparam \vga_control|h_cont[5] .power_up = "low";
// synopsys translate_on

// Location: LABCELL_X31_Y77_N18
cyclonev_lcell_comb \vga_control|Add3~9 (
// Equation(s):
// \vga_control|Add3~9_sumout  = SUM(( \vga_control|h_cont[6]~DUPLICATE_q  ) + ( GND ) + ( \vga_control|Add3~14  ))
// \vga_control|Add3~10  = CARRY(( \vga_control|h_cont[6]~DUPLICATE_q  ) + ( GND ) + ( \vga_control|Add3~14  ))

	.dataa(gnd),
	.datab(gnd),
	.datac(gnd),
	.datad(!\vga_control|h_cont[6]~DUPLICATE_q ),
	.datae(gnd),
	.dataf(gnd),
	.datag(gnd),
	.cin(\vga_control|Add3~14 ),
	.sharein(gnd),
	.combout(),
	.sumout(\vga_control|Add3~9_sumout ),
	.cout(\vga_control|Add3~10 ),
	.shareout());
// synopsys translate_off
defparam \vga_control|Add3~9 .extended_lut = "off";
defparam \vga_control|Add3~9 .lut_mask = 64'h0000FFFF000000FF;
defparam \vga_control|Add3~9 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X31_Y77_N20
dffeas \vga_control|h_cont[6]~DUPLICATE (
	.clk(rClk[0]),
	.d(\vga_control|Add3~9_sumout ),
	.asdata(vcc),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(\vga_control|LessThan7~1_combout ),
	.sload(gnd),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|h_cont[6]~DUPLICATE_q ),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|h_cont[6]~DUPLICATE .is_wysiwyg = "true";
defparam \vga_control|h_cont[6]~DUPLICATE .power_up = "low";
// synopsys translate_on

// Location: LABCELL_X31_Y77_N21
cyclonev_lcell_comb \vga_control|Add3~1 (
// Equation(s):
// \vga_control|Add3~1_sumout  = SUM(( \vga_control|h_cont [7] ) + ( GND ) + ( \vga_control|Add3~10  ))
// \vga_control|Add3~2  = CARRY(( \vga_control|h_cont [7] ) + ( GND ) + ( \vga_control|Add3~10  ))

	.dataa(gnd),
	.datab(gnd),
	.datac(!\vga_control|h_cont [7]),
	.datad(gnd),
	.datae(gnd),
	.dataf(gnd),
	.datag(gnd),
	.cin(\vga_control|Add3~10 ),
	.sharein(gnd),
	.combout(),
	.sumout(\vga_control|Add3~1_sumout ),
	.cout(\vga_control|Add3~2 ),
	.shareout());
// synopsys translate_off
defparam \vga_control|Add3~1 .extended_lut = "off";
defparam \vga_control|Add3~1 .lut_mask = 64'h0000FFFF00000F0F;
defparam \vga_control|Add3~1 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X31_Y77_N22
dffeas \vga_control|h_cont[7] (
	.clk(rClk[0]),
	.d(\vga_control|Add3~1_sumout ),
	.asdata(vcc),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(\vga_control|LessThan7~1_combout ),
	.sload(gnd),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|h_cont [7]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|h_cont[7] .is_wysiwyg = "true";
defparam \vga_control|h_cont[7] .power_up = "low";
// synopsys translate_on

// Location: LABCELL_X31_Y77_N24
cyclonev_lcell_comb \vga_control|Add3~21 (
// Equation(s):
// \vga_control|Add3~21_sumout  = SUM(( \vga_control|h_cont [8] ) + ( GND ) + ( \vga_control|Add3~2  ))
// \vga_control|Add3~22  = CARRY(( \vga_control|h_cont [8] ) + ( GND ) + ( \vga_control|Add3~2  ))

	.dataa(gnd),
	.datab(!\vga_control|h_cont [8]),
	.datac(gnd),
	.datad(gnd),
	.datae(gnd),
	.dataf(gnd),
	.datag(gnd),
	.cin(\vga_control|Add3~2 ),
	.sharein(gnd),
	.combout(),
	.sumout(\vga_control|Add3~21_sumout ),
	.cout(\vga_control|Add3~22 ),
	.shareout());
// synopsys translate_off
defparam \vga_control|Add3~21 .extended_lut = "off";
defparam \vga_control|Add3~21 .lut_mask = 64'h0000FFFF00003333;
defparam \vga_control|Add3~21 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X31_Y77_N25
dffeas \vga_control|h_cont[8] (
	.clk(rClk[0]),
	.d(\vga_control|Add3~21_sumout ),
	.asdata(vcc),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(\vga_control|LessThan7~1_combout ),
	.sload(gnd),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|h_cont [8]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|h_cont[8] .is_wysiwyg = "true";
defparam \vga_control|h_cont[8] .power_up = "low";
// synopsys translate_on

// Location: FF_X31_Y77_N29
dffeas \vga_control|h_cont[9] (
	.clk(rClk[0]),
	.d(\vga_control|Add3~17_sumout ),
	.asdata(vcc),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(\vga_control|LessThan7~1_combout ),
	.sload(gnd),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|h_cont [9]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|h_cont[9] .is_wysiwyg = "true";
defparam \vga_control|h_cont[9] .power_up = "low";
// synopsys translate_on

// Location: LABCELL_X30_Y77_N54
cyclonev_lcell_comb \vga_control|Equal0~0 (
// Equation(s):
// \vga_control|Equal0~0_combout  = ( !\vga_control|h_cont [7] & ( !\vga_control|h_cont [11] & ( (!\vga_control|h_cont [9] & (!\vga_control|h_cont [12] & (!\vga_control|h_cont [10] & !\vga_control|h_cont[8]~DUPLICATE_q ))) ) ) )

	.dataa(!\vga_control|h_cont [9]),
	.datab(!\vga_control|h_cont [12]),
	.datac(!\vga_control|h_cont [10]),
	.datad(!\vga_control|h_cont[8]~DUPLICATE_q ),
	.datae(!\vga_control|h_cont [7]),
	.dataf(!\vga_control|h_cont [11]),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(\vga_control|Equal0~0_combout ),
	.sumout(),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \vga_control|Equal0~0 .extended_lut = "off";
defparam \vga_control|Equal0~0 .lut_mask = 64'h8000000000000000;
defparam \vga_control|Equal0~0 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X31_Y77_N19
dffeas \vga_control|h_cont[6] (
	.clk(rClk[0]),
	.d(\vga_control|Add3~9_sumout ),
	.asdata(vcc),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(\vga_control|LessThan7~1_combout ),
	.sload(gnd),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|h_cont [6]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|h_cont[6] .is_wysiwyg = "true";
defparam \vga_control|h_cont[6] .power_up = "low";
// synopsys translate_on

// Location: LABCELL_X30_Y77_N48
cyclonev_lcell_comb \vga_control|LessThan8~0 (
// Equation(s):
// \vga_control|LessThan8~0_combout  = ( \vga_control|h_cont [6] & ( (!\vga_control|Equal0~0_combout ) # (\vga_control|h_cont [5]) ) ) # ( !\vga_control|h_cont [6] & ( !\vga_control|Equal0~0_combout  ) )

	.dataa(gnd),
	.datab(!\vga_control|Equal0~0_combout ),
	.datac(!\vga_control|h_cont [5]),
	.datad(gnd),
	.datae(gnd),
	.dataf(!\vga_control|h_cont [6]),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(\vga_control|LessThan8~0_combout ),
	.sumout(),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \vga_control|LessThan8~0 .extended_lut = "off";
defparam \vga_control|LessThan8~0 .lut_mask = 64'hCCCCCCCCCFCFCFCF;
defparam \vga_control|LessThan8~0 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X30_Y77_N50
dffeas \vga_control|mVGA_H_SYNC (
	.clk(rClk[0]),
	.d(\vga_control|LessThan8~0_combout ),
	.asdata(vcc),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(gnd),
	.sload(gnd),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|mVGA_H_SYNC~q ),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|mVGA_H_SYNC .is_wysiwyg = "true";
defparam \vga_control|mVGA_H_SYNC .power_up = "low";
// synopsys translate_on

// Location: FF_X31_Y77_N53
dffeas \vga_control|ovga_h_sync (
	.clk(rClk[0]),
	.d(gnd),
	.asdata(\vga_control|mVGA_H_SYNC~q ),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(gnd),
	.sload(vcc),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|ovga_h_sync~q ),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|ovga_h_sync .is_wysiwyg = "true";
defparam \vga_control|ovga_h_sync .power_up = "low";
// synopsys translate_on

// Location: LABCELL_X30_Y78_N0
cyclonev_lcell_comb \vga_control|Add4~5 (
// Equation(s):
// \vga_control|Add4~5_sumout  = SUM(( \vga_control|V_Cont [0] ) + ( VCC ) + ( !VCC ))
// \vga_control|Add4~6  = CARRY(( \vga_control|V_Cont [0] ) + ( VCC ) + ( !VCC ))

	.dataa(!\vga_control|V_Cont [0]),
	.datab(gnd),
	.datac(gnd),
	.datad(gnd),
	.datae(gnd),
	.dataf(gnd),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(),
	.sumout(\vga_control|Add4~5_sumout ),
	.cout(\vga_control|Add4~6 ),
	.shareout());
// synopsys translate_off
defparam \vga_control|Add4~5 .extended_lut = "off";
defparam \vga_control|Add4~5 .lut_mask = 64'h0000000000005555;
defparam \vga_control|Add4~5 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X31_Y77_N8
dffeas \vga_control|h_cont[2] (
	.clk(rClk[0]),
	.d(\vga_control|Add3~49_sumout ),
	.asdata(vcc),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(\vga_control|LessThan7~1_combout ),
	.sload(gnd),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|h_cont [2]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|h_cont[2] .is_wysiwyg = "true";
defparam \vga_control|h_cont[2] .power_up = "low";
// synopsys translate_on

// Location: LABCELL_X30_Y77_N51
cyclonev_lcell_comb \vga_control|Equal0~1 (
// Equation(s):
// \vga_control|Equal0~1_combout  = ( !\vga_control|h_cont [0] & ( (!\vga_control|h_cont [2] & (!\vga_control|h_cont [3] & !\vga_control|h_cont [1])) ) )

	.dataa(!\vga_control|h_cont [2]),
	.datab(gnd),
	.datac(!\vga_control|h_cont [3]),
	.datad(!\vga_control|h_cont [1]),
	.datae(gnd),
	.dataf(!\vga_control|h_cont [0]),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(\vga_control|Equal0~1_combout ),
	.sumout(),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \vga_control|Equal0~1 .extended_lut = "off";
defparam \vga_control|Equal0~1 .lut_mask = 64'hA000A00000000000;
defparam \vga_control|Equal0~1 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X31_Y77_N13
dffeas \vga_control|h_cont[4] (
	.clk(rClk[0]),
	.d(\vga_control|Add3~5_sumout ),
	.asdata(vcc),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(\vga_control|LessThan7~1_combout ),
	.sload(gnd),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|h_cont [4]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|h_cont[4] .is_wysiwyg = "true";
defparam \vga_control|h_cont[4] .power_up = "low";
// synopsys translate_on

// Location: LABCELL_X30_Y77_N36
cyclonev_lcell_comb \vga_control|Equal0~2 (
// Equation(s):
// \vga_control|Equal0~2_combout  = ( \vga_control|Equal0~0_combout  & ( !\vga_control|h_cont [4] & ( (!\vga_control|h_cont [5] & (\vga_control|Equal0~1_combout  & !\vga_control|h_cont[6]~DUPLICATE_q )) ) ) )

	.dataa(!\vga_control|h_cont [5]),
	.datab(gnd),
	.datac(!\vga_control|Equal0~1_combout ),
	.datad(!\vga_control|h_cont[6]~DUPLICATE_q ),
	.datae(!\vga_control|Equal0~0_combout ),
	.dataf(!\vga_control|h_cont [4]),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(\vga_control|Equal0~2_combout ),
	.sumout(),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \vga_control|Equal0~2 .extended_lut = "off";
defparam \vga_control|Equal0~2 .lut_mask = 64'h00000A0000000000;
defparam \vga_control|Equal0~2 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X30_Y78_N1
dffeas \vga_control|V_Cont[0] (
	.clk(rClk[0]),
	.d(\vga_control|Add4~5_sumout ),
	.asdata(vcc),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(\vga_control|LessThan9~1_combout ),
	.sload(gnd),
	.ena(\vga_control|Equal0~2_combout ),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|V_Cont [0]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|V_Cont[0] .is_wysiwyg = "true";
defparam \vga_control|V_Cont[0] .power_up = "low";
// synopsys translate_on

// Location: LABCELL_X30_Y78_N3
cyclonev_lcell_comb \vga_control|Add4~1 (
// Equation(s):
// \vga_control|Add4~1_sumout  = SUM(( \vga_control|V_Cont[1]~DUPLICATE_q  ) + ( GND ) + ( \vga_control|Add4~6  ))
// \vga_control|Add4~2  = CARRY(( \vga_control|V_Cont[1]~DUPLICATE_q  ) + ( GND ) + ( \vga_control|Add4~6  ))

	.dataa(gnd),
	.datab(gnd),
	.datac(gnd),
	.datad(!\vga_control|V_Cont[1]~DUPLICATE_q ),
	.datae(gnd),
	.dataf(gnd),
	.datag(gnd),
	.cin(\vga_control|Add4~6 ),
	.sharein(gnd),
	.combout(),
	.sumout(\vga_control|Add4~1_sumout ),
	.cout(\vga_control|Add4~2 ),
	.shareout());
// synopsys translate_off
defparam \vga_control|Add4~1 .extended_lut = "off";
defparam \vga_control|Add4~1 .lut_mask = 64'h0000FFFF000000FF;
defparam \vga_control|Add4~1 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X30_Y78_N4
dffeas \vga_control|V_Cont[1]~DUPLICATE (
	.clk(rClk[0]),
	.d(\vga_control|Add4~1_sumout ),
	.asdata(vcc),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(\vga_control|LessThan9~1_combout ),
	.sload(gnd),
	.ena(\vga_control|Equal0~2_combout ),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|V_Cont[1]~DUPLICATE_q ),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|V_Cont[1]~DUPLICATE .is_wysiwyg = "true";
defparam \vga_control|V_Cont[1]~DUPLICATE .power_up = "low";
// synopsys translate_on

// Location: LABCELL_X30_Y78_N6
cyclonev_lcell_comb \vga_control|Add4~17 (
// Equation(s):
// \vga_control|Add4~17_sumout  = SUM(( \vga_control|V_Cont[2]~DUPLICATE_q  ) + ( GND ) + ( \vga_control|Add4~2  ))
// \vga_control|Add4~18  = CARRY(( \vga_control|V_Cont[2]~DUPLICATE_q  ) + ( GND ) + ( \vga_control|Add4~2  ))

	.dataa(gnd),
	.datab(!\vga_control|V_Cont[2]~DUPLICATE_q ),
	.datac(gnd),
	.datad(gnd),
	.datae(gnd),
	.dataf(gnd),
	.datag(gnd),
	.cin(\vga_control|Add4~2 ),
	.sharein(gnd),
	.combout(),
	.sumout(\vga_control|Add4~17_sumout ),
	.cout(\vga_control|Add4~18 ),
	.shareout());
// synopsys translate_off
defparam \vga_control|Add4~17 .extended_lut = "off";
defparam \vga_control|Add4~17 .lut_mask = 64'h0000FFFF00003333;
defparam \vga_control|Add4~17 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X30_Y78_N8
dffeas \vga_control|V_Cont[2]~DUPLICATE (
	.clk(rClk[0]),
	.d(\vga_control|Add4~17_sumout ),
	.asdata(vcc),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(\vga_control|LessThan9~1_combout ),
	.sload(gnd),
	.ena(\vga_control|Equal0~2_combout ),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|V_Cont[2]~DUPLICATE_q ),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|V_Cont[2]~DUPLICATE .is_wysiwyg = "true";
defparam \vga_control|V_Cont[2]~DUPLICATE .power_up = "low";
// synopsys translate_on

// Location: LABCELL_X30_Y78_N9
cyclonev_lcell_comb \vga_control|Add4~13 (
// Equation(s):
// \vga_control|Add4~13_sumout  = SUM(( \vga_control|V_Cont [3] ) + ( GND ) + ( \vga_control|Add4~18  ))
// \vga_control|Add4~14  = CARRY(( \vga_control|V_Cont [3] ) + ( GND ) + ( \vga_control|Add4~18  ))

	.dataa(!\vga_control|V_Cont [3]),
	.datab(gnd),
	.datac(gnd),
	.datad(gnd),
	.datae(gnd),
	.dataf(gnd),
	.datag(gnd),
	.cin(\vga_control|Add4~18 ),
	.sharein(gnd),
	.combout(),
	.sumout(\vga_control|Add4~13_sumout ),
	.cout(\vga_control|Add4~14 ),
	.shareout());
// synopsys translate_off
defparam \vga_control|Add4~13 .extended_lut = "off";
defparam \vga_control|Add4~13 .lut_mask = 64'h0000FFFF00005555;
defparam \vga_control|Add4~13 .shared_arith = "off";
// synopsys translate_on

// Location: LABCELL_X30_Y78_N12
cyclonev_lcell_comb \vga_control|Add4~9 (
// Equation(s):
// \vga_control|Add4~9_sumout  = SUM(( \vga_control|V_Cont[4]~DUPLICATE_q  ) + ( GND ) + ( \vga_control|Add4~14  ))
// \vga_control|Add4~10  = CARRY(( \vga_control|V_Cont[4]~DUPLICATE_q  ) + ( GND ) + ( \vga_control|Add4~14  ))

	.dataa(gnd),
	.datab(!\vga_control|V_Cont[4]~DUPLICATE_q ),
	.datac(gnd),
	.datad(gnd),
	.datae(gnd),
	.dataf(gnd),
	.datag(gnd),
	.cin(\vga_control|Add4~14 ),
	.sharein(gnd),
	.combout(),
	.sumout(\vga_control|Add4~9_sumout ),
	.cout(\vga_control|Add4~10 ),
	.shareout());
// synopsys translate_off
defparam \vga_control|Add4~9 .extended_lut = "off";
defparam \vga_control|Add4~9 .lut_mask = 64'h0000FFFF00003333;
defparam \vga_control|Add4~9 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X30_Y78_N13
dffeas \vga_control|V_Cont[4]~DUPLICATE (
	.clk(rClk[0]),
	.d(\vga_control|Add4~9_sumout ),
	.asdata(vcc),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(\vga_control|LessThan9~1_combout ),
	.sload(gnd),
	.ena(\vga_control|Equal0~2_combout ),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|V_Cont[4]~DUPLICATE_q ),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|V_Cont[4]~DUPLICATE .is_wysiwyg = "true";
defparam \vga_control|V_Cont[4]~DUPLICATE .power_up = "low";
// synopsys translate_on

// Location: LABCELL_X30_Y78_N15
cyclonev_lcell_comb \vga_control|Add4~21 (
// Equation(s):
// \vga_control|Add4~21_sumout  = SUM(( \vga_control|V_Cont[5]~DUPLICATE_q  ) + ( GND ) + ( \vga_control|Add4~10  ))
// \vga_control|Add4~22  = CARRY(( \vga_control|V_Cont[5]~DUPLICATE_q  ) + ( GND ) + ( \vga_control|Add4~10  ))

	.dataa(gnd),
	.datab(gnd),
	.datac(!\vga_control|V_Cont[5]~DUPLICATE_q ),
	.datad(gnd),
	.datae(gnd),
	.dataf(gnd),
	.datag(gnd),
	.cin(\vga_control|Add4~10 ),
	.sharein(gnd),
	.combout(),
	.sumout(\vga_control|Add4~21_sumout ),
	.cout(\vga_control|Add4~22 ),
	.shareout());
// synopsys translate_off
defparam \vga_control|Add4~21 .extended_lut = "off";
defparam \vga_control|Add4~21 .lut_mask = 64'h0000FFFF00000F0F;
defparam \vga_control|Add4~21 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X30_Y78_N17
dffeas \vga_control|V_Cont[5]~DUPLICATE (
	.clk(rClk[0]),
	.d(\vga_control|Add4~21_sumout ),
	.asdata(vcc),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(\vga_control|LessThan9~1_combout ),
	.sload(gnd),
	.ena(\vga_control|Equal0~2_combout ),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|V_Cont[5]~DUPLICATE_q ),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|V_Cont[5]~DUPLICATE .is_wysiwyg = "true";
defparam \vga_control|V_Cont[5]~DUPLICATE .power_up = "low";
// synopsys translate_on

// Location: LABCELL_X30_Y78_N18
cyclonev_lcell_comb \vga_control|Add4~33 (
// Equation(s):
// \vga_control|Add4~33_sumout  = SUM(( \vga_control|V_Cont[6]~DUPLICATE_q  ) + ( GND ) + ( \vga_control|Add4~22  ))
// \vga_control|Add4~34  = CARRY(( \vga_control|V_Cont[6]~DUPLICATE_q  ) + ( GND ) + ( \vga_control|Add4~22  ))

	.dataa(gnd),
	.datab(!\vga_control|V_Cont[6]~DUPLICATE_q ),
	.datac(gnd),
	.datad(gnd),
	.datae(gnd),
	.dataf(gnd),
	.datag(gnd),
	.cin(\vga_control|Add4~22 ),
	.sharein(gnd),
	.combout(),
	.sumout(\vga_control|Add4~33_sumout ),
	.cout(\vga_control|Add4~34 ),
	.shareout());
// synopsys translate_off
defparam \vga_control|Add4~33 .extended_lut = "off";
defparam \vga_control|Add4~33 .lut_mask = 64'h0000FFFF00003333;
defparam \vga_control|Add4~33 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X30_Y78_N19
dffeas \vga_control|V_Cont[6]~DUPLICATE (
	.clk(rClk[0]),
	.d(\vga_control|Add4~33_sumout ),
	.asdata(vcc),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(\vga_control|LessThan9~1_combout ),
	.sload(gnd),
	.ena(\vga_control|Equal0~2_combout ),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|V_Cont[6]~DUPLICATE_q ),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|V_Cont[6]~DUPLICATE .is_wysiwyg = "true";
defparam \vga_control|V_Cont[6]~DUPLICATE .power_up = "low";
// synopsys translate_on

// Location: LABCELL_X30_Y78_N21
cyclonev_lcell_comb \vga_control|Add4~29 (
// Equation(s):
// \vga_control|Add4~29_sumout  = SUM(( \vga_control|V_Cont[7]~DUPLICATE_q  ) + ( GND ) + ( \vga_control|Add4~34  ))
// \vga_control|Add4~30  = CARRY(( \vga_control|V_Cont[7]~DUPLICATE_q  ) + ( GND ) + ( \vga_control|Add4~34  ))

	.dataa(gnd),
	.datab(gnd),
	.datac(gnd),
	.datad(!\vga_control|V_Cont[7]~DUPLICATE_q ),
	.datae(gnd),
	.dataf(gnd),
	.datag(gnd),
	.cin(\vga_control|Add4~34 ),
	.sharein(gnd),
	.combout(),
	.sumout(\vga_control|Add4~29_sumout ),
	.cout(\vga_control|Add4~30 ),
	.shareout());
// synopsys translate_off
defparam \vga_control|Add4~29 .extended_lut = "off";
defparam \vga_control|Add4~29 .lut_mask = 64'h0000FFFF000000FF;
defparam \vga_control|Add4~29 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X30_Y78_N22
dffeas \vga_control|V_Cont[7]~DUPLICATE (
	.clk(rClk[0]),
	.d(\vga_control|Add4~29_sumout ),
	.asdata(vcc),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(\vga_control|LessThan9~1_combout ),
	.sload(gnd),
	.ena(\vga_control|Equal0~2_combout ),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|V_Cont[7]~DUPLICATE_q ),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|V_Cont[7]~DUPLICATE .is_wysiwyg = "true";
defparam \vga_control|V_Cont[7]~DUPLICATE .power_up = "low";
// synopsys translate_on

// Location: LABCELL_X30_Y78_N24
cyclonev_lcell_comb \vga_control|Add4~25 (
// Equation(s):
// \vga_control|Add4~25_sumout  = SUM(( \vga_control|V_Cont[8]~DUPLICATE_q  ) + ( GND ) + ( \vga_control|Add4~30  ))
// \vga_control|Add4~26  = CARRY(( \vga_control|V_Cont[8]~DUPLICATE_q  ) + ( GND ) + ( \vga_control|Add4~30  ))

	.dataa(gnd),
	.datab(!\vga_control|V_Cont[8]~DUPLICATE_q ),
	.datac(gnd),
	.datad(gnd),
	.datae(gnd),
	.dataf(gnd),
	.datag(gnd),
	.cin(\vga_control|Add4~30 ),
	.sharein(gnd),
	.combout(),
	.sumout(\vga_control|Add4~25_sumout ),
	.cout(\vga_control|Add4~26 ),
	.shareout());
// synopsys translate_off
defparam \vga_control|Add4~25 .extended_lut = "off";
defparam \vga_control|Add4~25 .lut_mask = 64'h0000FFFF00003333;
defparam \vga_control|Add4~25 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X30_Y78_N25
dffeas \vga_control|V_Cont[8]~DUPLICATE (
	.clk(rClk[0]),
	.d(\vga_control|Add4~25_sumout ),
	.asdata(vcc),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(\vga_control|LessThan9~1_combout ),
	.sload(gnd),
	.ena(\vga_control|Equal0~2_combout ),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|V_Cont[8]~DUPLICATE_q ),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|V_Cont[8]~DUPLICATE .is_wysiwyg = "true";
defparam \vga_control|V_Cont[8]~DUPLICATE .power_up = "low";
// synopsys translate_on

// Location: LABCELL_X30_Y78_N27
cyclonev_lcell_comb \vga_control|Add4~37 (
// Equation(s):
// \vga_control|Add4~37_sumout  = SUM(( \vga_control|V_Cont[9]~DUPLICATE_q  ) + ( GND ) + ( \vga_control|Add4~26  ))
// \vga_control|Add4~38  = CARRY(( \vga_control|V_Cont[9]~DUPLICATE_q  ) + ( GND ) + ( \vga_control|Add4~26  ))

	.dataa(!\vga_control|V_Cont[9]~DUPLICATE_q ),
	.datab(gnd),
	.datac(gnd),
	.datad(gnd),
	.datae(gnd),
	.dataf(gnd),
	.datag(gnd),
	.cin(\vga_control|Add4~26 ),
	.sharein(gnd),
	.combout(),
	.sumout(\vga_control|Add4~37_sumout ),
	.cout(\vga_control|Add4~38 ),
	.shareout());
// synopsys translate_off
defparam \vga_control|Add4~37 .extended_lut = "off";
defparam \vga_control|Add4~37 .lut_mask = 64'h0000FFFF00005555;
defparam \vga_control|Add4~37 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X30_Y78_N29
dffeas \vga_control|V_Cont[9]~DUPLICATE (
	.clk(rClk[0]),
	.d(\vga_control|Add4~37_sumout ),
	.asdata(vcc),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(\vga_control|LessThan9~1_combout ),
	.sload(gnd),
	.ena(\vga_control|Equal0~2_combout ),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|V_Cont[9]~DUPLICATE_q ),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|V_Cont[9]~DUPLICATE .is_wysiwyg = "true";
defparam \vga_control|V_Cont[9]~DUPLICATE .power_up = "low";
// synopsys translate_on

// Location: LABCELL_X30_Y78_N30
cyclonev_lcell_comb \vga_control|Add4~49 (
// Equation(s):
// \vga_control|Add4~49_sumout  = SUM(( \vga_control|V_Cont[10]~DUPLICATE_q  ) + ( GND ) + ( \vga_control|Add4~38  ))
// \vga_control|Add4~50  = CARRY(( \vga_control|V_Cont[10]~DUPLICATE_q  ) + ( GND ) + ( \vga_control|Add4~38  ))

	.dataa(gnd),
	.datab(!\vga_control|V_Cont[10]~DUPLICATE_q ),
	.datac(gnd),
	.datad(gnd),
	.datae(gnd),
	.dataf(gnd),
	.datag(gnd),
	.cin(\vga_control|Add4~38 ),
	.sharein(gnd),
	.combout(),
	.sumout(\vga_control|Add4~49_sumout ),
	.cout(\vga_control|Add4~50 ),
	.shareout());
// synopsys translate_off
defparam \vga_control|Add4~49 .extended_lut = "off";
defparam \vga_control|Add4~49 .lut_mask = 64'h0000FFFF00003333;
defparam \vga_control|Add4~49 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X30_Y78_N32
dffeas \vga_control|V_Cont[10]~DUPLICATE (
	.clk(rClk[0]),
	.d(\vga_control|Add4~49_sumout ),
	.asdata(vcc),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(\vga_control|LessThan9~1_combout ),
	.sload(gnd),
	.ena(\vga_control|Equal0~2_combout ),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|V_Cont[10]~DUPLICATE_q ),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|V_Cont[10]~DUPLICATE .is_wysiwyg = "true";
defparam \vga_control|V_Cont[10]~DUPLICATE .power_up = "low";
// synopsys translate_on

// Location: LABCELL_X30_Y78_N33
cyclonev_lcell_comb \vga_control|Add4~45 (
// Equation(s):
// \vga_control|Add4~45_sumout  = SUM(( \vga_control|V_Cont[11]~DUPLICATE_q  ) + ( GND ) + ( \vga_control|Add4~50  ))
// \vga_control|Add4~46  = CARRY(( \vga_control|V_Cont[11]~DUPLICATE_q  ) + ( GND ) + ( \vga_control|Add4~50  ))

	.dataa(!\vga_control|V_Cont[11]~DUPLICATE_q ),
	.datab(gnd),
	.datac(gnd),
	.datad(gnd),
	.datae(gnd),
	.dataf(gnd),
	.datag(gnd),
	.cin(\vga_control|Add4~50 ),
	.sharein(gnd),
	.combout(),
	.sumout(\vga_control|Add4~45_sumout ),
	.cout(\vga_control|Add4~46 ),
	.shareout());
// synopsys translate_off
defparam \vga_control|Add4~45 .extended_lut = "off";
defparam \vga_control|Add4~45 .lut_mask = 64'h0000FFFF00005555;
defparam \vga_control|Add4~45 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X30_Y78_N35
dffeas \vga_control|V_Cont[11]~DUPLICATE (
	.clk(rClk[0]),
	.d(\vga_control|Add4~45_sumout ),
	.asdata(vcc),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(\vga_control|LessThan9~1_combout ),
	.sload(gnd),
	.ena(\vga_control|Equal0~2_combout ),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|V_Cont[11]~DUPLICATE_q ),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|V_Cont[11]~DUPLICATE .is_wysiwyg = "true";
defparam \vga_control|V_Cont[11]~DUPLICATE .power_up = "low";
// synopsys translate_on

// Location: LABCELL_X30_Y78_N36
cyclonev_lcell_comb \vga_control|Add4~41 (
// Equation(s):
// \vga_control|Add4~41_sumout  = SUM(( \vga_control|V_Cont[12]~DUPLICATE_q  ) + ( GND ) + ( \vga_control|Add4~46  ))

	.dataa(gnd),
	.datab(gnd),
	.datac(!\vga_control|V_Cont[12]~DUPLICATE_q ),
	.datad(gnd),
	.datae(gnd),
	.dataf(gnd),
	.datag(gnd),
	.cin(\vga_control|Add4~46 ),
	.sharein(gnd),
	.combout(),
	.sumout(\vga_control|Add4~41_sumout ),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \vga_control|Add4~41 .extended_lut = "off";
defparam \vga_control|Add4~41 .lut_mask = 64'h0000FFFF00000F0F;
defparam \vga_control|Add4~41 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X30_Y78_N38
dffeas \vga_control|V_Cont[12]~DUPLICATE (
	.clk(rClk[0]),
	.d(\vga_control|Add4~41_sumout ),
	.asdata(vcc),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(\vga_control|LessThan9~1_combout ),
	.sload(gnd),
	.ena(\vga_control|Equal0~2_combout ),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|V_Cont[12]~DUPLICATE_q ),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|V_Cont[12]~DUPLICATE .is_wysiwyg = "true";
defparam \vga_control|V_Cont[12]~DUPLICATE .power_up = "low";
// synopsys translate_on

// Location: LABCELL_X30_Y78_N45
cyclonev_lcell_comb \vga_control|mvga_r~5 (
// Equation(s):
// \vga_control|mvga_r~5_combout  = ( !\vga_control|V_Cont[11]~DUPLICATE_q  & ( (!\vga_control|V_Cont[10]~DUPLICATE_q  & !\vga_control|V_Cont[12]~DUPLICATE_q ) ) )

	.dataa(gnd),
	.datab(gnd),
	.datac(!\vga_control|V_Cont[10]~DUPLICATE_q ),
	.datad(!\vga_control|V_Cont[12]~DUPLICATE_q ),
	.datae(gnd),
	.dataf(!\vga_control|V_Cont[11]~DUPLICATE_q ),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(\vga_control|mvga_r~5_combout ),
	.sumout(),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \vga_control|mvga_r~5 .extended_lut = "off";
defparam \vga_control|mvga_r~5 .lut_mask = 64'hF000F00000000000;
defparam \vga_control|mvga_r~5 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X30_Y78_N26
dffeas \vga_control|V_Cont[8] (
	.clk(rClk[0]),
	.d(\vga_control|Add4~25_sumout ),
	.asdata(vcc),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(\vga_control|LessThan9~1_combout ),
	.sload(gnd),
	.ena(\vga_control|Equal0~2_combout ),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|V_Cont [8]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|V_Cont[8] .is_wysiwyg = "true";
defparam \vga_control|V_Cont[8] .power_up = "low";
// synopsys translate_on

// Location: FF_X30_Y78_N20
dffeas \vga_control|V_Cont[6] (
	.clk(rClk[0]),
	.d(\vga_control|Add4~33_sumout ),
	.asdata(vcc),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(\vga_control|LessThan9~1_combout ),
	.sload(gnd),
	.ena(\vga_control|Equal0~2_combout ),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|V_Cont [6]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|V_Cont[6] .is_wysiwyg = "true";
defparam \vga_control|V_Cont[6] .power_up = "low";
// synopsys translate_on

// Location: FF_X30_Y78_N23
dffeas \vga_control|V_Cont[7] (
	.clk(rClk[0]),
	.d(\vga_control|Add4~29_sumout ),
	.asdata(vcc),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(\vga_control|LessThan9~1_combout ),
	.sload(gnd),
	.ena(\vga_control|Equal0~2_combout ),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|V_Cont [7]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|V_Cont[7] .is_wysiwyg = "true";
defparam \vga_control|V_Cont[7] .power_up = "low";
// synopsys translate_on

// Location: LABCELL_X30_Y78_N48
cyclonev_lcell_comb \vga_control|LessThan6~2 (
// Equation(s):
// \vga_control|LessThan6~2_combout  = ( !\vga_control|V_Cont[5]~DUPLICATE_q  & ( (!\vga_control|V_Cont [8] & (!\vga_control|V_Cont [6] & !\vga_control|V_Cont [7])) ) )

	.dataa(!\vga_control|V_Cont [8]),
	.datab(gnd),
	.datac(!\vga_control|V_Cont [6]),
	.datad(!\vga_control|V_Cont [7]),
	.datae(gnd),
	.dataf(!\vga_control|V_Cont[5]~DUPLICATE_q ),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(\vga_control|LessThan6~2_combout ),
	.sumout(),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \vga_control|LessThan6~2 .extended_lut = "off";
defparam \vga_control|LessThan6~2 .lut_mask = 64'hA000A00000000000;
defparam \vga_control|LessThan6~2 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X30_Y78_N7
dffeas \vga_control|V_Cont[2] (
	.clk(rClk[0]),
	.d(\vga_control|Add4~17_sumout ),
	.asdata(vcc),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(\vga_control|LessThan9~1_combout ),
	.sload(gnd),
	.ena(\vga_control|Equal0~2_combout ),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|V_Cont [2]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|V_Cont[2] .is_wysiwyg = "true";
defparam \vga_control|V_Cont[2] .power_up = "low";
// synopsys translate_on

// Location: FF_X30_Y78_N2
dffeas \vga_control|V_Cont[0]~DUPLICATE (
	.clk(rClk[0]),
	.d(\vga_control|Add4~5_sumout ),
	.asdata(vcc),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(\vga_control|LessThan9~1_combout ),
	.sload(gnd),
	.ena(\vga_control|Equal0~2_combout ),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|V_Cont[0]~DUPLICATE_q ),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|V_Cont[0]~DUPLICATE .is_wysiwyg = "true";
defparam \vga_control|V_Cont[0]~DUPLICATE .power_up = "low";
// synopsys translate_on

// Location: MLABCELL_X28_Y78_N36
cyclonev_lcell_comb \vga_control|LessThan9~0 (
// Equation(s):
// \vga_control|LessThan9~0_combout  = ( \vga_control|V_Cont[0]~DUPLICATE_q  & ( \vga_control|V_Cont[3]~DUPLICATE_q  & ( \vga_control|V_Cont [2] ) ) ) # ( !\vga_control|V_Cont[0]~DUPLICATE_q  & ( \vga_control|V_Cont[3]~DUPLICATE_q  & ( 
// (\vga_control|V_Cont[1]~DUPLICATE_q  & \vga_control|V_Cont [2]) ) ) )

	.dataa(gnd),
	.datab(gnd),
	.datac(!\vga_control|V_Cont[1]~DUPLICATE_q ),
	.datad(!\vga_control|V_Cont [2]),
	.datae(!\vga_control|V_Cont[0]~DUPLICATE_q ),
	.dataf(!\vga_control|V_Cont[3]~DUPLICATE_q ),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(\vga_control|LessThan9~0_combout ),
	.sumout(),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \vga_control|LessThan9~0 .extended_lut = "off";
defparam \vga_control|LessThan9~0 .lut_mask = 64'h00000000000F00FF;
defparam \vga_control|LessThan9~0 .shared_arith = "off";
// synopsys translate_on

// Location: LABCELL_X30_Y78_N42
cyclonev_lcell_comb \vga_control|LessThan9~1 (
// Equation(s):
// \vga_control|LessThan9~1_combout  = ( \vga_control|V_Cont[4]~DUPLICATE_q  & ( (!\vga_control|mvga_r~5_combout ) # (\vga_control|V_Cont[9]~DUPLICATE_q ) ) ) # ( !\vga_control|V_Cont[4]~DUPLICATE_q  & ( (!\vga_control|mvga_r~5_combout ) # 
// ((\vga_control|V_Cont[9]~DUPLICATE_q  & ((!\vga_control|LessThan6~2_combout ) # (\vga_control|LessThan9~0_combout )))) ) )

	.dataa(!\vga_control|V_Cont[9]~DUPLICATE_q ),
	.datab(!\vga_control|mvga_r~5_combout ),
	.datac(!\vga_control|LessThan6~2_combout ),
	.datad(!\vga_control|LessThan9~0_combout ),
	.datae(gnd),
	.dataf(!\vga_control|V_Cont[4]~DUPLICATE_q ),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(\vga_control|LessThan9~1_combout ),
	.sumout(),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \vga_control|LessThan9~1 .extended_lut = "off";
defparam \vga_control|LessThan9~1 .lut_mask = 64'hDCDDDCDDDDDDDDDD;
defparam \vga_control|LessThan9~1 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X30_Y78_N10
dffeas \vga_control|V_Cont[3] (
	.clk(rClk[0]),
	.d(\vga_control|Add4~13_sumout ),
	.asdata(vcc),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(\vga_control|LessThan9~1_combout ),
	.sload(gnd),
	.ena(\vga_control|Equal0~2_combout ),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|V_Cont [3]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|V_Cont[3] .is_wysiwyg = "true";
defparam \vga_control|V_Cont[3] .power_up = "low";
// synopsys translate_on

// Location: FF_X30_Y78_N11
dffeas \vga_control|V_Cont[3]~DUPLICATE (
	.clk(rClk[0]),
	.d(\vga_control|Add4~13_sumout ),
	.asdata(vcc),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(\vga_control|LessThan9~1_combout ),
	.sload(gnd),
	.ena(\vga_control|Equal0~2_combout ),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|V_Cont[3]~DUPLICATE_q ),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|V_Cont[3]~DUPLICATE .is_wysiwyg = "true";
defparam \vga_control|V_Cont[3]~DUPLICATE .power_up = "low";
// synopsys translate_on

// Location: FF_X31_Y77_N41
dffeas \vga_control|mVGA_V_SYNC~DUPLICATE (
	.clk(rClk[0]),
	.d(gnd),
	.asdata(\vga_control|mVGA_V_SYNC~0_combout ),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(gnd),
	.sload(vcc),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|mVGA_V_SYNC~DUPLICATE_q ),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|mVGA_V_SYNC~DUPLICATE .is_wysiwyg = "true";
defparam \vga_control|mVGA_V_SYNC~DUPLICATE .power_up = "low";
// synopsys translate_on

// Location: FF_X30_Y78_N5
dffeas \vga_control|V_Cont[1] (
	.clk(rClk[0]),
	.d(\vga_control|Add4~1_sumout ),
	.asdata(vcc),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(\vga_control|LessThan9~1_combout ),
	.sload(gnd),
	.ena(\vga_control|Equal0~2_combout ),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|V_Cont [1]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|V_Cont[1] .is_wysiwyg = "true";
defparam \vga_control|V_Cont[1] .power_up = "low";
// synopsys translate_on

// Location: FF_X30_Y78_N28
dffeas \vga_control|V_Cont[9] (
	.clk(rClk[0]),
	.d(\vga_control|Add4~37_sumout ),
	.asdata(vcc),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(\vga_control|LessThan9~1_combout ),
	.sload(gnd),
	.ena(\vga_control|Equal0~2_combout ),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|V_Cont [9]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|V_Cont[9] .is_wysiwyg = "true";
defparam \vga_control|V_Cont[9] .power_up = "low";
// synopsys translate_on

// Location: LABCELL_X30_Y78_N57
cyclonev_lcell_comb \vga_control|LessThan10~0 (
// Equation(s):
// \vga_control|LessThan10~0_combout  = ( \vga_control|LessThan6~2_combout  & ( (!\vga_control|V_Cont [1] & (!\vga_control|V_Cont [9] & \vga_control|mvga_r~5_combout )) ) )

	.dataa(!\vga_control|V_Cont [1]),
	.datab(gnd),
	.datac(!\vga_control|V_Cont [9]),
	.datad(!\vga_control|mvga_r~5_combout ),
	.datae(gnd),
	.dataf(!\vga_control|LessThan6~2_combout ),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(\vga_control|LessThan10~0_combout ),
	.sumout(),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \vga_control|LessThan10~0 .extended_lut = "off";
defparam \vga_control|LessThan10~0 .lut_mask = 64'h0000000000A000A0;
defparam \vga_control|LessThan10~0 .shared_arith = "off";
// synopsys translate_on

// Location: LABCELL_X31_Y77_N48
cyclonev_lcell_comb \vga_control|mVGA_V_SYNC~0 (
// Equation(s):
// \vga_control|mVGA_V_SYNC~0_combout  = ( \vga_control|V_Cont[4]~DUPLICATE_q  & ( \vga_control|LessThan10~0_combout  & ( (\vga_control|Equal0~2_combout ) # (\vga_control|mVGA_V_SYNC~DUPLICATE_q ) ) ) ) # ( !\vga_control|V_Cont[4]~DUPLICATE_q  & ( 
// \vga_control|LessThan10~0_combout  & ( (!\vga_control|Equal0~2_combout  & (((\vga_control|mVGA_V_SYNC~DUPLICATE_q )))) # (\vga_control|Equal0~2_combout  & (((\vga_control|V_Cont [2])) # (\vga_control|V_Cont[3]~DUPLICATE_q ))) ) ) ) # ( 
// \vga_control|V_Cont[4]~DUPLICATE_q  & ( !\vga_control|LessThan10~0_combout  & ( (\vga_control|Equal0~2_combout ) # (\vga_control|mVGA_V_SYNC~DUPLICATE_q ) ) ) ) # ( !\vga_control|V_Cont[4]~DUPLICATE_q  & ( !\vga_control|LessThan10~0_combout  & ( 
// (\vga_control|Equal0~2_combout ) # (\vga_control|mVGA_V_SYNC~DUPLICATE_q ) ) ) )

	.dataa(!\vga_control|V_Cont[3]~DUPLICATE_q ),
	.datab(!\vga_control|mVGA_V_SYNC~DUPLICATE_q ),
	.datac(!\vga_control|Equal0~2_combout ),
	.datad(!\vga_control|V_Cont [2]),
	.datae(!\vga_control|V_Cont[4]~DUPLICATE_q ),
	.dataf(!\vga_control|LessThan10~0_combout ),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(\vga_control|mVGA_V_SYNC~0_combout ),
	.sumout(),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \vga_control|mVGA_V_SYNC~0 .extended_lut = "off";
defparam \vga_control|mVGA_V_SYNC~0 .lut_mask = 64'h3F3F3F3F353F3F3F;
defparam \vga_control|mVGA_V_SYNC~0 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X31_Y77_N40
dffeas \vga_control|mVGA_V_SYNC (
	.clk(rClk[0]),
	.d(gnd),
	.asdata(\vga_control|mVGA_V_SYNC~0_combout ),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(gnd),
	.sload(vcc),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|mVGA_V_SYNC~q ),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|mVGA_V_SYNC .is_wysiwyg = "true";
defparam \vga_control|mVGA_V_SYNC .power_up = "low";
// synopsys translate_on

// Location: FF_X31_Y77_N46
dffeas \vga_control|ovga_v_sync (
	.clk(rClk[0]),
	.d(gnd),
	.asdata(\vga_control|mVGA_V_SYNC~q ),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(gnd),
	.sload(vcc),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|ovga_v_sync~q ),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|ovga_v_sync .is_wysiwyg = "true";
defparam \vga_control|ovga_v_sync .power_up = "low";
// synopsys translate_on

// Location: LABCELL_X31_Y77_N42
cyclonev_lcell_comb \vga_control|mVGA_BLANK (
// Equation(s):
// \vga_control|mVGA_BLANK~combout  = ( \vga_control|mVGA_V_SYNC~q  & ( \vga_control|mVGA_H_SYNC~q  ) )

	.dataa(!\vga_control|mVGA_H_SYNC~q ),
	.datab(gnd),
	.datac(gnd),
	.datad(gnd),
	.datae(gnd),
	.dataf(!\vga_control|mVGA_V_SYNC~q ),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(\vga_control|mVGA_BLANK~combout ),
	.sumout(),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \vga_control|mVGA_BLANK .extended_lut = "off";
defparam \vga_control|mVGA_BLANK .lut_mask = 64'h0000000055555555;
defparam \vga_control|mVGA_BLANK .shared_arith = "off";
// synopsys translate_on

// Location: FF_X31_Y77_N43
dffeas \vga_control|ovga_blank (
	.clk(rClk[0]),
	.d(\vga_control|mVGA_BLANK~combout ),
	.asdata(vcc),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(gnd),
	.sload(gnd),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|ovga_blank~q ),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|ovga_blank .is_wysiwyg = "true";
defparam \vga_control|ovga_blank .power_up = "low";
// synopsys translate_on

// Location: FF_X30_Y78_N37
dffeas \vga_control|V_Cont[12] (
	.clk(rClk[0]),
	.d(\vga_control|Add4~41_sumout ),
	.asdata(vcc),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(\vga_control|LessThan9~1_combout ),
	.sload(gnd),
	.ena(\vga_control|Equal0~2_combout ),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|V_Cont [12]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|V_Cont[12] .is_wysiwyg = "true";
defparam \vga_control|V_Cont[12] .power_up = "low";
// synopsys translate_on

// Location: FF_X30_Y78_N31
dffeas \vga_control|V_Cont[10] (
	.clk(rClk[0]),
	.d(\vga_control|Add4~49_sumout ),
	.asdata(vcc),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(\vga_control|LessThan9~1_combout ),
	.sload(gnd),
	.ena(\vga_control|Equal0~2_combout ),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|V_Cont [10]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|V_Cont[10] .is_wysiwyg = "true";
defparam \vga_control|V_Cont[10] .power_up = "low";
// synopsys translate_on

// Location: LABCELL_X30_Y77_N6
cyclonev_lcell_comb \vga_control|mvga_r~1 (
// Equation(s):
// \vga_control|mvga_r~1_combout  = ( !\vga_control|V_Cont[11]~DUPLICATE_q  & ( !\vga_control|h_cont [11] & ( (!\vga_control|V_Cont [12] & (!\vga_control|h_cont [12] & (!\vga_control|h_cont [10] & !\vga_control|V_Cont [10]))) ) ) )

	.dataa(!\vga_control|V_Cont [12]),
	.datab(!\vga_control|h_cont [12]),
	.datac(!\vga_control|h_cont [10]),
	.datad(!\vga_control|V_Cont [10]),
	.datae(!\vga_control|V_Cont[11]~DUPLICATE_q ),
	.dataf(!\vga_control|h_cont [11]),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(\vga_control|mvga_r~1_combout ),
	.sumout(),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \vga_control|mvga_r~1 .extended_lut = "off";
defparam \vga_control|mvga_r~1 .lut_mask = 64'h8000000000000000;
defparam \vga_control|mvga_r~1 .shared_arith = "off";
// synopsys translate_on

// Location: LABCELL_X30_Y77_N27
cyclonev_lcell_comb \vga_control|mvga_r~0 (
// Equation(s):
// \vga_control|mvga_r~0_combout  = ( \vga_control|h_cont[6]~DUPLICATE_q  & ( \vga_control|h_cont [4] & ( (!\vga_control|h_cont [9] & (!\vga_control|h_cont[8]~DUPLICATE_q  & !\vga_control|h_cont [7])) # (\vga_control|h_cont [9] & 
// (\vga_control|h_cont[8]~DUPLICATE_q )) ) ) ) # ( !\vga_control|h_cont[6]~DUPLICATE_q  & ( \vga_control|h_cont [4] & ( (!\vga_control|h_cont [9] & (!\vga_control|h_cont[8]~DUPLICATE_q  & !\vga_control|h_cont [7])) # (\vga_control|h_cont [9] & 
// (\vga_control|h_cont[8]~DUPLICATE_q )) ) ) ) # ( \vga_control|h_cont[6]~DUPLICATE_q  & ( !\vga_control|h_cont [4] & ( (!\vga_control|h_cont [9] & (!\vga_control|h_cont[8]~DUPLICATE_q  & !\vga_control|h_cont [7])) # (\vga_control|h_cont [9] & 
// (\vga_control|h_cont[8]~DUPLICATE_q )) ) ) ) # ( !\vga_control|h_cont[6]~DUPLICATE_q  & ( !\vga_control|h_cont [4] & ( (!\vga_control|h_cont [9] & (!\vga_control|h_cont[8]~DUPLICATE_q  & ((!\vga_control|h_cont [7]) # (!\vga_control|h_cont [5])))) # 
// (\vga_control|h_cont [9] & (\vga_control|h_cont[8]~DUPLICATE_q  & ((\vga_control|h_cont [5]) # (\vga_control|h_cont [7])))) ) ) )

	.dataa(!\vga_control|h_cont [9]),
	.datab(!\vga_control|h_cont[8]~DUPLICATE_q ),
	.datac(!\vga_control|h_cont [7]),
	.datad(!\vga_control|h_cont [5]),
	.datae(!\vga_control|h_cont[6]~DUPLICATE_q ),
	.dataf(!\vga_control|h_cont [4]),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(\vga_control|mvga_r~0_combout ),
	.sumout(),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \vga_control|mvga_r~0 .extended_lut = "off";
defparam \vga_control|mvga_r~0 .lut_mask = 64'h8991919191919191;
defparam \vga_control|mvga_r~0 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X30_Y78_N16
dffeas \vga_control|V_Cont[5] (
	.clk(rClk[0]),
	.d(\vga_control|Add4~21_sumout ),
	.asdata(vcc),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(\vga_control|LessThan9~1_combout ),
	.sload(gnd),
	.ena(\vga_control|Equal0~2_combout ),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|V_Cont [5]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|V_Cont[5] .is_wysiwyg = "true";
defparam \vga_control|V_Cont[5] .power_up = "low";
// synopsys translate_on

// Location: LABCELL_X30_Y78_N51
cyclonev_lcell_comb \vga_control|LessThan6~1 (
// Equation(s):
// \vga_control|LessThan6~1_combout  = ( !\vga_control|V_Cont [6] & ( (!\vga_control|V_Cont [8] & !\vga_control|V_Cont [7]) ) )

	.dataa(!\vga_control|V_Cont [8]),
	.datab(gnd),
	.datac(gnd),
	.datad(!\vga_control|V_Cont [7]),
	.datae(gnd),
	.dataf(!\vga_control|V_Cont [6]),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(\vga_control|LessThan6~1_combout ),
	.sumout(),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \vga_control|LessThan6~1 .extended_lut = "off";
defparam \vga_control|LessThan6~1 .lut_mask = 64'hAA00AA0000000000;
defparam \vga_control|LessThan6~1 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X30_Y78_N14
dffeas \vga_control|V_Cont[4] (
	.clk(rClk[0]),
	.d(\vga_control|Add4~9_sumout ),
	.asdata(vcc),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(\vga_control|LessThan9~1_combout ),
	.sload(gnd),
	.ena(\vga_control|Equal0~2_combout ),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|V_Cont [4]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|V_Cont[4] .is_wysiwyg = "true";
defparam \vga_control|V_Cont[4] .power_up = "low";
// synopsys translate_on

// Location: LABCELL_X30_Y78_N54
cyclonev_lcell_comb \vga_control|LessThan6~0 (
// Equation(s):
// \vga_control|LessThan6~0_combout  = ( !\vga_control|V_Cont [4] & ( (!\vga_control|V_Cont[2]~DUPLICATE_q  & (!\vga_control|V_Cont [3] & ((!\vga_control|V_Cont [1]) # (!\vga_control|V_Cont[0]~DUPLICATE_q )))) ) )

	.dataa(!\vga_control|V_Cont [1]),
	.datab(!\vga_control|V_Cont[2]~DUPLICATE_q ),
	.datac(!\vga_control|V_Cont[0]~DUPLICATE_q ),
	.datad(!\vga_control|V_Cont [3]),
	.datae(gnd),
	.dataf(!\vga_control|V_Cont [4]),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(\vga_control|LessThan6~0_combout ),
	.sumout(),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \vga_control|LessThan6~0 .extended_lut = "off";
defparam \vga_control|LessThan6~0 .lut_mask = 64'hC800C80000000000;
defparam \vga_control|LessThan6~0 .shared_arith = "off";
// synopsys translate_on

// Location: LABCELL_X29_Y77_N18
cyclonev_lcell_comb \vga_control|mvga_r~2 (
// Equation(s):
// \vga_control|mvga_r~2_combout  = ( \vga_control|LessThan6~1_combout  & ( \vga_control|LessThan6~0_combout  & ( (\vga_control|mvga_r~1_combout  & (\vga_control|V_Cont[9]~DUPLICATE_q  & (!\vga_control|mvga_r~0_combout  & !\vga_control|V_Cont [5]))) ) ) ) # 
// ( !\vga_control|LessThan6~1_combout  & ( \vga_control|LessThan6~0_combout  & ( (\vga_control|mvga_r~1_combout  & (!\vga_control|V_Cont[9]~DUPLICATE_q  & !\vga_control|mvga_r~0_combout )) ) ) ) # ( \vga_control|LessThan6~1_combout  & ( 
// !\vga_control|LessThan6~0_combout  & ( (\vga_control|mvga_r~1_combout  & (!\vga_control|V_Cont[9]~DUPLICATE_q  & (!\vga_control|mvga_r~0_combout  & \vga_control|V_Cont [5]))) ) ) ) # ( !\vga_control|LessThan6~1_combout  & ( 
// !\vga_control|LessThan6~0_combout  & ( (\vga_control|mvga_r~1_combout  & (!\vga_control|V_Cont[9]~DUPLICATE_q  & !\vga_control|mvga_r~0_combout )) ) ) )

	.dataa(!\vga_control|mvga_r~1_combout ),
	.datab(!\vga_control|V_Cont[9]~DUPLICATE_q ),
	.datac(!\vga_control|mvga_r~0_combout ),
	.datad(!\vga_control|V_Cont [5]),
	.datae(!\vga_control|LessThan6~1_combout ),
	.dataf(!\vga_control|LessThan6~0_combout ),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(\vga_control|mvga_r~2_combout ),
	.sumout(),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \vga_control|mvga_r~2 .extended_lut = "off";
defparam \vga_control|mvga_r~2 .lut_mask = 64'h4040004040401000;
defparam \vga_control|mvga_r~2 .shared_arith = "off";
// synopsys translate_on

// Location: CLKCTRL_G6
cyclonev_clkena \CLOCK_50~inputCLKENA0 (
	.inclk(\CLOCK_50~input_o ),
	.ena(vcc),
	.outclk(\CLOCK_50~inputCLKENA0_outclk ),
	.enaout());
// synopsys translate_off
defparam \CLOCK_50~inputCLKENA0 .clock_type = "global clock";
defparam \CLOCK_50~inputCLKENA0 .disable_mode = "low";
defparam \CLOCK_50~inputCLKENA0 .ena_register_mode = "always enabled";
defparam \CLOCK_50~inputCLKENA0 .ena_register_power_up = "high";
defparam \CLOCK_50~inputCLKENA0 .test_syn = "high";
// synopsys translate_on

// Location: MLABCELL_X28_Y77_N0
cyclonev_lcell_comb \vga_control|Add2~25 (
// Equation(s):
// \vga_control|Add2~25_sumout  = SUM(( \vga_control|V_Cont[0]~DUPLICATE_q  ) + ( \vga_control|V_Cont [1] ) + ( !VCC ))
// \vga_control|Add2~26  = CARRY(( \vga_control|V_Cont[0]~DUPLICATE_q  ) + ( \vga_control|V_Cont [1] ) + ( !VCC ))

	.dataa(gnd),
	.datab(!\vga_control|V_Cont[0]~DUPLICATE_q ),
	.datac(!\vga_control|V_Cont [1]),
	.datad(gnd),
	.datae(gnd),
	.dataf(gnd),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(),
	.sumout(\vga_control|Add2~25_sumout ),
	.cout(\vga_control|Add2~26 ),
	.shareout());
// synopsys translate_off
defparam \vga_control|Add2~25 .extended_lut = "off";
defparam \vga_control|Add2~25 .lut_mask = 64'h0000F0F000003333;
defparam \vga_control|Add2~25 .shared_arith = "off";
// synopsys translate_on

// Location: MLABCELL_X28_Y77_N3
cyclonev_lcell_comb \vga_control|Add2~29 (
// Equation(s):
// \vga_control|Add2~29_sumout  = SUM(( \vga_control|V_Cont [2] ) + ( VCC ) + ( \vga_control|Add2~26  ))
// \vga_control|Add2~30  = CARRY(( \vga_control|V_Cont [2] ) + ( VCC ) + ( \vga_control|Add2~26  ))

	.dataa(gnd),
	.datab(gnd),
	.datac(gnd),
	.datad(!\vga_control|V_Cont [2]),
	.datae(gnd),
	.dataf(gnd),
	.datag(gnd),
	.cin(\vga_control|Add2~26 ),
	.sharein(gnd),
	.combout(),
	.sumout(\vga_control|Add2~29_sumout ),
	.cout(\vga_control|Add2~30 ),
	.shareout());
// synopsys translate_off
defparam \vga_control|Add2~29 .extended_lut = "off";
defparam \vga_control|Add2~29 .lut_mask = 64'h00000000000000FF;
defparam \vga_control|Add2~29 .shared_arith = "off";
// synopsys translate_on

// Location: MLABCELL_X28_Y77_N6
cyclonev_lcell_comb \vga_control|Add2~17 (
// Equation(s):
// \vga_control|Add2~17_sumout  = SUM(( \vga_control|V_Cont[3]~DUPLICATE_q  ) + ( VCC ) + ( \vga_control|Add2~30  ))
// \vga_control|Add2~18  = CARRY(( \vga_control|V_Cont[3]~DUPLICATE_q  ) + ( VCC ) + ( \vga_control|Add2~30  ))

	.dataa(gnd),
	.datab(gnd),
	.datac(gnd),
	.datad(!\vga_control|V_Cont[3]~DUPLICATE_q ),
	.datae(gnd),
	.dataf(gnd),
	.datag(gnd),
	.cin(\vga_control|Add2~30 ),
	.sharein(gnd),
	.combout(),
	.sumout(\vga_control|Add2~17_sumout ),
	.cout(\vga_control|Add2~18 ),
	.shareout());
// synopsys translate_off
defparam \vga_control|Add2~17 .extended_lut = "off";
defparam \vga_control|Add2~17 .lut_mask = 64'h00000000000000FF;
defparam \vga_control|Add2~17 .shared_arith = "off";
// synopsys translate_on

// Location: MLABCELL_X28_Y77_N9
cyclonev_lcell_comb \vga_control|Add2~21 (
// Equation(s):
// \vga_control|Add2~21_sumout  = SUM(( \vga_control|V_Cont[4]~DUPLICATE_q  ) + ( VCC ) + ( \vga_control|Add2~18  ))
// \vga_control|Add2~22  = CARRY(( \vga_control|V_Cont[4]~DUPLICATE_q  ) + ( VCC ) + ( \vga_control|Add2~18  ))

	.dataa(!\vga_control|V_Cont[4]~DUPLICATE_q ),
	.datab(gnd),
	.datac(gnd),
	.datad(gnd),
	.datae(gnd),
	.dataf(gnd),
	.datag(gnd),
	.cin(\vga_control|Add2~18 ),
	.sharein(gnd),
	.combout(),
	.sumout(\vga_control|Add2~21_sumout ),
	.cout(\vga_control|Add2~22 ),
	.shareout());
// synopsys translate_off
defparam \vga_control|Add2~21 .extended_lut = "off";
defparam \vga_control|Add2~21 .lut_mask = 64'h0000000000005555;
defparam \vga_control|Add2~21 .shared_arith = "off";
// synopsys translate_on

// Location: MLABCELL_X28_Y77_N12
cyclonev_lcell_comb \vga_control|Add2~33 (
// Equation(s):
// \vga_control|Add2~33_sumout  = SUM(( \vga_control|V_Cont[5]~DUPLICATE_q  ) + ( GND ) + ( \vga_control|Add2~22  ))
// \vga_control|Add2~34  = CARRY(( \vga_control|V_Cont[5]~DUPLICATE_q  ) + ( GND ) + ( \vga_control|Add2~22  ))

	.dataa(gnd),
	.datab(!\vga_control|V_Cont[5]~DUPLICATE_q ),
	.datac(gnd),
	.datad(gnd),
	.datae(gnd),
	.dataf(gnd),
	.datag(gnd),
	.cin(\vga_control|Add2~22 ),
	.sharein(gnd),
	.combout(),
	.sumout(\vga_control|Add2~33_sumout ),
	.cout(\vga_control|Add2~34 ),
	.shareout());
// synopsys translate_off
defparam \vga_control|Add2~33 .extended_lut = "off";
defparam \vga_control|Add2~33 .lut_mask = 64'h0000FFFF00003333;
defparam \vga_control|Add2~33 .shared_arith = "off";
// synopsys translate_on

// Location: MLABCELL_X28_Y77_N15
cyclonev_lcell_comb \vga_control|Add2~13 (
// Equation(s):
// \vga_control|Add2~13_sumout  = SUM(( \vga_control|V_Cont [6] ) + ( VCC ) + ( \vga_control|Add2~34  ))
// \vga_control|Add2~14  = CARRY(( \vga_control|V_Cont [6] ) + ( VCC ) + ( \vga_control|Add2~34  ))

	.dataa(gnd),
	.datab(gnd),
	.datac(gnd),
	.datad(!\vga_control|V_Cont [6]),
	.datae(gnd),
	.dataf(gnd),
	.datag(gnd),
	.cin(\vga_control|Add2~34 ),
	.sharein(gnd),
	.combout(),
	.sumout(\vga_control|Add2~13_sumout ),
	.cout(\vga_control|Add2~14 ),
	.shareout());
// synopsys translate_off
defparam \vga_control|Add2~13 .extended_lut = "off";
defparam \vga_control|Add2~13 .lut_mask = 64'h00000000000000FF;
defparam \vga_control|Add2~13 .shared_arith = "off";
// synopsys translate_on

// Location: MLABCELL_X28_Y77_N18
cyclonev_lcell_comb \vga_control|Add2~37 (
// Equation(s):
// \vga_control|Add2~37_sumout  = SUM(( \vga_control|V_Cont [7] ) + ( VCC ) + ( \vga_control|Add2~14  ))
// \vga_control|Add2~38  = CARRY(( \vga_control|V_Cont [7] ) + ( VCC ) + ( \vga_control|Add2~14  ))

	.dataa(gnd),
	.datab(gnd),
	.datac(!\vga_control|V_Cont [7]),
	.datad(gnd),
	.datae(gnd),
	.dataf(gnd),
	.datag(gnd),
	.cin(\vga_control|Add2~14 ),
	.sharein(gnd),
	.combout(),
	.sumout(\vga_control|Add2~37_sumout ),
	.cout(\vga_control|Add2~38 ),
	.shareout());
// synopsys translate_off
defparam \vga_control|Add2~37 .extended_lut = "off";
defparam \vga_control|Add2~37 .lut_mask = 64'h0000000000000F0F;
defparam \vga_control|Add2~37 .shared_arith = "off";
// synopsys translate_on

// Location: MLABCELL_X28_Y77_N21
cyclonev_lcell_comb \vga_control|Add2~41 (
// Equation(s):
// \vga_control|Add2~41_sumout  = SUM(( \vga_control|V_Cont [8] ) + ( VCC ) + ( \vga_control|Add2~38  ))
// \vga_control|Add2~42  = CARRY(( \vga_control|V_Cont [8] ) + ( VCC ) + ( \vga_control|Add2~38  ))

	.dataa(gnd),
	.datab(gnd),
	.datac(!\vga_control|V_Cont [8]),
	.datad(gnd),
	.datae(gnd),
	.dataf(gnd),
	.datag(gnd),
	.cin(\vga_control|Add2~38 ),
	.sharein(gnd),
	.combout(),
	.sumout(\vga_control|Add2~41_sumout ),
	.cout(\vga_control|Add2~42 ),
	.shareout());
// synopsys translate_off
defparam \vga_control|Add2~41 .extended_lut = "off";
defparam \vga_control|Add2~41 .lut_mask = 64'h0000000000000F0F;
defparam \vga_control|Add2~41 .shared_arith = "off";
// synopsys translate_on

// Location: MLABCELL_X28_Y77_N24
cyclonev_lcell_comb \vga_control|Add2~5 (
// Equation(s):
// \vga_control|Add2~5_sumout  = SUM(( \vga_control|V_Cont[9]~DUPLICATE_q  ) + ( VCC ) + ( \vga_control|Add2~42  ))
// \vga_control|Add2~6  = CARRY(( \vga_control|V_Cont[9]~DUPLICATE_q  ) + ( VCC ) + ( \vga_control|Add2~42  ))

	.dataa(gnd),
	.datab(gnd),
	.datac(!\vga_control|V_Cont[9]~DUPLICATE_q ),
	.datad(gnd),
	.datae(gnd),
	.dataf(gnd),
	.datag(gnd),
	.cin(\vga_control|Add2~42 ),
	.sharein(gnd),
	.combout(),
	.sumout(\vga_control|Add2~5_sumout ),
	.cout(\vga_control|Add2~6 ),
	.shareout());
// synopsys translate_off
defparam \vga_control|Add2~5 .extended_lut = "off";
defparam \vga_control|Add2~5 .lut_mask = 64'h0000000000000F0F;
defparam \vga_control|Add2~5 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X28_Y77_N25
dffeas \vga_control|row[9] (
	.clk(rClk[0]),
	.d(\vga_control|Add2~5_sumout ),
	.asdata(vcc),
	.clrn(vcc),
	.aload(gnd),
	.sclr(gnd),
	.sload(gnd),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|row [9]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|row[9] .is_wysiwyg = "true";
defparam \vga_control|row[9] .power_up = "low";
// synopsys translate_on

// Location: MLABCELL_X28_Y77_N27
cyclonev_lcell_comb \vga_control|Add2~9 (
// Equation(s):
// \vga_control|Add2~9_sumout  = SUM(( \vga_control|V_Cont[10]~DUPLICATE_q  ) + ( VCC ) + ( \vga_control|Add2~6  ))
// \vga_control|Add2~10  = CARRY(( \vga_control|V_Cont[10]~DUPLICATE_q  ) + ( VCC ) + ( \vga_control|Add2~6  ))

	.dataa(gnd),
	.datab(gnd),
	.datac(!\vga_control|V_Cont[10]~DUPLICATE_q ),
	.datad(gnd),
	.datae(gnd),
	.dataf(gnd),
	.datag(gnd),
	.cin(\vga_control|Add2~6 ),
	.sharein(gnd),
	.combout(),
	.sumout(\vga_control|Add2~9_sumout ),
	.cout(\vga_control|Add2~10 ),
	.shareout());
// synopsys translate_off
defparam \vga_control|Add2~9 .extended_lut = "off";
defparam \vga_control|Add2~9 .lut_mask = 64'h0000000000000F0F;
defparam \vga_control|Add2~9 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X28_Y77_N28
dffeas \vga_control|row[10] (
	.clk(rClk[0]),
	.d(\vga_control|Add2~9_sumout ),
	.asdata(vcc),
	.clrn(vcc),
	.aload(gnd),
	.sclr(gnd),
	.sload(gnd),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|row [10]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|row[10] .is_wysiwyg = "true";
defparam \vga_control|row[10] .power_up = "low";
// synopsys translate_on

// Location: FF_X30_Y78_N34
dffeas \vga_control|V_Cont[11] (
	.clk(rClk[0]),
	.d(\vga_control|Add4~45_sumout ),
	.asdata(vcc),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(\vga_control|LessThan9~1_combout ),
	.sload(gnd),
	.ena(\vga_control|Equal0~2_combout ),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|V_Cont [11]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|V_Cont[11] .is_wysiwyg = "true";
defparam \vga_control|V_Cont[11] .power_up = "low";
// synopsys translate_on

// Location: MLABCELL_X28_Y77_N30
cyclonev_lcell_comb \vga_control|Add2~1 (
// Equation(s):
// \vga_control|Add2~1_sumout  = SUM(( \vga_control|V_Cont [11] ) + ( VCC ) + ( \vga_control|Add2~10  ))
// \vga_control|Add2~2  = CARRY(( \vga_control|V_Cont [11] ) + ( VCC ) + ( \vga_control|Add2~10  ))

	.dataa(gnd),
	.datab(gnd),
	.datac(!\vga_control|V_Cont [11]),
	.datad(gnd),
	.datae(gnd),
	.dataf(gnd),
	.datag(gnd),
	.cin(\vga_control|Add2~10 ),
	.sharein(gnd),
	.combout(),
	.sumout(\vga_control|Add2~1_sumout ),
	.cout(\vga_control|Add2~2 ),
	.shareout());
// synopsys translate_off
defparam \vga_control|Add2~1 .extended_lut = "off";
defparam \vga_control|Add2~1 .lut_mask = 64'h0000000000000F0F;
defparam \vga_control|Add2~1 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X28_Y77_N31
dffeas \vga_control|row[11] (
	.clk(rClk[0]),
	.d(\vga_control|Add2~1_sumout ),
	.asdata(vcc),
	.clrn(vcc),
	.aload(gnd),
	.sclr(gnd),
	.sload(gnd),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|row [11]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|row[11] .is_wysiwyg = "true";
defparam \vga_control|row[11] .power_up = "low";
// synopsys translate_on

// Location: MLABCELL_X28_Y77_N33
cyclonev_lcell_comb \vga_control|Add2~45 (
// Equation(s):
// \vga_control|Add2~45_sumout  = SUM(( \vga_control|V_Cont[12]~DUPLICATE_q  ) + ( VCC ) + ( \vga_control|Add2~2  ))

	.dataa(gnd),
	.datab(gnd),
	.datac(!\vga_control|V_Cont[12]~DUPLICATE_q ),
	.datad(gnd),
	.datae(gnd),
	.dataf(gnd),
	.datag(gnd),
	.cin(\vga_control|Add2~2 ),
	.sharein(gnd),
	.combout(),
	.sumout(\vga_control|Add2~45_sumout ),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \vga_control|Add2~45 .extended_lut = "off";
defparam \vga_control|Add2~45 .lut_mask = 64'h0000000000000F0F;
defparam \vga_control|Add2~45 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X28_Y77_N35
dffeas \vga_control|row[12] (
	.clk(rClk[0]),
	.d(\vga_control|Add2~45_sumout ),
	.asdata(vcc),
	.clrn(vcc),
	.aload(gnd),
	.sclr(gnd),
	.sload(gnd),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|row [12]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|row[12] .is_wysiwyg = "true";
defparam \vga_control|row[12] .power_up = "low";
// synopsys translate_on

// Location: MLABCELL_X28_Y77_N57
cyclonev_lcell_comb \red_c~0 (
// Equation(s):
// \red_c~0_combout  = ( !\vga_control|row [12] & ( (!\vga_control|row [9] & (!\vga_control|row [10] & !\vga_control|row [11])) ) )

	.dataa(gnd),
	.datab(!\vga_control|row [9]),
	.datac(!\vga_control|row [10]),
	.datad(!\vga_control|row [11]),
	.datae(gnd),
	.dataf(!\vga_control|row [12]),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(\red_c~0_combout ),
	.sumout(),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \red_c~0 .extended_lut = "off";
defparam \red_c~0 .lut_mask = 64'hC000C00000000000;
defparam \red_c~0 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X28_Y77_N22
dffeas \vga_control|row[8] (
	.clk(rClk[0]),
	.d(\vga_control|Add2~41_sumout ),
	.asdata(vcc),
	.clrn(vcc),
	.aload(gnd),
	.sclr(gnd),
	.sload(gnd),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|row [8]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|row[8] .is_wysiwyg = "true";
defparam \vga_control|row[8] .power_up = "low";
// synopsys translate_on

// Location: FF_X28_Y77_N20
dffeas \vga_control|row[7] (
	.clk(rClk[0]),
	.d(\vga_control|Add2~37_sumout ),
	.asdata(vcc),
	.clrn(vcc),
	.aload(gnd),
	.sclr(gnd),
	.sload(gnd),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|row [7]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|row[7] .is_wysiwyg = "true";
defparam \vga_control|row[7] .power_up = "low";
// synopsys translate_on

// Location: LABCELL_X29_Y77_N39
cyclonev_lcell_comb \LessThan4~0 (
// Equation(s):
// \LessThan4~0_combout  = ( \vga_control|row [7] & ( \vga_control|row [8] ) )

	.dataa(!\vga_control|row [8]),
	.datab(gnd),
	.datac(gnd),
	.datad(gnd),
	.datae(gnd),
	.dataf(!\vga_control|row [7]),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(\LessThan4~0_combout ),
	.sumout(),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \LessThan4~0 .extended_lut = "off";
defparam \LessThan4~0 .lut_mask = 64'h0000000055555555;
defparam \LessThan4~0 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X28_Y77_N17
dffeas \vga_control|row[6] (
	.clk(rClk[0]),
	.d(\vga_control|Add2~13_sumout ),
	.asdata(vcc),
	.clrn(vcc),
	.aload(gnd),
	.sclr(gnd),
	.sload(gnd),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|row [6]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|row[6] .is_wysiwyg = "true";
defparam \vga_control|row[6] .power_up = "low";
// synopsys translate_on

// Location: FF_X28_Y77_N4
dffeas \vga_control|row[2] (
	.clk(rClk[0]),
	.d(\vga_control|Add2~29_sumout ),
	.asdata(vcc),
	.clrn(vcc),
	.aload(gnd),
	.sclr(gnd),
	.sload(gnd),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|row [2]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|row[2] .is_wysiwyg = "true";
defparam \vga_control|row[2] .power_up = "low";
// synopsys translate_on

// Location: LABCELL_X27_Y77_N12
cyclonev_lcell_comb \vga_control|row[0]~0 (
// Equation(s):
// \vga_control|row[0]~0_combout  = !\vga_control|V_Cont[0]~DUPLICATE_q 

	.dataa(gnd),
	.datab(gnd),
	.datac(gnd),
	.datad(!\vga_control|V_Cont[0]~DUPLICATE_q ),
	.datae(gnd),
	.dataf(gnd),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(\vga_control|row[0]~0_combout ),
	.sumout(),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \vga_control|row[0]~0 .extended_lut = "off";
defparam \vga_control|row[0]~0 .lut_mask = 64'hFF00FF00FF00FF00;
defparam \vga_control|row[0]~0 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X28_Y77_N40
dffeas \vga_control|row[0]~DUPLICATE (
	.clk(rClk[0]),
	.d(gnd),
	.asdata(\vga_control|row[0]~0_combout ),
	.clrn(vcc),
	.aload(gnd),
	.sclr(gnd),
	.sload(vcc),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|row[0]~DUPLICATE_q ),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|row[0]~DUPLICATE .is_wysiwyg = "true";
defparam \vga_control|row[0]~DUPLICATE .power_up = "low";
// synopsys translate_on

// Location: FF_X28_Y77_N2
dffeas \vga_control|row[1]~DUPLICATE (
	.clk(rClk[0]),
	.d(\vga_control|Add2~25_sumout ),
	.asdata(vcc),
	.clrn(vcc),
	.aload(gnd),
	.sclr(gnd),
	.sload(gnd),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|row[1]~DUPLICATE_q ),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|row[1]~DUPLICATE .is_wysiwyg = "true";
defparam \vga_control|row[1]~DUPLICATE .power_up = "low";
// synopsys translate_on

// Location: FF_X28_Y77_N8
dffeas \vga_control|row[3]~DUPLICATE (
	.clk(rClk[0]),
	.d(\vga_control|Add2~17_sumout ),
	.asdata(vcc),
	.clrn(vcc),
	.aload(gnd),
	.sclr(gnd),
	.sload(gnd),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|row[3]~DUPLICATE_q ),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|row[3]~DUPLICATE .is_wysiwyg = "true";
defparam \vga_control|row[3]~DUPLICATE .power_up = "low";
// synopsys translate_on

// Location: FF_X28_Y77_N10
dffeas \vga_control|row[4]~DUPLICATE (
	.clk(rClk[0]),
	.d(\vga_control|Add2~21_sumout ),
	.asdata(vcc),
	.clrn(vcc),
	.aload(gnd),
	.sclr(gnd),
	.sload(gnd),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|row[4]~DUPLICATE_q ),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|row[4]~DUPLICATE .is_wysiwyg = "true";
defparam \vga_control|row[4]~DUPLICATE .power_up = "low";
// synopsys translate_on

// Location: FF_X28_Y77_N14
dffeas \vga_control|row[5]~DUPLICATE (
	.clk(rClk[0]),
	.d(\vga_control|Add2~33_sumout ),
	.asdata(vcc),
	.clrn(vcc),
	.aload(gnd),
	.sclr(gnd),
	.sload(gnd),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|row[5]~DUPLICATE_q ),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|row[5]~DUPLICATE .is_wysiwyg = "true";
defparam \vga_control|row[5]~DUPLICATE .power_up = "low";
// synopsys translate_on

// Location: LABCELL_X27_Y77_N6
cyclonev_lcell_comb \LessThan2~0 (
// Equation(s):
// \LessThan2~0_combout  = ( !\vga_control|row[4]~DUPLICATE_q  & ( !\vga_control|row[5]~DUPLICATE_q  & ( (!\vga_control|row [2] & (!\vga_control|row[0]~DUPLICATE_q  & (!\vga_control|row[1]~DUPLICATE_q  & !\vga_control|row[3]~DUPLICATE_q ))) ) ) )

	.dataa(!\vga_control|row [2]),
	.datab(!\vga_control|row[0]~DUPLICATE_q ),
	.datac(!\vga_control|row[1]~DUPLICATE_q ),
	.datad(!\vga_control|row[3]~DUPLICATE_q ),
	.datae(!\vga_control|row[4]~DUPLICATE_q ),
	.dataf(!\vga_control|row[5]~DUPLICATE_q ),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(\LessThan2~0_combout ),
	.sumout(),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \LessThan2~0 .extended_lut = "off";
defparam \LessThan2~0 .lut_mask = 64'h8000000000000000;
defparam \LessThan2~0 .shared_arith = "off";
// synopsys translate_on

// Location: LABCELL_X27_Y77_N36
cyclonev_lcell_comb \red_c~1 (
// Equation(s):
// \red_c~1_combout  = ( \LessThan2~0_combout  & ( \red_c~0_combout  ) ) # ( !\LessThan2~0_combout  & ( (\red_c~0_combout  & ((!\LessThan4~0_combout ) # (!\vga_control|row [6]))) ) )

	.dataa(!\red_c~0_combout ),
	.datab(gnd),
	.datac(!\LessThan4~0_combout ),
	.datad(!\vga_control|row [6]),
	.datae(gnd),
	.dataf(!\LessThan2~0_combout ),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(\red_c~1_combout ),
	.sumout(),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \red_c~1 .extended_lut = "off";
defparam \red_c~1 .lut_mask = 64'h5550555055555555;
defparam \red_c~1 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X28_Y77_N13
dffeas \vga_control|row[5] (
	.clk(rClk[0]),
	.d(\vga_control|Add2~33_sumout ),
	.asdata(vcc),
	.clrn(vcc),
	.aload(gnd),
	.sclr(gnd),
	.sload(gnd),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|row [5]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|row[5] .is_wysiwyg = "true";
defparam \vga_control|row[5] .power_up = "low";
// synopsys translate_on

// Location: FF_X28_Y77_N1
dffeas \vga_control|row[1] (
	.clk(rClk[0]),
	.d(\vga_control|Add2~25_sumout ),
	.asdata(vcc),
	.clrn(vcc),
	.aload(gnd),
	.sclr(gnd),
	.sload(gnd),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|row [1]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|row[1] .is_wysiwyg = "true";
defparam \vga_control|row[1] .power_up = "low";
// synopsys translate_on

// Location: FF_X28_Y77_N7
dffeas \vga_control|row[3] (
	.clk(rClk[0]),
	.d(\vga_control|Add2~17_sumout ),
	.asdata(vcc),
	.clrn(vcc),
	.aload(gnd),
	.sclr(gnd),
	.sload(gnd),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|row [3]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|row[3] .is_wysiwyg = "true";
defparam \vga_control|row[3] .power_up = "low";
// synopsys translate_on

// Location: MLABCELL_X28_Y77_N48
cyclonev_lcell_comb \LessThan4~1 (
// Equation(s):
// \LessThan4~1_combout  = ( \vga_control|row [3] & ( (!\vga_control|row [5] & !\vga_control|row[4]~DUPLICATE_q ) ) ) # ( !\vga_control|row [3] & ( (!\vga_control|row [5] & ((!\vga_control|row[4]~DUPLICATE_q ) # ((!\vga_control|row [1] & !\vga_control|row 
// [2])))) ) )

	.dataa(!\vga_control|row [5]),
	.datab(!\vga_control|row[4]~DUPLICATE_q ),
	.datac(!\vga_control|row [1]),
	.datad(!\vga_control|row [2]),
	.datae(gnd),
	.dataf(!\vga_control|row [3]),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(\LessThan4~1_combout ),
	.sumout(),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \LessThan4~1 .extended_lut = "off";
defparam \LessThan4~1 .lut_mask = 64'hA888A88888888888;
defparam \LessThan4~1 .shared_arith = "off";
// synopsys translate_on

// Location: LABCELL_X29_Y77_N9
cyclonev_lcell_comb \LessThan4~2 (
// Equation(s):
// \LessThan4~2_combout  = ( \LessThan4~0_combout  & ( (\vga_control|row [6] & !\LessThan4~1_combout ) ) )

	.dataa(!\vga_control|row [6]),
	.datab(gnd),
	.datac(!\LessThan4~1_combout ),
	.datad(gnd),
	.datae(gnd),
	.dataf(!\LessThan4~0_combout ),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(\LessThan4~2_combout ),
	.sumout(),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \LessThan4~2 .extended_lut = "off";
defparam \LessThan4~2 .lut_mask = 64'h0000000050505050;
defparam \LessThan4~2 .shared_arith = "off";
// synopsys translate_on

// Location: LABCELL_X29_Y78_N0
cyclonev_lcell_comb \vga_control|Add1~50 (
// Equation(s):
// \vga_control|Add1~50_cout  = CARRY(( \vga_control|h_cont [0] ) + ( VCC ) + ( !VCC ))

	.dataa(gnd),
	.datab(gnd),
	.datac(gnd),
	.datad(!\vga_control|h_cont [0]),
	.datae(gnd),
	.dataf(gnd),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(),
	.sumout(),
	.cout(\vga_control|Add1~50_cout ),
	.shareout());
// synopsys translate_off
defparam \vga_control|Add1~50 .extended_lut = "off";
defparam \vga_control|Add1~50 .lut_mask = 64'h00000000000000FF;
defparam \vga_control|Add1~50 .shared_arith = "off";
// synopsys translate_on

// Location: LABCELL_X29_Y78_N3
cyclonev_lcell_comb \vga_control|Add1~46 (
// Equation(s):
// \vga_control|Add1~46_cout  = CARRY(( \vga_control|h_cont [1] ) + ( VCC ) + ( \vga_control|Add1~50_cout  ))

	.dataa(gnd),
	.datab(gnd),
	.datac(!\vga_control|h_cont [1]),
	.datad(gnd),
	.datae(gnd),
	.dataf(gnd),
	.datag(gnd),
	.cin(\vga_control|Add1~50_cout ),
	.sharein(gnd),
	.combout(),
	.sumout(),
	.cout(\vga_control|Add1~46_cout ),
	.shareout());
// synopsys translate_off
defparam \vga_control|Add1~46 .extended_lut = "off";
defparam \vga_control|Add1~46 .lut_mask = 64'h0000000000000F0F;
defparam \vga_control|Add1~46 .shared_arith = "off";
// synopsys translate_on

// Location: LABCELL_X29_Y78_N6
cyclonev_lcell_comb \vga_control|Add1~17 (
// Equation(s):
// \vga_control|Add1~17_sumout  = SUM(( \vga_control|h_cont[2]~DUPLICATE_q  ) + ( GND ) + ( \vga_control|Add1~46_cout  ))
// \vga_control|Add1~18  = CARRY(( \vga_control|h_cont[2]~DUPLICATE_q  ) + ( GND ) + ( \vga_control|Add1~46_cout  ))

	.dataa(gnd),
	.datab(gnd),
	.datac(!\vga_control|h_cont[2]~DUPLICATE_q ),
	.datad(gnd),
	.datae(gnd),
	.dataf(gnd),
	.datag(gnd),
	.cin(\vga_control|Add1~46_cout ),
	.sharein(gnd),
	.combout(),
	.sumout(\vga_control|Add1~17_sumout ),
	.cout(\vga_control|Add1~18 ),
	.shareout());
// synopsys translate_off
defparam \vga_control|Add1~17 .extended_lut = "off";
defparam \vga_control|Add1~17 .lut_mask = 64'h0000FFFF00000F0F;
defparam \vga_control|Add1~17 .shared_arith = "off";
// synopsys translate_on

// Location: LABCELL_X29_Y78_N9
cyclonev_lcell_comb \vga_control|Add1~5 (
// Equation(s):
// \vga_control|Add1~5_sumout  = SUM(( \vga_control|h_cont [3] ) + ( GND ) + ( \vga_control|Add1~18  ))
// \vga_control|Add1~6  = CARRY(( \vga_control|h_cont [3] ) + ( GND ) + ( \vga_control|Add1~18  ))

	.dataa(!\vga_control|h_cont [3]),
	.datab(gnd),
	.datac(gnd),
	.datad(gnd),
	.datae(gnd),
	.dataf(gnd),
	.datag(gnd),
	.cin(\vga_control|Add1~18 ),
	.sharein(gnd),
	.combout(),
	.sumout(\vga_control|Add1~5_sumout ),
	.cout(\vga_control|Add1~6 ),
	.shareout());
// synopsys translate_off
defparam \vga_control|Add1~5 .extended_lut = "off";
defparam \vga_control|Add1~5 .lut_mask = 64'h0000FFFF00005555;
defparam \vga_control|Add1~5 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X29_Y78_N10
dffeas \vga_control|col[3] (
	.clk(rClk[0]),
	.d(\vga_control|Add1~5_sumout ),
	.asdata(vcc),
	.clrn(vcc),
	.aload(gnd),
	.sclr(gnd),
	.sload(gnd),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|col [3]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|col[3] .is_wysiwyg = "true";
defparam \vga_control|col[3] .power_up = "low";
// synopsys translate_on

// Location: FF_X29_Y78_N8
dffeas \vga_control|col[2] (
	.clk(rClk[0]),
	.d(\vga_control|Add1~17_sumout ),
	.asdata(vcc),
	.clrn(vcc),
	.aload(gnd),
	.sclr(gnd),
	.sload(gnd),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|col [2]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|col[2] .is_wysiwyg = "true";
defparam \vga_control|col[2] .power_up = "low";
// synopsys translate_on

// Location: LABCELL_X29_Y78_N12
cyclonev_lcell_comb \vga_control|Add1~9 (
// Equation(s):
// \vga_control|Add1~9_sumout  = SUM(( \vga_control|h_cont[4]~DUPLICATE_q  ) + ( VCC ) + ( \vga_control|Add1~6  ))
// \vga_control|Add1~10  = CARRY(( \vga_control|h_cont[4]~DUPLICATE_q  ) + ( VCC ) + ( \vga_control|Add1~6  ))

	.dataa(gnd),
	.datab(!\vga_control|h_cont[4]~DUPLICATE_q ),
	.datac(gnd),
	.datad(gnd),
	.datae(gnd),
	.dataf(gnd),
	.datag(gnd),
	.cin(\vga_control|Add1~6 ),
	.sharein(gnd),
	.combout(),
	.sumout(\vga_control|Add1~9_sumout ),
	.cout(\vga_control|Add1~10 ),
	.shareout());
// synopsys translate_off
defparam \vga_control|Add1~9 .extended_lut = "off";
defparam \vga_control|Add1~9 .lut_mask = 64'h0000000000003333;
defparam \vga_control|Add1~9 .shared_arith = "off";
// synopsys translate_on

// Location: LABCELL_X29_Y78_N15
cyclonev_lcell_comb \vga_control|Add1~13 (
// Equation(s):
// \vga_control|Add1~13_sumout  = SUM(( \vga_control|h_cont [5] ) + ( VCC ) + ( \vga_control|Add1~10  ))
// \vga_control|Add1~14  = CARRY(( \vga_control|h_cont [5] ) + ( VCC ) + ( \vga_control|Add1~10  ))

	.dataa(gnd),
	.datab(gnd),
	.datac(gnd),
	.datad(!\vga_control|h_cont [5]),
	.datae(gnd),
	.dataf(gnd),
	.datag(gnd),
	.cin(\vga_control|Add1~10 ),
	.sharein(gnd),
	.combout(),
	.sumout(\vga_control|Add1~13_sumout ),
	.cout(\vga_control|Add1~14 ),
	.shareout());
// synopsys translate_off
defparam \vga_control|Add1~13 .extended_lut = "off";
defparam \vga_control|Add1~13 .lut_mask = 64'h00000000000000FF;
defparam \vga_control|Add1~13 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X29_Y78_N16
dffeas \vga_control|col[5] (
	.clk(rClk[0]),
	.d(\vga_control|Add1~13_sumout ),
	.asdata(vcc),
	.clrn(vcc),
	.aload(gnd),
	.sclr(gnd),
	.sload(gnd),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|col [5]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|col[5] .is_wysiwyg = "true";
defparam \vga_control|col[5] .power_up = "low";
// synopsys translate_on

// Location: FF_X29_Y78_N13
dffeas \vga_control|col[4] (
	.clk(rClk[0]),
	.d(\vga_control|Add1~9_sumout ),
	.asdata(vcc),
	.clrn(vcc),
	.aload(gnd),
	.sclr(gnd),
	.sload(gnd),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|col [4]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|col[4] .is_wysiwyg = "true";
defparam \vga_control|col[4] .power_up = "low";
// synopsys translate_on

// Location: LABCELL_X29_Y78_N18
cyclonev_lcell_comb \vga_control|Add1~37 (
// Equation(s):
// \vga_control|Add1~37_sumout  = SUM(( \vga_control|h_cont[6]~DUPLICATE_q  ) + ( VCC ) + ( \vga_control|Add1~14  ))
// \vga_control|Add1~38  = CARRY(( \vga_control|h_cont[6]~DUPLICATE_q  ) + ( VCC ) + ( \vga_control|Add1~14  ))

	.dataa(gnd),
	.datab(!\vga_control|h_cont[6]~DUPLICATE_q ),
	.datac(gnd),
	.datad(gnd),
	.datae(gnd),
	.dataf(gnd),
	.datag(gnd),
	.cin(\vga_control|Add1~14 ),
	.sharein(gnd),
	.combout(),
	.sumout(\vga_control|Add1~37_sumout ),
	.cout(\vga_control|Add1~38 ),
	.shareout());
// synopsys translate_off
defparam \vga_control|Add1~37 .extended_lut = "off";
defparam \vga_control|Add1~37 .lut_mask = 64'h0000000000003333;
defparam \vga_control|Add1~37 .shared_arith = "off";
// synopsys translate_on

// Location: LABCELL_X29_Y78_N21
cyclonev_lcell_comb \vga_control|Add1~41 (
// Equation(s):
// \vga_control|Add1~41_sumout  = SUM(( \vga_control|h_cont [7] ) + ( GND ) + ( \vga_control|Add1~38  ))
// \vga_control|Add1~42  = CARRY(( \vga_control|h_cont [7] ) + ( GND ) + ( \vga_control|Add1~38  ))

	.dataa(gnd),
	.datab(gnd),
	.datac(!\vga_control|h_cont [7]),
	.datad(gnd),
	.datae(gnd),
	.dataf(gnd),
	.datag(gnd),
	.cin(\vga_control|Add1~38 ),
	.sharein(gnd),
	.combout(),
	.sumout(\vga_control|Add1~41_sumout ),
	.cout(\vga_control|Add1~42 ),
	.shareout());
// synopsys translate_off
defparam \vga_control|Add1~41 .extended_lut = "off";
defparam \vga_control|Add1~41 .lut_mask = 64'h0000FFFF00000F0F;
defparam \vga_control|Add1~41 .shared_arith = "off";
// synopsys translate_on

// Location: LABCELL_X29_Y78_N24
cyclonev_lcell_comb \vga_control|Add1~1 (
// Equation(s):
// \vga_control|Add1~1_sumout  = SUM(( \vga_control|h_cont[8]~DUPLICATE_q  ) + ( VCC ) + ( \vga_control|Add1~42  ))
// \vga_control|Add1~2  = CARRY(( \vga_control|h_cont[8]~DUPLICATE_q  ) + ( VCC ) + ( \vga_control|Add1~42  ))

	.dataa(gnd),
	.datab(!\vga_control|h_cont[8]~DUPLICATE_q ),
	.datac(gnd),
	.datad(gnd),
	.datae(gnd),
	.dataf(gnd),
	.datag(gnd),
	.cin(\vga_control|Add1~42 ),
	.sharein(gnd),
	.combout(),
	.sumout(\vga_control|Add1~1_sumout ),
	.cout(\vga_control|Add1~2 ),
	.shareout());
// synopsys translate_off
defparam \vga_control|Add1~1 .extended_lut = "off";
defparam \vga_control|Add1~1 .lut_mask = 64'h0000000000003333;
defparam \vga_control|Add1~1 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X29_Y78_N26
dffeas \vga_control|col[8] (
	.clk(rClk[0]),
	.d(\vga_control|Add1~1_sumout ),
	.asdata(vcc),
	.clrn(vcc),
	.aload(gnd),
	.sclr(gnd),
	.sload(gnd),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|col [8]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|col[8] .is_wysiwyg = "true";
defparam \vga_control|col[8] .power_up = "low";
// synopsys translate_on

// Location: MLABCELL_X28_Y78_N3
cyclonev_lcell_comb \always1~0 (
// Equation(s):
// \always1~0_combout  = ( \vga_control|col [4] & ( \vga_control|col [8] & ( (\vga_control|col [2]) # (\vga_control|col [3]) ) ) ) # ( !\vga_control|col [4] & ( !\vga_control|col [8] & ( (!\vga_control|col [3] & !\vga_control|col [5]) ) ) )

	.dataa(!\vga_control|col [3]),
	.datab(!\vga_control|col [2]),
	.datac(gnd),
	.datad(!\vga_control|col [5]),
	.datae(!\vga_control|col [4]),
	.dataf(!\vga_control|col [8]),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(\always1~0_combout ),
	.sumout(),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \always1~0 .extended_lut = "off";
defparam \always1~0 .lut_mask = 64'hAA00000000007777;
defparam \always1~0 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X28_Y77_N11
dffeas \vga_control|row[4] (
	.clk(rClk[0]),
	.d(\vga_control|Add2~21_sumout ),
	.asdata(vcc),
	.clrn(vcc),
	.aload(gnd),
	.sclr(gnd),
	.sload(gnd),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|row [4]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|row[4] .is_wysiwyg = "true";
defparam \vga_control|row[4] .power_up = "low";
// synopsys translate_on

// Location: MLABCELL_X28_Y77_N51
cyclonev_lcell_comb \LessThan3~0 (
// Equation(s):
// \LessThan3~0_combout  = ( !\vga_control|row [3] & ( (!\vga_control|row [4] & !\vga_control|row [5]) ) )

	.dataa(gnd),
	.datab(gnd),
	.datac(!\vga_control|row [4]),
	.datad(!\vga_control|row [5]),
	.datae(gnd),
	.dataf(!\vga_control|row [3]),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(\LessThan3~0_combout ),
	.sumout(),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \LessThan3~0 .extended_lut = "off";
defparam \LessThan3~0 .lut_mask = 64'hF000F00000000000;
defparam \LessThan3~0 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X28_Y77_N23
dffeas \vga_control|row[8]~DUPLICATE (
	.clk(rClk[0]),
	.d(\vga_control|Add2~41_sumout ),
	.asdata(vcc),
	.clrn(vcc),
	.aload(gnd),
	.sclr(gnd),
	.sload(gnd),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|row[8]~DUPLICATE_q ),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|row[8]~DUPLICATE .is_wysiwyg = "true";
defparam \vga_control|row[8]~DUPLICATE .power_up = "low";
// synopsys translate_on

// Location: LABCELL_X29_Y78_N27
cyclonev_lcell_comb \vga_control|Add1~21 (
// Equation(s):
// \vga_control|Add1~21_sumout  = SUM(( \vga_control|h_cont [9] ) + ( VCC ) + ( \vga_control|Add1~2  ))
// \vga_control|Add1~22  = CARRY(( \vga_control|h_cont [9] ) + ( VCC ) + ( \vga_control|Add1~2  ))

	.dataa(!\vga_control|h_cont [9]),
	.datab(gnd),
	.datac(gnd),
	.datad(gnd),
	.datae(gnd),
	.dataf(gnd),
	.datag(gnd),
	.cin(\vga_control|Add1~2 ),
	.sharein(gnd),
	.combout(),
	.sumout(\vga_control|Add1~21_sumout ),
	.cout(\vga_control|Add1~22 ),
	.shareout());
// synopsys translate_off
defparam \vga_control|Add1~21 .extended_lut = "off";
defparam \vga_control|Add1~21 .lut_mask = 64'h0000000000005555;
defparam \vga_control|Add1~21 .shared_arith = "off";
// synopsys translate_on

// Location: LABCELL_X29_Y78_N30
cyclonev_lcell_comb \vga_control|Add1~25 (
// Equation(s):
// \vga_control|Add1~25_sumout  = SUM(( \vga_control|h_cont [10] ) + ( VCC ) + ( \vga_control|Add1~22  ))
// \vga_control|Add1~26  = CARRY(( \vga_control|h_cont [10] ) + ( VCC ) + ( \vga_control|Add1~22  ))

	.dataa(gnd),
	.datab(!\vga_control|h_cont [10]),
	.datac(gnd),
	.datad(gnd),
	.datae(gnd),
	.dataf(gnd),
	.datag(gnd),
	.cin(\vga_control|Add1~22 ),
	.sharein(gnd),
	.combout(),
	.sumout(\vga_control|Add1~25_sumout ),
	.cout(\vga_control|Add1~26 ),
	.shareout());
// synopsys translate_off
defparam \vga_control|Add1~25 .extended_lut = "off";
defparam \vga_control|Add1~25 .lut_mask = 64'h0000000000003333;
defparam \vga_control|Add1~25 .shared_arith = "off";
// synopsys translate_on

// Location: LABCELL_X29_Y78_N33
cyclonev_lcell_comb \vga_control|Add1~29 (
// Equation(s):
// \vga_control|Add1~29_sumout  = SUM(( \vga_control|h_cont [11] ) + ( VCC ) + ( \vga_control|Add1~26  ))
// \vga_control|Add1~30  = CARRY(( \vga_control|h_cont [11] ) + ( VCC ) + ( \vga_control|Add1~26  ))

	.dataa(!\vga_control|h_cont [11]),
	.datab(gnd),
	.datac(gnd),
	.datad(gnd),
	.datae(gnd),
	.dataf(gnd),
	.datag(gnd),
	.cin(\vga_control|Add1~26 ),
	.sharein(gnd),
	.combout(),
	.sumout(\vga_control|Add1~29_sumout ),
	.cout(\vga_control|Add1~30 ),
	.shareout());
// synopsys translate_off
defparam \vga_control|Add1~29 .extended_lut = "off";
defparam \vga_control|Add1~29 .lut_mask = 64'h0000000000005555;
defparam \vga_control|Add1~29 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X29_Y78_N34
dffeas \vga_control|col[11] (
	.clk(rClk[0]),
	.d(\vga_control|Add1~29_sumout ),
	.asdata(vcc),
	.clrn(vcc),
	.aload(gnd),
	.sclr(gnd),
	.sload(gnd),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|col [11]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|col[11] .is_wysiwyg = "true";
defparam \vga_control|col[11] .power_up = "low";
// synopsys translate_on

// Location: FF_X29_Y78_N28
dffeas \vga_control|col[9] (
	.clk(rClk[0]),
	.d(\vga_control|Add1~21_sumout ),
	.asdata(vcc),
	.clrn(vcc),
	.aload(gnd),
	.sclr(gnd),
	.sload(gnd),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|col [9]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|col[9] .is_wysiwyg = "true";
defparam \vga_control|col[9] .power_up = "low";
// synopsys translate_on

// Location: LABCELL_X29_Y78_N36
cyclonev_lcell_comb \vga_control|Add1~33 (
// Equation(s):
// \vga_control|Add1~33_sumout  = SUM(( \vga_control|h_cont [12] ) + ( VCC ) + ( \vga_control|Add1~30  ))

	.dataa(gnd),
	.datab(gnd),
	.datac(!\vga_control|h_cont [12]),
	.datad(gnd),
	.datae(gnd),
	.dataf(gnd),
	.datag(gnd),
	.cin(\vga_control|Add1~30 ),
	.sharein(gnd),
	.combout(),
	.sumout(\vga_control|Add1~33_sumout ),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \vga_control|Add1~33 .extended_lut = "off";
defparam \vga_control|Add1~33 .lut_mask = 64'h0000000000000F0F;
defparam \vga_control|Add1~33 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X29_Y78_N37
dffeas \vga_control|col[12] (
	.clk(rClk[0]),
	.d(\vga_control|Add1~33_sumout ),
	.asdata(vcc),
	.clrn(vcc),
	.aload(gnd),
	.sclr(gnd),
	.sload(gnd),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|col [12]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|col[12] .is_wysiwyg = "true";
defparam \vga_control|col[12] .power_up = "low";
// synopsys translate_on

// Location: FF_X29_Y78_N31
dffeas \vga_control|col[10] (
	.clk(rClk[0]),
	.d(\vga_control|Add1~25_sumout ),
	.asdata(vcc),
	.clrn(vcc),
	.aload(gnd),
	.sclr(gnd),
	.sload(gnd),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|col [10]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|col[10] .is_wysiwyg = "true";
defparam \vga_control|col[10] .power_up = "low";
// synopsys translate_on

// Location: MLABCELL_X28_Y78_N30
cyclonev_lcell_comb \always1~1 (
// Equation(s):
// \always1~1_combout  = ( \vga_control|row [6] & ( !\vga_control|col [10] & ( (!\vga_control|col [11] & (!\vga_control|col [9] & !\vga_control|col [12])) ) ) ) # ( !\vga_control|row [6] & ( !\vga_control|col [10] & ( (!\vga_control|col [11] & 
// (\vga_control|row[8]~DUPLICATE_q  & (!\vga_control|col [9] & !\vga_control|col [12]))) ) ) )

	.dataa(!\vga_control|col [11]),
	.datab(!\vga_control|row[8]~DUPLICATE_q ),
	.datac(!\vga_control|col [9]),
	.datad(!\vga_control|col [12]),
	.datae(!\vga_control|row [6]),
	.dataf(!\vga_control|col [10]),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(\always1~1_combout ),
	.sumout(),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \always1~1 .extended_lut = "off";
defparam \always1~1 .lut_mask = 64'h2000A00000000000;
defparam \always1~1 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X29_Y78_N23
dffeas \vga_control|col[7] (
	.clk(rClk[0]),
	.d(\vga_control|Add1~41_sumout ),
	.asdata(vcc),
	.clrn(vcc),
	.aload(gnd),
	.sclr(gnd),
	.sload(gnd),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|col [7]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|col[7] .is_wysiwyg = "true";
defparam \vga_control|col[7] .power_up = "low";
// synopsys translate_on

// Location: FF_X29_Y78_N19
dffeas \vga_control|col[6] (
	.clk(rClk[0]),
	.d(\vga_control|Add1~37_sumout ),
	.asdata(vcc),
	.clrn(vcc),
	.aload(gnd),
	.sclr(gnd),
	.sload(gnd),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|col [6]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|col[6] .is_wysiwyg = "true";
defparam \vga_control|col[6] .power_up = "low";
// synopsys translate_on

// Location: MLABCELL_X28_Y78_N48
cyclonev_lcell_comb \always1~2 (
// Equation(s):
// \always1~2_combout  = ( !\vga_control|col [6] & ( \vga_control|col [8] & ( (!\vga_control|col [7] & (!\vga_control|col [5] & ((\vga_control|row [7]) # (\vga_control|row [8])))) ) ) ) # ( \vga_control|col [6] & ( !\vga_control|col [8] & ( (\vga_control|col 
// [7] & ((\vga_control|row [7]) # (\vga_control|row [8]))) ) ) )

	.dataa(!\vga_control|row [8]),
	.datab(!\vga_control|col [7]),
	.datac(!\vga_control|col [5]),
	.datad(!\vga_control|row [7]),
	.datae(!\vga_control|col [6]),
	.dataf(!\vga_control|col [8]),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(\always1~2_combout ),
	.sumout(),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \always1~2 .extended_lut = "off";
defparam \always1~2 .lut_mask = 64'h0000113340C00000;
defparam \always1~2 .shared_arith = "off";
// synopsys translate_on

// Location: MLABCELL_X28_Y78_N54
cyclonev_lcell_comb \always1~3 (
// Equation(s):
// \always1~3_combout  = ( \always1~1_combout  & ( \always1~2_combout  & ( (\red_c~0_combout  & (!\always1~0_combout  & ((!\LessThan3~0_combout ) # (\vga_control|row[8]~DUPLICATE_q )))) ) ) )

	.dataa(!\red_c~0_combout ),
	.datab(!\always1~0_combout ),
	.datac(!\LessThan3~0_combout ),
	.datad(!\vga_control|row[8]~DUPLICATE_q ),
	.datae(!\always1~1_combout ),
	.dataf(!\always1~2_combout ),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(\always1~3_combout ),
	.sumout(),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \always1~3 .extended_lut = "off";
defparam \always1~3 .lut_mask = 64'h0000000000004044;
defparam \always1~3 .shared_arith = "off";
// synopsys translate_on

// Location: LABCELL_X27_Y77_N21
cyclonev_lcell_comb \LessThan1~1 (
// Equation(s):
// \LessThan1~1_combout  = ( \vga_control|row[5]~DUPLICATE_q  & ( (\vga_control|row [7] & \vga_control|row[8]~DUPLICATE_q ) ) ) # ( !\vga_control|row[5]~DUPLICATE_q  & ( (\vga_control|row [7] & (\vga_control|row [6] & \vga_control|row[8]~DUPLICATE_q )) ) )

	.dataa(!\vga_control|row [7]),
	.datab(gnd),
	.datac(!\vga_control|row [6]),
	.datad(!\vga_control|row[8]~DUPLICATE_q ),
	.datae(gnd),
	.dataf(!\vga_control|row[5]~DUPLICATE_q ),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(\LessThan1~1_combout ),
	.sumout(),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \LessThan1~1 .extended_lut = "off";
defparam \LessThan1~1 .lut_mask = 64'h0005000500550055;
defparam \LessThan1~1 .shared_arith = "off";
// synopsys translate_on

// Location: MLABCELL_X28_Y77_N36
cyclonev_lcell_comb \LessThan1~0 (
// Equation(s):
// \LessThan1~0_combout  = ( !\vga_control|row [6] & ( !\vga_control|row[3]~DUPLICATE_q  & ( (!\vga_control|row [2] & (!\vga_control|row[4]~DUPLICATE_q  & ((!\vga_control|row [1]) # (!\vga_control|row[0]~DUPLICATE_q )))) ) ) )

	.dataa(!\vga_control|row [2]),
	.datab(!\vga_control|row[4]~DUPLICATE_q ),
	.datac(!\vga_control|row [1]),
	.datad(!\vga_control|row[0]~DUPLICATE_q ),
	.datae(!\vga_control|row [6]),
	.dataf(!\vga_control|row[3]~DUPLICATE_q ),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(\LessThan1~0_combout ),
	.sumout(),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \LessThan1~0 .extended_lut = "off";
defparam \LessThan1~0 .lut_mask = 64'h8880000000000000;
defparam \LessThan1~0 .shared_arith = "off";
// synopsys translate_on

// Location: MLABCELL_X28_Y77_N54
cyclonev_lcell_comb \LessThan1~2 (
// Equation(s):
// \LessThan1~2_combout  = ( \LessThan1~0_combout  & ( (!\vga_control|row [11] & (!\vga_control|row [9] & !\vga_control|row [10])) ) ) # ( !\LessThan1~0_combout  & ( (!\vga_control|row [11] & (!\vga_control|row [9] & (!\vga_control|row [10] & 
// !\LessThan1~1_combout ))) ) )

	.dataa(!\vga_control|row [11]),
	.datab(!\vga_control|row [9]),
	.datac(!\vga_control|row [10]),
	.datad(!\LessThan1~1_combout ),
	.datae(gnd),
	.dataf(!\LessThan1~0_combout ),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(\LessThan1~2_combout ),
	.sumout(),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \LessThan1~2 .extended_lut = "off";
defparam \LessThan1~2 .lut_mask = 64'h8000800080808080;
defparam \LessThan1~2 .shared_arith = "off";
// synopsys translate_on

// Location: LABCELL_X29_Y77_N48
cyclonev_lcell_comb \red_c[0]~2 (
// Equation(s):
// \red_c[0]~2_combout  = ( \LessThan1~2_combout  & ( ((!\LessThan4~2_combout  & \always1~3_combout )) # (\red_c~1_combout ) ) ) # ( !\LessThan1~2_combout  & ( (!\LessThan4~2_combout  & \always1~3_combout ) ) )

	.dataa(!\red_c~1_combout ),
	.datab(gnd),
	.datac(!\LessThan4~2_combout ),
	.datad(!\always1~3_combout ),
	.datae(gnd),
	.dataf(!\LessThan1~2_combout ),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(\red_c[0]~2_combout ),
	.sumout(),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \red_c[0]~2 .extended_lut = "off";
defparam \red_c[0]~2 .lut_mask = 64'h00F000F055F555F5;
defparam \red_c[0]~2 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X29_Y77_N50
dffeas \red[0] (
	.clk(\CLOCK_50~inputCLKENA0_outclk ),
	.d(\red_c[0]~2_combout ),
	.asdata(vcc),
	.clrn(vcc),
	.aload(gnd),
	.sclr(gnd),
	.sload(gnd),
	.ena(!rClk[0]),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(red[0]),
	.prn(vcc));
// synopsys translate_off
defparam \red[0] .is_wysiwyg = "true";
defparam \red[0] .power_up = "low";
// synopsys translate_on

// Location: LABCELL_X29_Y77_N0
cyclonev_lcell_comb \vga_control|mvga_r[0]~3 (
// Equation(s):
// \vga_control|mvga_r[0]~3_combout  = ( red[0] & ( \vga_control|mvga_r~2_combout  ) )

	.dataa(gnd),
	.datab(gnd),
	.datac(!\vga_control|mvga_r~2_combout ),
	.datad(gnd),
	.datae(gnd),
	.dataf(!red[0]),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(\vga_control|mvga_r[0]~3_combout ),
	.sumout(),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \vga_control|mvga_r[0]~3 .extended_lut = "off";
defparam \vga_control|mvga_r[0]~3 .lut_mask = 64'h000000000F0F0F0F;
defparam \vga_control|mvga_r[0]~3 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X29_Y77_N22
dffeas \vga_control|ored[0] (
	.clk(rClk[0]),
	.d(gnd),
	.asdata(\vga_control|mvga_r[0]~3_combout ),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(gnd),
	.sload(vcc),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|ored [0]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|ored[0] .is_wysiwyg = "true";
defparam \vga_control|ored[0] .power_up = "low";
// synopsys translate_on

// Location: LABCELL_X30_Y77_N42
cyclonev_lcell_comb \vga_control|ored[1]~feeder (
// Equation(s):
// \vga_control|ored[1]~feeder_combout  = ( \vga_control|mvga_r[0]~3_combout  )

	.dataa(gnd),
	.datab(gnd),
	.datac(gnd),
	.datad(gnd),
	.datae(gnd),
	.dataf(!\vga_control|mvga_r[0]~3_combout ),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(\vga_control|ored[1]~feeder_combout ),
	.sumout(),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \vga_control|ored[1]~feeder .extended_lut = "off";
defparam \vga_control|ored[1]~feeder .lut_mask = 64'h00000000FFFFFFFF;
defparam \vga_control|ored[1]~feeder .shared_arith = "off";
// synopsys translate_on

// Location: FF_X30_Y77_N43
dffeas \vga_control|ored[1] (
	.clk(rClk[0]),
	.d(\vga_control|ored[1]~feeder_combout ),
	.asdata(vcc),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(gnd),
	.sload(gnd),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|ored [1]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|ored[1] .is_wysiwyg = "true";
defparam \vga_control|ored[1] .power_up = "low";
// synopsys translate_on

// Location: FF_X28_Y77_N41
dffeas \vga_control|row[0] (
	.clk(rClk[0]),
	.d(gnd),
	.asdata(\vga_control|row[0]~0_combout ),
	.clrn(vcc),
	.aload(gnd),
	.sclr(gnd),
	.sload(vcc),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|row [0]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|row[0] .is_wysiwyg = "true";
defparam \vga_control|row[0] .power_up = "low";
// synopsys translate_on

// Location: LABCELL_X29_Y77_N51
cyclonev_lcell_comb \LessThan0~0 (
// Equation(s):
// \LessThan0~0_combout  = ( !\vga_control|row [6] & ( (!\vga_control|row [2]) # ((!\vga_control|row[1]~DUPLICATE_q  & !\vga_control|row [0])) ) )

	.dataa(gnd),
	.datab(!\vga_control|row [2]),
	.datac(!\vga_control|row[1]~DUPLICATE_q ),
	.datad(!\vga_control|row [0]),
	.datae(gnd),
	.dataf(!\vga_control|row [6]),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(\LessThan0~0_combout ),
	.sumout(),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \LessThan0~0 .extended_lut = "off";
defparam \LessThan0~0 .lut_mask = 64'hFCCCFCCC00000000;
defparam \LessThan0~0 .shared_arith = "off";
// synopsys translate_on

// Location: LABCELL_X27_Y77_N3
cyclonev_lcell_comb \LessThan0~1 (
// Equation(s):
// \LessThan0~1_combout  = ( !\vga_control|row [9] & ( (!\vga_control|row [10] & ((!\LessThan4~0_combout ) # ((\LessThan0~0_combout  & \LessThan3~0_combout )))) ) )

	.dataa(!\vga_control|row [10]),
	.datab(!\LessThan0~0_combout ),
	.datac(!\LessThan3~0_combout ),
	.datad(!\LessThan4~0_combout ),
	.datae(gnd),
	.dataf(!\vga_control|row [9]),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(\LessThan0~1_combout ),
	.sumout(),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \LessThan0~1 .extended_lut = "off";
defparam \LessThan0~1 .lut_mask = 64'hAA02AA0200000000;
defparam \LessThan0~1 .shared_arith = "off";
// synopsys translate_on

// Location: LABCELL_X27_Y77_N42
cyclonev_lcell_comb \red_c[2]~3 (
// Equation(s):
// \red_c[2]~3_combout  = ( \always1~3_combout  & ( \LessThan1~0_combout  & ( (!\LessThan4~2_combout ) # ((!\LessThan0~1_combout  & \red_c~1_combout )) ) ) ) # ( !\always1~3_combout  & ( \LessThan1~0_combout  & ( (!\LessThan0~1_combout  & \red_c~1_combout ) 
// ) ) ) # ( \always1~3_combout  & ( !\LessThan1~0_combout  & ( (!\LessThan4~2_combout ) # ((!\LessThan0~1_combout  & (\red_c~1_combout  & !\LessThan1~1_combout ))) ) ) ) # ( !\always1~3_combout  & ( !\LessThan1~0_combout  & ( (!\LessThan0~1_combout  & 
// (\red_c~1_combout  & !\LessThan1~1_combout )) ) ) )

	.dataa(!\LessThan0~1_combout ),
	.datab(!\red_c~1_combout ),
	.datac(!\LessThan4~2_combout ),
	.datad(!\LessThan1~1_combout ),
	.datae(!\always1~3_combout ),
	.dataf(!\LessThan1~0_combout ),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(\red_c[2]~3_combout ),
	.sumout(),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \red_c[2]~3 .extended_lut = "off";
defparam \red_c[2]~3 .lut_mask = 64'h2200F2F02222F2F2;
defparam \red_c[2]~3 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X27_Y77_N44
dffeas \red[2] (
	.clk(\CLOCK_50~inputCLKENA0_outclk ),
	.d(\red_c[2]~3_combout ),
	.asdata(vcc),
	.clrn(vcc),
	.aload(gnd),
	.sclr(gnd),
	.sload(gnd),
	.ena(!rClk[0]),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(red[2]),
	.prn(vcc));
// synopsys translate_off
defparam \red[2] .is_wysiwyg = "true";
defparam \red[2] .power_up = "low";
// synopsys translate_on

// Location: LABCELL_X27_Y77_N51
cyclonev_lcell_comb \vga_control|mvga_r[2]~4 (
// Equation(s):
// \vga_control|mvga_r[2]~4_combout  = (red[2] & \vga_control|mvga_r~2_combout )

	.dataa(gnd),
	.datab(gnd),
	.datac(!red[2]),
	.datad(!\vga_control|mvga_r~2_combout ),
	.datae(gnd),
	.dataf(gnd),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(\vga_control|mvga_r[2]~4_combout ),
	.sumout(),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \vga_control|mvga_r[2]~4 .extended_lut = "off";
defparam \vga_control|mvga_r[2]~4 .lut_mask = 64'h000F000F000F000F;
defparam \vga_control|mvga_r[2]~4 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X27_Y77_N32
dffeas \vga_control|ored[2] (
	.clk(rClk[0]),
	.d(gnd),
	.asdata(\vga_control|mvga_r[2]~4_combout ),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(gnd),
	.sload(vcc),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|ored [2]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|ored[2] .is_wysiwyg = "true";
defparam \vga_control|ored[2] .power_up = "low";
// synopsys translate_on

// Location: LABCELL_X27_Y77_N48
cyclonev_lcell_comb \vga_control|ored[3]~feeder (
// Equation(s):
// \vga_control|ored[3]~feeder_combout  = ( \vga_control|mvga_r[2]~4_combout  )

	.dataa(gnd),
	.datab(gnd),
	.datac(gnd),
	.datad(gnd),
	.datae(gnd),
	.dataf(!\vga_control|mvga_r[2]~4_combout ),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(\vga_control|ored[3]~feeder_combout ),
	.sumout(),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \vga_control|ored[3]~feeder .extended_lut = "off";
defparam \vga_control|ored[3]~feeder .lut_mask = 64'h00000000FFFFFFFF;
defparam \vga_control|ored[3]~feeder .shared_arith = "off";
// synopsys translate_on

// Location: FF_X27_Y77_N50
dffeas \vga_control|ored[3] (
	.clk(rClk[0]),
	.d(\vga_control|ored[3]~feeder_combout ),
	.asdata(vcc),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(gnd),
	.sload(gnd),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|ored [3]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|ored[3] .is_wysiwyg = "true";
defparam \vga_control|ored[3] .power_up = "low";
// synopsys translate_on

// Location: LABCELL_X30_Y77_N18
cyclonev_lcell_comb \vga_control|ored[4]~feeder (
// Equation(s):
// \vga_control|ored[4]~feeder_combout  = ( \vga_control|mvga_r[0]~3_combout  )

	.dataa(gnd),
	.datab(gnd),
	.datac(gnd),
	.datad(gnd),
	.datae(gnd),
	.dataf(!\vga_control|mvga_r[0]~3_combout ),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(\vga_control|ored[4]~feeder_combout ),
	.sumout(),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \vga_control|ored[4]~feeder .extended_lut = "off";
defparam \vga_control|ored[4]~feeder .lut_mask = 64'h00000000FFFFFFFF;
defparam \vga_control|ored[4]~feeder .shared_arith = "off";
// synopsys translate_on

// Location: FF_X30_Y77_N19
dffeas \vga_control|ored[4] (
	.clk(rClk[0]),
	.d(\vga_control|ored[4]~feeder_combout ),
	.asdata(vcc),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(gnd),
	.sload(gnd),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|ored [4]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|ored[4] .is_wysiwyg = "true";
defparam \vga_control|ored[4] .power_up = "low";
// synopsys translate_on

// Location: FF_X29_Y77_N41
dffeas \vga_control|ored[5] (
	.clk(rClk[0]),
	.d(gnd),
	.asdata(\vga_control|mvga_r[0]~3_combout ),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(gnd),
	.sload(vcc),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|ored [5]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|ored[5] .is_wysiwyg = "true";
defparam \vga_control|ored[5] .power_up = "low";
// synopsys translate_on

// Location: LABCELL_X27_Y77_N33
cyclonev_lcell_comb \vga_control|ored[6]~feeder (
// Equation(s):
// \vga_control|ored[6]~feeder_combout  = ( \vga_control|mvga_r[2]~4_combout  )

	.dataa(gnd),
	.datab(gnd),
	.datac(gnd),
	.datad(gnd),
	.datae(gnd),
	.dataf(!\vga_control|mvga_r[2]~4_combout ),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(\vga_control|ored[6]~feeder_combout ),
	.sumout(),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \vga_control|ored[6]~feeder .extended_lut = "off";
defparam \vga_control|ored[6]~feeder .lut_mask = 64'h00000000FFFFFFFF;
defparam \vga_control|ored[6]~feeder .shared_arith = "off";
// synopsys translate_on

// Location: FF_X27_Y77_N35
dffeas \vga_control|ored[6] (
	.clk(rClk[0]),
	.d(\vga_control|ored[6]~feeder_combout ),
	.asdata(vcc),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(gnd),
	.sload(gnd),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|ored [6]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|ored[6] .is_wysiwyg = "true";
defparam \vga_control|ored[6] .power_up = "low";
// synopsys translate_on

// Location: FF_X29_Y77_N56
dffeas \vga_control|ored[7] (
	.clk(rClk[0]),
	.d(gnd),
	.asdata(\vga_control|mvga_r[0]~3_combout ),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(gnd),
	.sload(vcc),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|ored [7]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|ored[7] .is_wysiwyg = "true";
defparam \vga_control|ored[7] .power_up = "low";
// synopsys translate_on

// Location: LABCELL_X29_Y77_N54
cyclonev_lcell_comb \LessThan0~2 (
// Equation(s):
// \LessThan0~2_combout  = (\LessThan0~0_combout  & \LessThan3~0_combout )

	.dataa(gnd),
	.datab(!\LessThan0~0_combout ),
	.datac(!\LessThan3~0_combout ),
	.datad(gnd),
	.datae(gnd),
	.dataf(gnd),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(\LessThan0~2_combout ),
	.sumout(),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \LessThan0~2 .extended_lut = "off";
defparam \LessThan0~2 .lut_mask = 64'h0303030303030303;
defparam \LessThan0~2 .shared_arith = "off";
// synopsys translate_on

// Location: MLABCELL_X28_Y77_N42
cyclonev_lcell_comb \green_c[2]~0 (
// Equation(s):
// \green_c[2]~0_combout  = ( \LessThan2~0_combout  & ( \LessThan4~0_combout  & ( (\red_c~0_combout  & ((!\LessThan1~2_combout ) # (\LessThan0~2_combout ))) ) ) ) # ( !\LessThan2~0_combout  & ( \LessThan4~0_combout  & ( (\red_c~0_combout  & 
// (!\vga_control|row [6] & ((!\LessThan1~2_combout ) # (\LessThan0~2_combout )))) ) ) ) # ( \LessThan2~0_combout  & ( !\LessThan4~0_combout  & ( \red_c~0_combout  ) ) ) # ( !\LessThan2~0_combout  & ( !\LessThan4~0_combout  & ( \red_c~0_combout  ) ) )

	.dataa(!\red_c~0_combout ),
	.datab(!\LessThan1~2_combout ),
	.datac(!\LessThan0~2_combout ),
	.datad(!\vga_control|row [6]),
	.datae(!\LessThan2~0_combout ),
	.dataf(!\LessThan4~0_combout ),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(\green_c[2]~0_combout ),
	.sumout(),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \green_c[2]~0 .extended_lut = "off";
defparam \green_c[2]~0 .lut_mask = 64'h5555555545004545;
defparam \green_c[2]~0 .shared_arith = "off";
// synopsys translate_on

// Location: LABCELL_X29_Y77_N12
cyclonev_lcell_comb \always1~4 (
// Equation(s):
// \always1~4_combout  = ( !\LessThan4~2_combout  & ( \always1~3_combout  ) )

	.dataa(gnd),
	.datab(!\always1~3_combout ),
	.datac(gnd),
	.datad(gnd),
	.datae(gnd),
	.dataf(!\LessThan4~2_combout ),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(\always1~4_combout ),
	.sumout(),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \always1~4 .extended_lut = "off";
defparam \always1~4 .lut_mask = 64'h3333333300000000;
defparam \always1~4 .shared_arith = "off";
// synopsys translate_on

// Location: LABCELL_X29_Y77_N24
cyclonev_lcell_comb \green_c[0]~1 (
// Equation(s):
// \green_c[0]~1_combout  = ( \always1~4_combout  ) # ( !\always1~4_combout  & ( \green_c[2]~0_combout  ) )

	.dataa(gnd),
	.datab(!\green_c[2]~0_combout ),
	.datac(gnd),
	.datad(gnd),
	.datae(!\always1~4_combout ),
	.dataf(gnd),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(\green_c[0]~1_combout ),
	.sumout(),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \green_c[0]~1 .extended_lut = "off";
defparam \green_c[0]~1 .lut_mask = 64'h3333FFFF3333FFFF;
defparam \green_c[0]~1 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X29_Y77_N26
dffeas \green[0] (
	.clk(\CLOCK_50~inputCLKENA0_outclk ),
	.d(\green_c[0]~1_combout ),
	.asdata(vcc),
	.clrn(vcc),
	.aload(gnd),
	.sclr(gnd),
	.sload(gnd),
	.ena(!rClk[0]),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(green[0]),
	.prn(vcc));
// synopsys translate_off
defparam \green[0] .is_wysiwyg = "true";
defparam \green[0] .power_up = "low";
// synopsys translate_on

// Location: LABCELL_X29_Y77_N30
cyclonev_lcell_comb \vga_control|mVGA_G[0]~0 (
// Equation(s):
// \vga_control|mVGA_G[0]~0_combout  = ( green[0] & ( \vga_control|mvga_r~2_combout  ) )

	.dataa(gnd),
	.datab(gnd),
	.datac(!\vga_control|mvga_r~2_combout ),
	.datad(gnd),
	.datae(gnd),
	.dataf(!green[0]),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(\vga_control|mVGA_G[0]~0_combout ),
	.sumout(),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \vga_control|mVGA_G[0]~0 .extended_lut = "off";
defparam \vga_control|mVGA_G[0]~0 .lut_mask = 64'h000000000F0F0F0F;
defparam \vga_control|mVGA_G[0]~0 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X29_Y77_N31
dffeas \vga_control|ogreen[0] (
	.clk(rClk[0]),
	.d(\vga_control|mVGA_G[0]~0_combout ),
	.asdata(vcc),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(gnd),
	.sload(gnd),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|ogreen [0]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|ogreen[0] .is_wysiwyg = "true";
defparam \vga_control|ogreen[0] .power_up = "low";
// synopsys translate_on

// Location: LABCELL_X27_Y77_N39
cyclonev_lcell_comb \green_c[1]~2 (
// Equation(s):
// \green_c[1]~2_combout  = ( !\LessThan1~2_combout  & ( (\red_c~1_combout  & ((!\always1~3_combout ) # (\LessThan4~2_combout ))) ) )

	.dataa(gnd),
	.datab(!\red_c~1_combout ),
	.datac(!\always1~3_combout ),
	.datad(!\LessThan4~2_combout ),
	.datae(gnd),
	.dataf(!\LessThan1~2_combout ),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(\green_c[1]~2_combout ),
	.sumout(),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \green_c[1]~2 .extended_lut = "off";
defparam \green_c[1]~2 .lut_mask = 64'h3033303300000000;
defparam \green_c[1]~2 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X27_Y77_N41
dffeas \green[1] (
	.clk(\CLOCK_50~inputCLKENA0_outclk ),
	.d(\green_c[1]~2_combout ),
	.asdata(vcc),
	.clrn(vcc),
	.aload(gnd),
	.sclr(gnd),
	.sload(gnd),
	.ena(!rClk[0]),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(green[1]),
	.prn(vcc));
// synopsys translate_off
defparam \green[1] .is_wysiwyg = "true";
defparam \green[1] .power_up = "low";
// synopsys translate_on

// Location: LABCELL_X27_Y77_N54
cyclonev_lcell_comb \vga_control|mVGA_G[1]~1 (
// Equation(s):
// \vga_control|mVGA_G[1]~1_combout  = ( green[1] & ( \vga_control|mvga_r~2_combout  ) )

	.dataa(gnd),
	.datab(gnd),
	.datac(gnd),
	.datad(!\vga_control|mvga_r~2_combout ),
	.datae(gnd),
	.dataf(!green[1]),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(\vga_control|mVGA_G[1]~1_combout ),
	.sumout(),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \vga_control|mVGA_G[1]~1 .extended_lut = "off";
defparam \vga_control|mVGA_G[1]~1 .lut_mask = 64'h0000000000FF00FF;
defparam \vga_control|mVGA_G[1]~1 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X27_Y77_N56
dffeas \vga_control|ogreen[1] (
	.clk(rClk[0]),
	.d(\vga_control|mVGA_G[1]~1_combout ),
	.asdata(vcc),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(gnd),
	.sload(gnd),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|ogreen [1]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|ogreen[1] .is_wysiwyg = "true";
defparam \vga_control|ogreen[1] .power_up = "low";
// synopsys translate_on

// Location: LABCELL_X29_Y77_N6
cyclonev_lcell_comb \green_c[2]~3 (
// Equation(s):
// \green_c[2]~3_combout  = ( \green_c[2]~0_combout  & ( !\always1~4_combout  ) )

	.dataa(gnd),
	.datab(!\always1~4_combout ),
	.datac(gnd),
	.datad(gnd),
	.datae(gnd),
	.dataf(!\green_c[2]~0_combout ),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(\green_c[2]~3_combout ),
	.sumout(),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \green_c[2]~3 .extended_lut = "off";
defparam \green_c[2]~3 .lut_mask = 64'h00000000CCCCCCCC;
defparam \green_c[2]~3 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X29_Y77_N8
dffeas \green[2] (
	.clk(\CLOCK_50~inputCLKENA0_outclk ),
	.d(\green_c[2]~3_combout ),
	.asdata(vcc),
	.clrn(vcc),
	.aload(gnd),
	.sclr(gnd),
	.sload(gnd),
	.ena(!rClk[0]),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(green[2]),
	.prn(vcc));
// synopsys translate_off
defparam \green[2] .is_wysiwyg = "true";
defparam \green[2] .power_up = "low";
// synopsys translate_on

// Location: LABCELL_X29_Y77_N57
cyclonev_lcell_comb \vga_control|mVGA_G[2]~2 (
// Equation(s):
// \vga_control|mVGA_G[2]~2_combout  = ( green[2] & ( \vga_control|mvga_r~2_combout  ) )

	.dataa(!\vga_control|mvga_r~2_combout ),
	.datab(gnd),
	.datac(gnd),
	.datad(gnd),
	.datae(gnd),
	.dataf(!green[2]),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(\vga_control|mVGA_G[2]~2_combout ),
	.sumout(),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \vga_control|mVGA_G[2]~2 .extended_lut = "off";
defparam \vga_control|mVGA_G[2]~2 .lut_mask = 64'h0000000055555555;
defparam \vga_control|mVGA_G[2]~2 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X29_Y77_N37
dffeas \vga_control|ogreen[2] (
	.clk(rClk[0]),
	.d(gnd),
	.asdata(\vga_control|mVGA_G[2]~2_combout ),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(gnd),
	.sload(vcc),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|ogreen [2]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|ogreen[2] .is_wysiwyg = "true";
defparam \vga_control|ogreen[2] .power_up = "low";
// synopsys translate_on

// Location: LABCELL_X27_Y77_N18
cyclonev_lcell_comb \green_c[3]~4 (
// Equation(s):
// \green_c[3]~4_combout  = ( \LessThan1~2_combout  & ( (\always1~3_combout  & !\LessThan4~2_combout ) ) ) # ( !\LessThan1~2_combout  & ( ((\always1~3_combout  & !\LessThan4~2_combout )) # (\red_c~1_combout ) ) )

	.dataa(gnd),
	.datab(!\red_c~1_combout ),
	.datac(!\always1~3_combout ),
	.datad(!\LessThan4~2_combout ),
	.datae(gnd),
	.dataf(!\LessThan1~2_combout ),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(\green_c[3]~4_combout ),
	.sumout(),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \green_c[3]~4 .extended_lut = "off";
defparam \green_c[3]~4 .lut_mask = 64'h3F333F330F000F00;
defparam \green_c[3]~4 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X27_Y77_N20
dffeas \green[3] (
	.clk(\CLOCK_50~inputCLKENA0_outclk ),
	.d(\green_c[3]~4_combout ),
	.asdata(vcc),
	.clrn(vcc),
	.aload(gnd),
	.sclr(gnd),
	.sload(gnd),
	.ena(!rClk[0]),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(green[3]),
	.prn(vcc));
// synopsys translate_off
defparam \green[3] .is_wysiwyg = "true";
defparam \green[3] .power_up = "low";
// synopsys translate_on

// Location: LABCELL_X27_Y77_N57
cyclonev_lcell_comb \vga_control|mVGA_G[3]~3 (
// Equation(s):
// \vga_control|mVGA_G[3]~3_combout  = ( green[3] & ( \vga_control|mvga_r~2_combout  ) )

	.dataa(gnd),
	.datab(gnd),
	.datac(gnd),
	.datad(!\vga_control|mvga_r~2_combout ),
	.datae(gnd),
	.dataf(!green[3]),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(\vga_control|mVGA_G[3]~3_combout ),
	.sumout(),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \vga_control|mVGA_G[3]~3 .extended_lut = "off";
defparam \vga_control|mVGA_G[3]~3 .lut_mask = 64'h0000000000FF00FF;
defparam \vga_control|mVGA_G[3]~3 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X27_Y77_N10
dffeas \vga_control|ogreen[3] (
	.clk(rClk[0]),
	.d(gnd),
	.asdata(\vga_control|mVGA_G[3]~3_combout ),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(gnd),
	.sload(vcc),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|ogreen [3]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|ogreen[3] .is_wysiwyg = "true";
defparam \vga_control|ogreen[3] .power_up = "low";
// synopsys translate_on

// Location: FF_X27_Y77_N2
dffeas \vga_control|ogreen[4] (
	.clk(rClk[0]),
	.d(gnd),
	.asdata(\vga_control|mVGA_G[3]~3_combout ),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(gnd),
	.sload(vcc),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|ogreen [4]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|ogreen[4] .is_wysiwyg = "true";
defparam \vga_control|ogreen[4] .power_up = "low";
// synopsys translate_on

// Location: FF_X29_Y77_N16
dffeas \vga_control|ogreen[5] (
	.clk(rClk[0]),
	.d(gnd),
	.asdata(\vga_control|mVGA_G[2]~2_combout ),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(gnd),
	.sload(vcc),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|ogreen [5]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|ogreen[5] .is_wysiwyg = "true";
defparam \vga_control|ogreen[5] .power_up = "low";
// synopsys translate_on

// Location: FF_X29_Y77_N2
dffeas \vga_control|ogreen[6] (
	.clk(rClk[0]),
	.d(gnd),
	.asdata(\vga_control|mVGA_G[2]~2_combout ),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(gnd),
	.sload(vcc),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|ogreen [6]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|ogreen[6] .is_wysiwyg = "true";
defparam \vga_control|ogreen[6] .power_up = "low";
// synopsys translate_on

// Location: FF_X29_Y77_N4
dffeas \vga_control|ogreen[7] (
	.clk(rClk[0]),
	.d(gnd),
	.asdata(\vga_control|mVGA_G[2]~2_combout ),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(gnd),
	.sload(vcc),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|ogreen [7]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|ogreen[7] .is_wysiwyg = "true";
defparam \vga_control|ogreen[7] .power_up = "low";
// synopsys translate_on

// Location: LABCELL_X27_Y77_N24
cyclonev_lcell_comb \blue_c[0]~0 (
// Equation(s):
// \blue_c[0]~0_combout  = ( \vga_control|row [11] & ( \LessThan1~2_combout  & ( (!\red_c~1_combout  & ((!\always1~3_combout ) # (\LessThan4~2_combout ))) ) ) ) # ( !\vga_control|row [11] & ( \LessThan1~2_combout  & ( (!\always1~3_combout  & 
// ((!\red_c~1_combout ) # ((\LessThan0~1_combout )))) # (\always1~3_combout  & (\LessThan4~2_combout  & ((!\red_c~1_combout ) # (\LessThan0~1_combout )))) ) ) ) # ( \vga_control|row [11] & ( !\LessThan1~2_combout  & ( (!\red_c~1_combout  & 
// ((!\always1~3_combout ) # (\LessThan4~2_combout ))) ) ) ) # ( !\vga_control|row [11] & ( !\LessThan1~2_combout  & ( (!\red_c~1_combout  & ((!\always1~3_combout ) # (\LessThan4~2_combout ))) ) ) )

	.dataa(!\always1~3_combout ),
	.datab(!\red_c~1_combout ),
	.datac(!\LessThan4~2_combout ),
	.datad(!\LessThan0~1_combout ),
	.datae(!\vga_control|row [11]),
	.dataf(!\LessThan1~2_combout ),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(\blue_c[0]~0_combout ),
	.sumout(),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \blue_c[0]~0 .extended_lut = "off";
defparam \blue_c[0]~0 .lut_mask = 64'h8C8C8C8C8CAF8C8C;
defparam \blue_c[0]~0 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X27_Y77_N26
dffeas \blue[0] (
	.clk(\CLOCK_50~inputCLKENA0_outclk ),
	.d(\blue_c[0]~0_combout ),
	.asdata(vcc),
	.clrn(vcc),
	.aload(gnd),
	.sclr(gnd),
	.sload(gnd),
	.ena(!rClk[0]),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(blue[0]),
	.prn(vcc));
// synopsys translate_off
defparam \blue[0] .is_wysiwyg = "true";
defparam \blue[0] .power_up = "low";
// synopsys translate_on

// Location: LABCELL_X27_Y77_N15
cyclonev_lcell_comb \vga_control|mVGA_B[0]~0 (
// Equation(s):
// \vga_control|mVGA_B[0]~0_combout  = ( blue[0] & ( \vga_control|mvga_r~2_combout  ) )

	.dataa(gnd),
	.datab(gnd),
	.datac(gnd),
	.datad(!\vga_control|mvga_r~2_combout ),
	.datae(gnd),
	.dataf(!blue[0]),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(\vga_control|mVGA_B[0]~0_combout ),
	.sumout(),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \vga_control|mVGA_B[0]~0 .extended_lut = "off";
defparam \vga_control|mVGA_B[0]~0 .lut_mask = 64'h0000000000FF00FF;
defparam \vga_control|mVGA_B[0]~0 .shared_arith = "off";
// synopsys translate_on

// Location: LABCELL_X27_Y77_N0
cyclonev_lcell_comb \vga_control|oblue[0]~feeder (
// Equation(s):
// \vga_control|oblue[0]~feeder_combout  = ( \vga_control|mVGA_B[0]~0_combout  )

	.dataa(gnd),
	.datab(gnd),
	.datac(gnd),
	.datad(gnd),
	.datae(gnd),
	.dataf(!\vga_control|mVGA_B[0]~0_combout ),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(\vga_control|oblue[0]~feeder_combout ),
	.sumout(),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \vga_control|oblue[0]~feeder .extended_lut = "off";
defparam \vga_control|oblue[0]~feeder .lut_mask = 64'h00000000FFFFFFFF;
defparam \vga_control|oblue[0]~feeder .shared_arith = "off";
// synopsys translate_on

// Location: FF_X27_Y77_N1
dffeas \vga_control|oblue[0] (
	.clk(rClk[0]),
	.d(\vga_control|oblue[0]~feeder_combout ),
	.asdata(vcc),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(gnd),
	.sload(gnd),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|oblue [0]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|oblue[0] .is_wysiwyg = "true";
defparam \vga_control|oblue[0] .power_up = "low";
// synopsys translate_on

// Location: FF_X27_Y77_N49
dffeas \vga_control|oblue[1] (
	.clk(rClk[0]),
	.d(gnd),
	.asdata(\vga_control|mVGA_B[0]~0_combout ),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(gnd),
	.sload(vcc),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|oblue [1]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|oblue[1] .is_wysiwyg = "true";
defparam \vga_control|oblue[1] .power_up = "low";
// synopsys translate_on

// Location: LABCELL_X27_Y77_N30
cyclonev_lcell_comb \vga_control|oblue[2]~feeder (
// Equation(s):
// \vga_control|oblue[2]~feeder_combout  = ( \vga_control|mVGA_B[0]~0_combout  )

	.dataa(gnd),
	.datab(gnd),
	.datac(gnd),
	.datad(gnd),
	.datae(gnd),
	.dataf(!\vga_control|mVGA_B[0]~0_combout ),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(\vga_control|oblue[2]~feeder_combout ),
	.sumout(),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \vga_control|oblue[2]~feeder .extended_lut = "off";
defparam \vga_control|oblue[2]~feeder .lut_mask = 64'h00000000FFFFFFFF;
defparam \vga_control|oblue[2]~feeder .shared_arith = "off";
// synopsys translate_on

// Location: FF_X27_Y77_N31
dffeas \vga_control|oblue[2] (
	.clk(rClk[0]),
	.d(\vga_control|oblue[2]~feeder_combout ),
	.asdata(vcc),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(gnd),
	.sload(gnd),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|oblue [2]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|oblue[2] .is_wysiwyg = "true";
defparam \vga_control|oblue[2] .power_up = "low";
// synopsys translate_on

// Location: FF_X27_Y77_N34
dffeas \vga_control|oblue[3] (
	.clk(rClk[0]),
	.d(gnd),
	.asdata(\vga_control|mVGA_B[0]~0_combout ),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(gnd),
	.sload(vcc),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|oblue [3]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|oblue[3] .is_wysiwyg = "true";
defparam \vga_control|oblue[3] .power_up = "low";
// synopsys translate_on

// Location: LABCELL_X29_Y77_N42
cyclonev_lcell_comb \blue_c[4]~1 (
// Equation(s):
// \blue_c[4]~1_combout  = ( \always1~3_combout  & ( \LessThan1~2_combout  & ( (!\LessThan4~2_combout ) # ((!\red_c~1_combout ) # ((!\vga_control|row [11] & \LessThan0~1_combout ))) ) ) ) # ( !\always1~3_combout  & ( \LessThan1~2_combout  & ( 
// (!\red_c~1_combout ) # ((!\vga_control|row [11] & \LessThan0~1_combout )) ) ) ) # ( \always1~3_combout  & ( !\LessThan1~2_combout  & ( (!\LessThan4~2_combout ) # (!\red_c~1_combout ) ) ) ) # ( !\always1~3_combout  & ( !\LessThan1~2_combout  & ( 
// !\red_c~1_combout  ) ) )

	.dataa(!\LessThan4~2_combout ),
	.datab(!\vga_control|row [11]),
	.datac(!\LessThan0~1_combout ),
	.datad(!\red_c~1_combout ),
	.datae(!\always1~3_combout ),
	.dataf(!\LessThan1~2_combout ),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(\blue_c[4]~1_combout ),
	.sumout(),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \blue_c[4]~1 .extended_lut = "off";
defparam \blue_c[4]~1 .lut_mask = 64'hFF00FFAAFF0CFFAE;
defparam \blue_c[4]~1 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X29_Y77_N44
dffeas \blue[4] (
	.clk(\CLOCK_50~inputCLKENA0_outclk ),
	.d(\blue_c[4]~1_combout ),
	.asdata(vcc),
	.clrn(vcc),
	.aload(gnd),
	.sclr(gnd),
	.sload(gnd),
	.ena(!rClk[0]),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(blue[4]),
	.prn(vcc));
// synopsys translate_off
defparam \blue[4] .is_wysiwyg = "true";
defparam \blue[4] .power_up = "low";
// synopsys translate_on

// Location: LABCELL_X29_Y77_N33
cyclonev_lcell_comb \vga_control|mVGA_B[4]~1 (
// Equation(s):
// \vga_control|mVGA_B[4]~1_combout  = ( blue[4] & ( \vga_control|mvga_r~2_combout  ) )

	.dataa(!\vga_control|mvga_r~2_combout ),
	.datab(gnd),
	.datac(gnd),
	.datad(gnd),
	.datae(gnd),
	.dataf(!blue[4]),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(\vga_control|mVGA_B[4]~1_combout ),
	.sumout(),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \vga_control|mVGA_B[4]~1 .extended_lut = "off";
defparam \vga_control|mVGA_B[4]~1 .lut_mask = 64'h0000000055555555;
defparam \vga_control|mVGA_B[4]~1 .shared_arith = "off";
// synopsys translate_on

// Location: FF_X29_Y77_N58
dffeas \vga_control|oblue[4] (
	.clk(rClk[0]),
	.d(gnd),
	.asdata(\vga_control|mVGA_B[4]~1_combout ),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(gnd),
	.sload(vcc),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|oblue [4]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|oblue[4] .is_wysiwyg = "true";
defparam \vga_control|oblue[4] .power_up = "low";
// synopsys translate_on

// Location: FF_X29_Y77_N19
dffeas \vga_control|oblue[5] (
	.clk(rClk[0]),
	.d(gnd),
	.asdata(\vga_control|mVGA_B[4]~1_combout ),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(gnd),
	.sload(vcc),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|oblue [5]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|oblue[5] .is_wysiwyg = "true";
defparam \vga_control|oblue[5] .power_up = "low";
// synopsys translate_on

// Location: FF_X30_Y77_N25
dffeas \vga_control|oblue[6] (
	.clk(rClk[0]),
	.d(gnd),
	.asdata(\vga_control|mVGA_B[4]~1_combout ),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(gnd),
	.sload(vcc),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|oblue [6]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|oblue[6] .is_wysiwyg = "true";
defparam \vga_control|oblue[6] .power_up = "low";
// synopsys translate_on

// Location: FF_X30_Y77_N31
dffeas \vga_control|oblue[7] (
	.clk(rClk[0]),
	.d(gnd),
	.asdata(\vga_control|mVGA_B[4]~1_combout ),
	.clrn(\KEY[0]~input_o ),
	.aload(gnd),
	.sclr(gnd),
	.sload(vcc),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\vga_control|oblue [7]),
	.prn(vcc));
// synopsys translate_off
defparam \vga_control|oblue[7] .is_wysiwyg = "true";
defparam \vga_control|oblue[7] .power_up = "low";
// synopsys translate_on

// Location: IOIBUF_X36_Y0_N18
cyclonev_io_ibuf \KEY[1]~input (
	.i(KEY[1]),
	.ibar(gnd),
	.dynamicterminationcontrol(gnd),
	.o(\KEY[1]~input_o ));
// synopsys translate_off
defparam \KEY[1]~input .bus_hold = "false";
defparam \KEY[1]~input .simulate_z_as = "z";
// synopsys translate_on

// Location: IOIBUF_X40_Y0_N1
cyclonev_io_ibuf \KEY[2]~input (
	.i(KEY[2]),
	.ibar(gnd),
	.dynamicterminationcontrol(gnd),
	.o(\KEY[2]~input_o ));
// synopsys translate_off
defparam \KEY[2]~input .bus_hold = "false";
defparam \KEY[2]~input .simulate_z_as = "z";
// synopsys translate_on

// Location: IOIBUF_X12_Y0_N18
cyclonev_io_ibuf \SW[0]~input (
	.i(SW[0]),
	.ibar(gnd),
	.dynamicterminationcontrol(gnd),
	.o(\SW[0]~input_o ));
// synopsys translate_off
defparam \SW[0]~input .bus_hold = "false";
defparam \SW[0]~input .simulate_z_as = "z";
// synopsys translate_on

// Location: IOIBUF_X16_Y0_N1
cyclonev_io_ibuf \SW[1]~input (
	.i(SW[1]),
	.ibar(gnd),
	.dynamicterminationcontrol(gnd),
	.o(\SW[1]~input_o ));
// synopsys translate_off
defparam \SW[1]~input .bus_hold = "false";
defparam \SW[1]~input .simulate_z_as = "z";
// synopsys translate_on

// Location: IOIBUF_X8_Y0_N35
cyclonev_io_ibuf \SW[2]~input (
	.i(SW[2]),
	.ibar(gnd),
	.dynamicterminationcontrol(gnd),
	.o(\SW[2]~input_o ));
// synopsys translate_off
defparam \SW[2]~input .bus_hold = "false";
defparam \SW[2]~input .simulate_z_as = "z";
// synopsys translate_on

// Location: IOIBUF_X4_Y0_N52
cyclonev_io_ibuf \SW[3]~input (
	.i(SW[3]),
	.ibar(gnd),
	.dynamicterminationcontrol(gnd),
	.o(\SW[3]~input_o ));
// synopsys translate_off
defparam \SW[3]~input .bus_hold = "false";
defparam \SW[3]~input .simulate_z_as = "z";
// synopsys translate_on

// Location: IOIBUF_X2_Y0_N41
cyclonev_io_ibuf \SW[4]~input (
	.i(SW[4]),
	.ibar(gnd),
	.dynamicterminationcontrol(gnd),
	.o(\SW[4]~input_o ));
// synopsys translate_off
defparam \SW[4]~input .bus_hold = "false";
defparam \SW[4]~input .simulate_z_as = "z";
// synopsys translate_on

// Location: IOIBUF_X16_Y0_N18
cyclonev_io_ibuf \SW[5]~input (
	.i(SW[5]),
	.ibar(gnd),
	.dynamicterminationcontrol(gnd),
	.o(\SW[5]~input_o ));
// synopsys translate_off
defparam \SW[5]~input .bus_hold = "false";
defparam \SW[5]~input .simulate_z_as = "z";
// synopsys translate_on

// Location: IOIBUF_X4_Y0_N35
cyclonev_io_ibuf \SW[6]~input (
	.i(SW[6]),
	.ibar(gnd),
	.dynamicterminationcontrol(gnd),
	.o(\SW[6]~input_o ));
// synopsys translate_off
defparam \SW[6]~input .bus_hold = "false";
defparam \SW[6]~input .simulate_z_as = "z";
// synopsys translate_on

// Location: IOIBUF_X4_Y0_N1
cyclonev_io_ibuf \SW[7]~input (
	.i(SW[7]),
	.ibar(gnd),
	.dynamicterminationcontrol(gnd),
	.o(\SW[7]~input_o ));
// synopsys translate_off
defparam \SW[7]~input .bus_hold = "false";
defparam \SW[7]~input .simulate_z_as = "z";
// synopsys translate_on

// Location: IOIBUF_X4_Y0_N18
cyclonev_io_ibuf \SW[8]~input (
	.i(SW[8]),
	.ibar(gnd),
	.dynamicterminationcontrol(gnd),
	.o(\SW[8]~input_o ));
// synopsys translate_off
defparam \SW[8]~input .bus_hold = "false";
defparam \SW[8]~input .simulate_z_as = "z";
// synopsys translate_on

// Location: MLABCELL_X34_Y44_N0
cyclonev_lcell_comb \~QUARTUS_CREATED_GND~I (
// Equation(s):

	.dataa(gnd),
	.datab(gnd),
	.datac(gnd),
	.datad(gnd),
	.datae(gnd),
	.dataf(gnd),
	.datag(gnd),
	.cin(gnd),
	.sharein(gnd),
	.combout(\~QUARTUS_CREATED_GND~I_combout ),
	.sumout(),
	.cout(),
	.shareout());
// synopsys translate_off
defparam \~QUARTUS_CREATED_GND~I .extended_lut = "off";
defparam \~QUARTUS_CREATED_GND~I .lut_mask = 64'h0000000000000000;
defparam \~QUARTUS_CREATED_GND~I .shared_arith = "off";
// synopsys translate_on

endmodule
